From e3ccffe9335ce3bdba93640588fab4560d18485e Mon Sep 17 00:00:00 2001
From: devi priya <quic_devipriy@quicinc.com>
Date: Thu, 1 Aug 2024 11:18:00 +0530
Subject: [PATCH 02/22] v6.13: dt-bindings: PCI: qcom: Document the IPQ9574
 PCIe controller
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

Document the PCIe controller on IPQ9574 platform.

Link: https://lore.kernel.org/r/20240801054803.3015572-2-quic_srichara@quicinc.com
Signed-off-by: devi priya <quic_devipriy@quicinc.com>
Signed-off-by: Sricharan Ramabadhran <quic_srichara@quicinc.com>
Signed-off-by: Krzysztof Wilczyński <kwilczynski@kernel.org>
Reviewed-by: Krzysztof Kozlowski <krzysztof.kozlowski@linaro.org>
Reviewed-by: Manivannan Sadhasivam <manivannan.sadhasivam@linaro.org>
---
 .../devicetree/bindings/pci/qcom,pcie.yaml    | 50 +++++++++++++++++++
 1 file changed, 50 insertions(+)

--- a/Documentation/devicetree/bindings/pci/qcom,pcie.yaml
+++ b/Documentation/devicetree/bindings/pci/qcom,pcie.yaml
@@ -26,6 +26,7 @@ properties:
           - qcom,pcie-ipq8064-v2
           - qcom,pcie-ipq8074
           - qcom,pcie-ipq8074-gen3
+          - qcom,pcie-ipq9574
           - qcom,pcie-msm8996
           - qcom,pcie-qcs404
           - qcom,pcie-sdm845
@@ -164,6 +165,7 @@ allOf:
             enum:
               - qcom,pcie-ipq6018
               - qcom,pcie-ipq8074-gen3
+              - qcom,pcie-ipq9574
     then:
       properties:
         reg:
@@ -405,6 +407,53 @@ allOf:
         compatible:
           contains:
             enum:
+              - qcom,pcie-ipq9574
+    then:
+      properties:
+        clocks:
+          minItems: 6
+          maxItems: 6
+        clock-names:
+          items:
+            - const: axi_m # AXI Master clock
+            - const: axi_s # AXI Slave clock
+            - const: axi_bridge
+            - const: rchng
+            - const: ahb
+            - const: aux
+
+        resets:
+          minItems: 8
+          maxItems: 8
+        reset-names:
+          items:
+            - const: pipe # PIPE reset
+            - const: sticky # Core Sticky reset
+            - const: axi_s_sticky # AXI Slave Sticky reset
+            - const: axi_s # AXI Slave reset
+            - const: axi_m_sticky # AXI Master Sticky reset
+            - const: axi_m # AXI Master reset
+            - const: aux # AUX Reset
+            - const: ahb # AHB Reset
+
+        interrupts:
+          minItems: 8
+        interrupt-names:
+          items:
+            - const: msi0
+            - const: msi1
+            - const: msi2
+            - const: msi3
+            - const: msi4
+            - const: msi5
+            - const: msi6
+            - const: msi7
+
+  - if:
+      properties:
+        compatible:
+          contains:
+            enum:
               - qcom,pcie-qcs404
     then:
       properties:
@@ -510,6 +559,7 @@ allOf:
                 - qcom,pcie-ipq8064v2
                 - qcom,pcie-ipq8074
                 - qcom,pcie-ipq8074-gen3
+                - qcom,pcie-ipq9574
                 - qcom,pcie-qcs404
     then:
       required:
