#include "qcom-ipq8064-v2.0-smb208.dtsi"

#include <dt-bindings/input/input.h>
#include <dt-bindings/leds/common.h>

/ {
	model = "NEC Aterm WG2600HP";
	compatible = "nec,wg2600hp", "qcom,ipq8064";

	memory@0 {
		reg = <0x42000000 0x1e000000>;
		device_type = "memory";
	};

	aliases {
		mdio-gpio0 = &mdio0;

		led-boot = &power_green;
		led-failsafe = &power_red;
		led-running = &power_green;
		led-upgrade = &power_green;
	};

	keys {
		compatible = "gpio-keys";
		pinctrl-0 = <&button_pins>;
		pinctrl-names = "default";

		wps {
			label = "wps";
			gpios = <&qcom_pinmux 16 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_WPS_BUTTON>;
			debounce-interval = <60>;
			wakeup-source;
		};

		reset {
			label = "reset";
			gpios = <&qcom_pinmux 54 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
			debounce-interval = <60>;
			wakeup-source;
		};

		bridge {
			label = "bridge";
			gpios = <&qcom_pinmux 24 GPIO_ACTIVE_LOW>;
			linux,code = <BTN_0>;
			linux,input-type = <EV_SW>;
			debounce-interval = <60>;
			wakeup-source;
		};

		converter {
			label = "converter";
			gpios = <&qcom_pinmux 25 GPIO_ACTIVE_LOW>;
			linux,code = <BTN_0>;
			linux,input-type = <EV_SW>;
			debounce-interval = <60>;
			wakeup-source;
		};
	};

	leds {
		compatible = "gpio-leds";
		pinctrl-0 = <&led_pins>;
		pinctrl-names = "default";

		converter_green {
			label = "green:converter";
			gpios = <&qcom_pinmux 6 GPIO_ACTIVE_HIGH>;
		};

		power_red: power_red {
			function = LED_FUNCTION_POWER;
			color = <LED_COLOR_ID_RED>;
			gpios = <&qcom_pinmux 7 GPIO_ACTIVE_HIGH>;
		};

		active_green {
			label = "green:active";
			gpios = <&qcom_pinmux 8 GPIO_ACTIVE_HIGH>;
		};

		active_red {
			label = "red:active";
			gpios = <&qcom_pinmux 9 GPIO_ACTIVE_HIGH>;
		};

		power_green: power_green {
			function = LED_FUNCTION_POWER;
			color = <LED_COLOR_ID_GREEN>;
			gpios = <&qcom_pinmux 14 GPIO_ACTIVE_HIGH>;
		};

		converter_red {
			label = "red:converter";
			gpios = <&qcom_pinmux 15 GPIO_ACTIVE_HIGH>;
		};

		wlan2g_green {
			label = "green:wlan2g";
			gpios = <&qcom_pinmux 55 GPIO_ACTIVE_HIGH>;
		};

		wlan2g_red {
			label = "red:wlan2g";
			gpios = <&qcom_pinmux 56 GPIO_ACTIVE_HIGH>;
		};

		wlan5g_green {
			label = "green:wlan5g";
			gpios = <&qcom_pinmux 57 GPIO_ACTIVE_HIGH>;
		};

		wlan5g_red {
			label = "red:wlan5g";
			gpios = <&qcom_pinmux 58 GPIO_ACTIVE_HIGH>;
		};

		tv_green {
			label = "green:tv";
			gpios = <&qcom_pinmux 64 GPIO_ACTIVE_HIGH>;
		};

		tv_red {
			label = "red:tv";
			gpios = <&qcom_pinmux 65 GPIO_ACTIVE_HIGH>;
		};
	};
};

&CPU_SPC {
	status = "disabled";
};

&adm_dma {
	status = "okay";
};

&mdio0 {
	status = "okay";

	pinctrl-0 = <&mdio0_pins>;
	pinctrl-names = "default";

switch@10 {
		compatible = "qca,qca8337";
		#address-cells = <1>;
		#size-cells = <0>;
		reg = <0x10>;

		ports {
			#address-cells = <1>;
			#size-cells = <0>;

			port@0 {
				reg = <0>;
				label = "cpu";
				ethernet = <&gmac1>;
				phy-mode = "rgmii";
				tx-internal-delay-ps = <1000>;

				fixed-link {
					speed = <1000>;
					full-duplex;
				};
			};

			port@1 {
				reg = <1>;
				label = "wan";
				phy-mode = "internal";
				phy-handle = <&phy_port1>;
			};

			port@2 {
				reg = <2>;
				label = "lan1";
				phy-mode = "internal";
				phy-handle = <&phy_port2>;
			};

			port@3 {
				reg = <3>;
				label = "lan2";
				phy-mode = "internal";
				phy-handle = <&phy_port3>;
			};

			port@4 {
				reg = <4>;
				label = "lan3";
				phy-mode = "internal";
				phy-handle = <&phy_port4>;
			};

			port@5 {
				reg = <5>;
				label = "lan4";
				phy-mode = "internal";
				phy-handle = <&phy_port5>;
			};

			port@6 {
				reg = <6>;
				label = "cpu";
				ethernet = <&gmac2>;
				phy-mode = "sgmii";
				qca,sgmii-enable-pll;
				qca,sgmii-rxclk-falling-edge;

				fixed-link {
					speed = <1000>;
					full-duplex;
				};
			};
		};

		mdio {
			#address-cells = <1>;
			#size-cells = <0>;

			phy_port1: phy@0 {
				reg = <0>;
			};

			phy_port2: phy@1 {
				reg = <1>;
			};

			phy_port3: phy@2 {
				reg = <2>;
			};

			phy_port4: phy@3 {
				reg = <3>;
			};

			phy_port5: phy@4 {
				reg = <4>;
			};
		};
	};
};

&gmac1 {
	status = "okay";

	phy-mode = "rgmii";
	qcom,id = <1>;

	pinctrl-0 = <&rgmii2_pins>;
	pinctrl-names = "default";

	nvmem-cells = <&macaddr_PRODUCTDATA_6>;
	nvmem-cell-names = "mac-address";

	fixed-link {
		speed = <1000>;
		full-duplex;
	};
};

&gmac2 {
	status = "okay";

	phy-mode = "sgmii";
	qcom,id = <2>;

	nvmem-cells = <&macaddr_PRODUCTDATA_0>;
	nvmem-cell-names = "mac-address";

	fixed-link {
		speed = <1000>;
		full-duplex;
	};
};

&gsbi5 {
	status = "okay";

	qcom,mode = <GSBI_PROT_SPI>;

	spi@1a280000 {
		status = "okay";

		pinctrl-0 = <&spi_pins>;
		pinctrl-names = "default";

		cs-gpios = <&qcom_pinmux 20 GPIO_ACTIVE_HIGH>;

		flash@0 {
			compatible = "jedec,spi-nor";
			spi-max-frequency = <50000000>;
			reg = <0>;

			partitions {
				compatible = "fixed-partitions";
				#address-cells = <1>;
				#size-cells = <1>;

				SBL1@0 {
					label = "SBL1";
					reg = <0x0 0x20000>;
					read-only;
				};

				MIBIB@20000 {
					label = "MIBIB";
					reg = <0x20000 0x20000>;
					read-only;
				};

				SBL2@40000 {
					label = "SBL2";
					reg = <0x40000 0x40000>;
					read-only;
				};

				SBL3@80000 {
					label = "SBL3";
					reg = <0x80000 0x80000>;
					read-only;
				};

				DDRCONFIG@100000 {
					label = "DDRCONFIG";
					reg = <0x100000 0x10000>;
					read-only;
				};

				SSD@110000 {
					label = "SSD";
					reg = <0x110000 0x10000>;
					read-only;
				};

				TZ@120000 {
					label = "TZ";
					reg = <0x120000 0x80000>;
					read-only;
				};

				RPM@1a0000 {
					label = "RPM";
					reg = <0x1a0000 0x80000>;
					read-only;
				};

				APPSBL@220000 {
					label = "APPSBL";
					reg = <0x220000 0x80000>;
					read-only;
				};

				APPSBLENV@2a0000 {
					label = "APPSBLENV";
					reg = <0x2a0000 0x10000>;
				};

				PRODUCTDATA: PRODUCTDATA@2b0000 {
					label = "PRODUCTDATA";
					reg = <0x2b0000 0x30000>;
					read-only;

					nvmem-layout {
						compatible = "fixed-layout";
						#address-cells = <1>;
						#size-cells = <1>;

						macaddr_PRODUCTDATA_0: macaddr@0 {
							reg = <0x0 0x6>;
						};

						macaddr_PRODUCTDATA_6: macaddr@6 {
							reg = <0x6 0x6>;
						};

						macaddr_PRODUCTDATA_c: macaddr@c {
							reg = <0xc 0x6>;
						};

						macaddr_PRODUCTDATA_12: macaddr@12 {
							reg = <0x12 0x6>;
						};
					};
				};

				ART@2e0000 {
					label = "ART";
					reg = <0x2e0000 0x40000>;
					read-only;

					nvmem-layout {
						compatible = "fixed-layout";
						#address-cells = <1>;
						#size-cells = <1>;

						precal_ART_1000: precal@1000 {
							reg = <0x1000 0x2f20>;
						};

						precal_ART_5000: precal@5000 {
							reg = <0x5000 0x2f20>;
						};
					};
				};

				TP@320000 {
					label = "TP";
					reg = <0x320000 0x40000>;
					read-only;
				};

				TINY@360000 {
					label = "TINY";
					reg = <0x360000 0x500000>;
					read-only;
				};

				firmware@860000 {
					compatible = "denx,uimage";
					label = "firmware";
					reg = <0x860000 0x17a0000>;
				};
			};
		};
	};
};

&hs_phy_0 {
	status = "okay";
};

&ss_phy_0 {
	status = "okay";
};

&usb3_0 {
	status = "okay";

	pinctrl-0 = <&usb_pwr_en_pins>;
	pinctrl-names = "default";
};

&hs_phy_1 {
	status = "okay";
};

&ss_phy_1 {
	status = "okay";
};

&usb3_1 {
	status = "okay";
};

&pcie0 {
	status = "okay";

	bridge@0,0 {
		reg = <0x00000000 0 0 0 0>;
		#address-cells = <3>;
		#size-cells = <2>;
		ranges;

		wifi@1,0 {
			compatible = "qcom,ath10k";
			reg = <0x00010000 0 0 0 0>;

			nvmem-cells = <&macaddr_PRODUCTDATA_12>, <&precal_ART_1000>;
			nvmem-cell-names = "mac-address", "pre-calibration";
		};
	};
};

&pcie1 {
	status = "okay";
	max-link-speed = <1>;

	bridge@0,0 {
		reg = <0x00000000 0 0 0 0>;
		#address-cells = <3>;
		#size-cells = <2>;
		ranges;

		wifi@1,0 {
			compatible = "qcom,ath10k";
			reg = <0x00010000 0 0 0 0>;

			nvmem-cells = <&macaddr_PRODUCTDATA_c>, <&precal_ART_5000>;
			nvmem-cell-names = "mac-address", "pre-calibration";
		};
	};
};

&qcom_pinmux {
	button_pins: button_pins {
		mux {
			pins = "gpio16", "gpio54", "gpio24", "gpio25";
			function = "gpio";
			drive-strength = <2>;
			bias-pull-up;
		};
	};

	led_pins: led_pins {
		mux {
			pins = "gpio6", "gpio7", "gpio8", "gpio9", "gpio14",
				"gpio15", "gpio55", "gpio56", "gpio57", "gpio58",
				"gpio64", "gpio65";
			function = "gpio";
			drive-strength = <2>;
			bias-pull-down;
		};
	};

	spi_pins: spi_pins {
		mux {
			pins = "gpio18", "gpio19", "gpio21";
			function = "gsbi5";
			bias-pull-down;
		};

		data {
			pins = "gpio18", "gpio19";
			drive-strength = <10>;
		};

		cs {
			pins = "gpio20";
			drive-strength = <10>;
			bias-pull-up;
		};

		clk {
			pins = "gpio21";
			drive-strength = <12>;
		};
	};

	usb_pwr_en_pins: usb_pwr_en_pins {
		mux {
			pins = "gpio22";
			function = "gpio";
			drive-strength = <2>;
			bias-pull-down;
			output-high;
		};
	};
};
