--- a/arch/arm64/boot/dts/rockchip/rk3576-rock-4d.dts
+++ b/arch/arm64/boot/dts/rockchip/rk3576-rock-4d.dts
@@ -771,7 +771,7 @@
 	max-frequency = <200000000>;
 	no-sdio;
 	no-mmc;
-	sd-uhs-sdr104;
+	sd-uhs-sdr50;
 	vmmc-supply = <&vcc_3v3_s3>;
 	vqmmc-supply = <&vccio_sd_s0>;
 	status = "okay";
