From 4c452f7ea86212934ae896842847d1671e13a18b Mon Sep 17 00:00:00 2001
From: "SkyLake.Huang" <skylake.huang@mediatek.com>
Date: Sat, 9 Nov 2024 00:34:51 +0800
Subject: [PATCH] net: phy: mediatek: Re-organize MediaTek ethernet phy drivers

Re-organize MediaTek ethernet phy driver files and get ready to integrate
some common functions and add new 2.5G phy driver.
mtk-ge.c: MT7530 Gphy on MT7621 & MT7531 Gphy
mtk-ge-soc.c: Built-in Gphy on MT7981 & Built-in switch Gphy on MT7988
mtk-2p5ge.c: Planned for built-in 2.5G phy on MT7988

Reviewed-by: Andrew Lunn <andrew@lunn.ch>
Signed-off-by: SkyLake.Huang <skylake.huang@mediatek.com>
Signed-off-by: David S. Miller <davem@davemloft.net>
---
 MAINTAINERS                                   |  4 ++--
 drivers/net/phy/Kconfig                       | 17 +-------------
 drivers/net/phy/Makefile                      |  3 +--
 drivers/net/phy/mediatek/Kconfig              | 22 +++++++++++++++++++
 drivers/net/phy/mediatek/Makefile             |  3 +++
 .../mtk-ge-soc.c}                             |  0
 .../phy/{mediatek-ge.c => mediatek/mtk-ge.c}  |  0
 7 files changed, 29 insertions(+), 20 deletions(-)
 create mode 100644 drivers/net/phy/mediatek/Kconfig
 create mode 100644 drivers/net/phy/mediatek/Makefile
 rename drivers/net/phy/{mediatek-ge-soc.c => mediatek/mtk-ge-soc.c} (100%)
 rename drivers/net/phy/{mediatek-ge.c => mediatek/mtk-ge.c} (100%)

--- a/drivers/net/phy/Kconfig
+++ b/drivers/net/phy/Kconfig
@@ -234,22 +234,7 @@ config MAXLINEAR_GPHY
 	  Support for the Maxlinear GPY115, GPY211, GPY212, GPY215,
 	  GPY241, GPY245 PHYs.
 
-config MEDIATEK_GE_PHY
-	tristate "MediaTek Gigabit Ethernet PHYs"
-	help
-	  Supports the MediaTek Gigabit Ethernet PHYs.
-
-config MEDIATEK_GE_SOC_PHY
-	tristate "MediaTek SoC Ethernet PHYs"
-	depends on (ARM64 && ARCH_MEDIATEK) || COMPILE_TEST
-	depends on NVMEM_MTK_EFUSE
-	help
-	  Supports MediaTek SoC built-in Gigabit Ethernet PHYs.
-
-	  Include support for built-in Ethernet PHYs which are present in
-	  the MT7981 and MT7988 SoCs. These PHYs need calibration data
-	  present in the SoCs efuse and will dynamically calibrate VCM
-	  (common-mode voltage) during startup.
+source "drivers/net/phy/mediatek/Kconfig"
 
 config MICREL_PHY
 	tristate "Micrel PHYs"
--- a/drivers/net/phy/Makefile
+++ b/drivers/net/phy/Makefile
@@ -66,8 +66,7 @@ obj-$(CONFIG_MARVELL_PHY)	+= marvell.o
 obj-$(CONFIG_MARVELL_88Q2XXX_PHY)	+= marvell-88q2xxx.o
 obj-$(CONFIG_MARVELL_88X2222_PHY)	+= marvell-88x2222.o
 obj-$(CONFIG_MAXLINEAR_GPHY)	+= mxl-gpy.o
-obj-$(CONFIG_MEDIATEK_GE_PHY)	+= mediatek-ge.o
-obj-$(CONFIG_MEDIATEK_GE_SOC_PHY)	+= mediatek-ge-soc.o
+obj-y				+= mediatek/
 obj-$(CONFIG_MESON_GXL_PHY)	+= meson-gxl.o
 obj-$(CONFIG_MICREL_KS8995MA)	+= spi_ks8995.o
 obj-$(CONFIG_MICREL_PHY)	+= micrel.o
--- /dev/null
+++ b/drivers/net/phy/mediatek/Kconfig
@@ -0,0 +1,22 @@
+# SPDX-License-Identifier: GPL-2.0-only
+config MEDIATEK_GE_PHY
+	tristate "MediaTek Gigabit Ethernet PHYs"
+	help
+	  Supports the MediaTek non-built-in Gigabit Ethernet PHYs.
+
+	  Non-built-in Gigabit Ethernet PHYs include mt7530/mt7531.
+	  You may find mt7530 inside mt7621. This driver shares some
+	  common operations with MediaTek SoC built-in Gigabit
+	  Ethernet PHYs.
+
+config MEDIATEK_GE_SOC_PHY
+	tristate "MediaTek SoC Ethernet PHYs"
+	depends on (ARM64 && ARCH_MEDIATEK) || COMPILE_TEST
+	depends on NVMEM_MTK_EFUSE
+	help
+	  Supports MediaTek SoC built-in Gigabit Ethernet PHYs.
+
+	  Include support for built-in Ethernet PHYs which are present in
+	  the MT7981 and MT7988 SoCs. These PHYs need calibration data
+	  present in the SoCs efuse and will dynamically calibrate VCM
+	  (common-mode voltage) during startup.
--- /dev/null
+++ b/drivers/net/phy/mediatek/Makefile
@@ -0,0 +1,3 @@
+# SPDX-License-Identifier: GPL-2.0
+obj-$(CONFIG_MEDIATEK_GE_PHY)		+= mtk-ge.o
+obj-$(CONFIG_MEDIATEK_GE_SOC_PHY)	+= mtk-ge-soc.o
--- a/drivers/net/phy/mediatek-ge-soc.c
+++ /dev/null
@@ -1,1610 +0,0 @@
-// SPDX-License-Identifier: GPL-2.0+
-#include <linux/bitfield.h>
-#include <linux/bitmap.h>
-#include <linux/mfd/syscon.h>
-#include <linux/module.h>
-#include <linux/nvmem-consumer.h>
-#include <linux/pinctrl/consumer.h>
-#include <linux/phy.h>
-#include <linux/regmap.h>
-
-#define MTK_GPHY_ID_MT7981			0x03a29461
-#define MTK_GPHY_ID_MT7988			0x03a29481
-
-#define MTK_EXT_PAGE_ACCESS			0x1f
-#define MTK_PHY_PAGE_STANDARD			0x0000
-#define MTK_PHY_PAGE_EXTENDED_3			0x0003
-
-#define MTK_PHY_LPI_REG_14			0x14
-#define MTK_PHY_LPI_WAKE_TIMER_1000_MASK	GENMASK(8, 0)
-
-#define MTK_PHY_LPI_REG_1c			0x1c
-#define MTK_PHY_SMI_DET_ON_THRESH_MASK		GENMASK(13, 8)
-
-#define MTK_PHY_PAGE_EXTENDED_2A30		0x2a30
-#define MTK_PHY_PAGE_EXTENDED_52B5		0x52b5
-
-#define ANALOG_INTERNAL_OPERATION_MAX_US	20
-#define TXRESERVE_MIN				0
-#define TXRESERVE_MAX				7
-
-#define MTK_PHY_ANARG_RG			0x10
-#define   MTK_PHY_TCLKOFFSET_MASK		GENMASK(12, 8)
-
-/* Registers on MDIO_MMD_VEND1 */
-#define MTK_PHY_TXVLD_DA_RG			0x12
-#define   MTK_PHY_DA_TX_I2MPB_A_GBE_MASK	GENMASK(15, 10)
-#define   MTK_PHY_DA_TX_I2MPB_A_TBT_MASK	GENMASK(5, 0)
-
-#define MTK_PHY_TX_I2MPB_TEST_MODE_A2		0x16
-#define   MTK_PHY_DA_TX_I2MPB_A_HBT_MASK	GENMASK(15, 10)
-#define   MTK_PHY_DA_TX_I2MPB_A_TST_MASK	GENMASK(5, 0)
-
-#define MTK_PHY_TX_I2MPB_TEST_MODE_B1		0x17
-#define   MTK_PHY_DA_TX_I2MPB_B_GBE_MASK	GENMASK(13, 8)
-#define   MTK_PHY_DA_TX_I2MPB_B_TBT_MASK	GENMASK(5, 0)
-
-#define MTK_PHY_TX_I2MPB_TEST_MODE_B2		0x18
-#define   MTK_PHY_DA_TX_I2MPB_B_HBT_MASK	GENMASK(13, 8)
-#define   MTK_PHY_DA_TX_I2MPB_B_TST_MASK	GENMASK(5, 0)
-
-#define MTK_PHY_TX_I2MPB_TEST_MODE_C1		0x19
-#define   MTK_PHY_DA_TX_I2MPB_C_GBE_MASK	GENMASK(13, 8)
-#define   MTK_PHY_DA_TX_I2MPB_C_TBT_MASK	GENMASK(5, 0)
-
-#define MTK_PHY_TX_I2MPB_TEST_MODE_C2		0x20
-#define   MTK_PHY_DA_TX_I2MPB_C_HBT_MASK	GENMASK(13, 8)
-#define   MTK_PHY_DA_TX_I2MPB_C_TST_MASK	GENMASK(5, 0)
-
-#define MTK_PHY_TX_I2MPB_TEST_MODE_D1		0x21
-#define   MTK_PHY_DA_TX_I2MPB_D_GBE_MASK	GENMASK(13, 8)
-#define   MTK_PHY_DA_TX_I2MPB_D_TBT_MASK	GENMASK(5, 0)
-
-#define MTK_PHY_TX_I2MPB_TEST_MODE_D2		0x22
-#define   MTK_PHY_DA_TX_I2MPB_D_HBT_MASK	GENMASK(13, 8)
-#define   MTK_PHY_DA_TX_I2MPB_D_TST_MASK	GENMASK(5, 0)
-
-#define MTK_PHY_RXADC_CTRL_RG7			0xc6
-#define   MTK_PHY_DA_AD_BUF_BIAS_LP_MASK	GENMASK(9, 8)
-
-#define MTK_PHY_RXADC_CTRL_RG9			0xc8
-#define   MTK_PHY_DA_RX_PSBN_TBT_MASK		GENMASK(14, 12)
-#define   MTK_PHY_DA_RX_PSBN_HBT_MASK		GENMASK(10, 8)
-#define   MTK_PHY_DA_RX_PSBN_GBE_MASK		GENMASK(6, 4)
-#define   MTK_PHY_DA_RX_PSBN_LP_MASK		GENMASK(2, 0)
-
-#define MTK_PHY_LDO_OUTPUT_V			0xd7
-
-#define MTK_PHY_RG_ANA_CAL_RG0			0xdb
-#define   MTK_PHY_RG_CAL_CKINV			BIT(12)
-#define   MTK_PHY_RG_ANA_CALEN			BIT(8)
-#define   MTK_PHY_RG_ZCALEN_A			BIT(0)
-
-#define MTK_PHY_RG_ANA_CAL_RG1			0xdc
-#define   MTK_PHY_RG_ZCALEN_B			BIT(12)
-#define   MTK_PHY_RG_ZCALEN_C			BIT(8)
-#define   MTK_PHY_RG_ZCALEN_D			BIT(4)
-#define   MTK_PHY_RG_TXVOS_CALEN		BIT(0)
-
-#define MTK_PHY_RG_ANA_CAL_RG5			0xe0
-#define   MTK_PHY_RG_REXT_TRIM_MASK		GENMASK(13, 8)
-
-#define MTK_PHY_RG_TX_FILTER			0xfe
-
-#define MTK_PHY_RG_LPI_PCS_DSP_CTRL_REG120	0x120
-#define   MTK_PHY_LPI_SIG_EN_LO_THRESH1000_MASK	GENMASK(12, 8)
-#define   MTK_PHY_LPI_SIG_EN_HI_THRESH1000_MASK	GENMASK(4, 0)
-
-#define MTK_PHY_RG_LPI_PCS_DSP_CTRL_REG122	0x122
-#define   MTK_PHY_LPI_NORM_MSE_HI_THRESH1000_MASK	GENMASK(7, 0)
-
-#define MTK_PHY_RG_TESTMUX_ADC_CTRL		0x144
-#define   MTK_PHY_RG_TXEN_DIG_MASK		GENMASK(5, 5)
-
-#define MTK_PHY_RG_CR_TX_AMP_OFFSET_A_B		0x172
-#define   MTK_PHY_CR_TX_AMP_OFFSET_A_MASK	GENMASK(13, 8)
-#define   MTK_PHY_CR_TX_AMP_OFFSET_B_MASK	GENMASK(6, 0)
-
-#define MTK_PHY_RG_CR_TX_AMP_OFFSET_C_D		0x173
-#define   MTK_PHY_CR_TX_AMP_OFFSET_C_MASK	GENMASK(13, 8)
-#define   MTK_PHY_CR_TX_AMP_OFFSET_D_MASK	GENMASK(6, 0)
-
-#define MTK_PHY_RG_AD_CAL_COMP			0x17a
-#define   MTK_PHY_AD_CAL_COMP_OUT_MASK		GENMASK(8, 8)
-
-#define MTK_PHY_RG_AD_CAL_CLK			0x17b
-#define   MTK_PHY_DA_CAL_CLK			BIT(0)
-
-#define MTK_PHY_RG_AD_CALIN			0x17c
-#define   MTK_PHY_DA_CALIN_FLAG			BIT(0)
-
-#define MTK_PHY_RG_DASN_DAC_IN0_A		0x17d
-#define   MTK_PHY_DASN_DAC_IN0_A_MASK		GENMASK(9, 0)
-
-#define MTK_PHY_RG_DASN_DAC_IN0_B		0x17e
-#define   MTK_PHY_DASN_DAC_IN0_B_MASK		GENMASK(9, 0)
-
-#define MTK_PHY_RG_DASN_DAC_IN0_C		0x17f
-#define   MTK_PHY_DASN_DAC_IN0_C_MASK		GENMASK(9, 0)
-
-#define MTK_PHY_RG_DASN_DAC_IN0_D		0x180
-#define   MTK_PHY_DASN_DAC_IN0_D_MASK		GENMASK(9, 0)
-
-#define MTK_PHY_RG_DASN_DAC_IN1_A		0x181
-#define   MTK_PHY_DASN_DAC_IN1_A_MASK		GENMASK(9, 0)
-
-#define MTK_PHY_RG_DASN_DAC_IN1_B		0x182
-#define   MTK_PHY_DASN_DAC_IN1_B_MASK		GENMASK(9, 0)
-
-#define MTK_PHY_RG_DASN_DAC_IN1_C		0x183
-#define   MTK_PHY_DASN_DAC_IN1_C_MASK		GENMASK(9, 0)
-
-#define MTK_PHY_RG_DASN_DAC_IN1_D		0x184
-#define   MTK_PHY_DASN_DAC_IN1_D_MASK		GENMASK(9, 0)
-
-#define MTK_PHY_RG_DEV1E_REG19b			0x19b
-#define   MTK_PHY_BYPASS_DSP_LPI_READY		BIT(8)
-
-#define MTK_PHY_RG_LP_IIR2_K1_L			0x22a
-#define MTK_PHY_RG_LP_IIR2_K1_U			0x22b
-#define MTK_PHY_RG_LP_IIR2_K2_L			0x22c
-#define MTK_PHY_RG_LP_IIR2_K2_U			0x22d
-#define MTK_PHY_RG_LP_IIR2_K3_L			0x22e
-#define MTK_PHY_RG_LP_IIR2_K3_U			0x22f
-#define MTK_PHY_RG_LP_IIR2_K4_L			0x230
-#define MTK_PHY_RG_LP_IIR2_K4_U			0x231
-#define MTK_PHY_RG_LP_IIR2_K5_L			0x232
-#define MTK_PHY_RG_LP_IIR2_K5_U			0x233
-
-#define MTK_PHY_RG_DEV1E_REG234			0x234
-#define   MTK_PHY_TR_OPEN_LOOP_EN_MASK		GENMASK(0, 0)
-#define   MTK_PHY_LPF_X_AVERAGE_MASK		GENMASK(7, 4)
-#define   MTK_PHY_TR_LP_IIR_EEE_EN		BIT(12)
-
-#define MTK_PHY_RG_LPF_CNT_VAL			0x235
-
-#define MTK_PHY_RG_DEV1E_REG238			0x238
-#define   MTK_PHY_LPI_SLV_SEND_TX_TIMER_MASK	GENMASK(8, 0)
-#define   MTK_PHY_LPI_SLV_SEND_TX_EN		BIT(12)
-
-#define MTK_PHY_RG_DEV1E_REG239			0x239
-#define   MTK_PHY_LPI_SEND_LOC_TIMER_MASK	GENMASK(8, 0)
-#define   MTK_PHY_LPI_TXPCS_LOC_RCV		BIT(12)
-
-#define MTK_PHY_RG_DEV1E_REG27C			0x27c
-#define   MTK_PHY_VGASTATE_FFE_THR_ST1_MASK	GENMASK(12, 8)
-#define MTK_PHY_RG_DEV1E_REG27D			0x27d
-#define   MTK_PHY_VGASTATE_FFE_THR_ST2_MASK	GENMASK(4, 0)
-
-#define MTK_PHY_RG_DEV1E_REG2C7			0x2c7
-#define   MTK_PHY_MAX_GAIN_MASK			GENMASK(4, 0)
-#define   MTK_PHY_MIN_GAIN_MASK			GENMASK(12, 8)
-
-#define MTK_PHY_RG_DEV1E_REG2D1			0x2d1
-#define   MTK_PHY_VCO_SLICER_THRESH_BITS_HIGH_EEE_MASK	GENMASK(7, 0)
-#define   MTK_PHY_LPI_SKIP_SD_SLV_TR		BIT(8)
-#define   MTK_PHY_LPI_TR_READY			BIT(9)
-#define   MTK_PHY_LPI_VCO_EEE_STG0_EN		BIT(10)
-
-#define MTK_PHY_RG_DEV1E_REG323			0x323
-#define   MTK_PHY_EEE_WAKE_MAS_INT_DC		BIT(0)
-#define   MTK_PHY_EEE_WAKE_SLV_INT_DC		BIT(4)
-
-#define MTK_PHY_RG_DEV1E_REG324			0x324
-#define   MTK_PHY_SMI_DETCNT_MAX_MASK		GENMASK(5, 0)
-#define   MTK_PHY_SMI_DET_MAX_EN		BIT(8)
-
-#define MTK_PHY_RG_DEV1E_REG326			0x326
-#define   MTK_PHY_LPI_MODE_SD_ON		BIT(0)
-#define   MTK_PHY_RESET_RANDUPD_CNT		BIT(1)
-#define   MTK_PHY_TREC_UPDATE_ENAB_CLR		BIT(2)
-#define   MTK_PHY_LPI_QUIT_WAIT_DFE_SIG_DET_OFF	BIT(4)
-#define   MTK_PHY_TR_READY_SKIP_AFE_WAKEUP	BIT(5)
-
-#define MTK_PHY_LDO_PUMP_EN_PAIRAB		0x502
-#define MTK_PHY_LDO_PUMP_EN_PAIRCD		0x503
-
-#define MTK_PHY_DA_TX_R50_PAIR_A		0x53d
-#define MTK_PHY_DA_TX_R50_PAIR_B		0x53e
-#define MTK_PHY_DA_TX_R50_PAIR_C		0x53f
-#define MTK_PHY_DA_TX_R50_PAIR_D		0x540
-
-/* Registers on MDIO_MMD_VEND2 */
-#define MTK_PHY_LED0_ON_CTRL			0x24
-#define MTK_PHY_LED1_ON_CTRL			0x26
-#define   MTK_PHY_LED_ON_MASK			GENMASK(6, 0)
-#define   MTK_PHY_LED_ON_LINK1000		BIT(0)
-#define   MTK_PHY_LED_ON_LINK100		BIT(1)
-#define   MTK_PHY_LED_ON_LINK10			BIT(2)
-#define   MTK_PHY_LED_ON_LINK			(MTK_PHY_LED_ON_LINK10 |\
-						 MTK_PHY_LED_ON_LINK100 |\
-						 MTK_PHY_LED_ON_LINK1000)
-#define   MTK_PHY_LED_ON_LINKDOWN		BIT(3)
-#define   MTK_PHY_LED_ON_FDX			BIT(4) /* Full duplex */
-#define   MTK_PHY_LED_ON_HDX			BIT(5) /* Half duplex */
-#define   MTK_PHY_LED_ON_FORCE_ON		BIT(6)
-#define   MTK_PHY_LED_ON_POLARITY		BIT(14)
-#define   MTK_PHY_LED_ON_ENABLE			BIT(15)
-
-#define MTK_PHY_LED0_BLINK_CTRL			0x25
-#define MTK_PHY_LED1_BLINK_CTRL			0x27
-#define   MTK_PHY_LED_BLINK_1000TX		BIT(0)
-#define   MTK_PHY_LED_BLINK_1000RX		BIT(1)
-#define   MTK_PHY_LED_BLINK_100TX		BIT(2)
-#define   MTK_PHY_LED_BLINK_100RX		BIT(3)
-#define   MTK_PHY_LED_BLINK_10TX		BIT(4)
-#define   MTK_PHY_LED_BLINK_10RX		BIT(5)
-#define   MTK_PHY_LED_BLINK_RX			(MTK_PHY_LED_BLINK_10RX |\
-						 MTK_PHY_LED_BLINK_100RX |\
-						 MTK_PHY_LED_BLINK_1000RX)
-#define   MTK_PHY_LED_BLINK_TX			(MTK_PHY_LED_BLINK_10TX |\
-						 MTK_PHY_LED_BLINK_100TX |\
-						 MTK_PHY_LED_BLINK_1000TX)
-#define   MTK_PHY_LED_BLINK_COLLISION		BIT(6)
-#define   MTK_PHY_LED_BLINK_RX_CRC_ERR		BIT(7)
-#define   MTK_PHY_LED_BLINK_RX_IDLE_ERR		BIT(8)
-#define   MTK_PHY_LED_BLINK_FORCE_BLINK		BIT(9)
-
-#define MTK_PHY_LED1_DEFAULT_POLARITIES		BIT(1)
-
-#define MTK_PHY_RG_BG_RASEL			0x115
-#define   MTK_PHY_RG_BG_RASEL_MASK		GENMASK(2, 0)
-
-/* 'boottrap' register reflecting the configuration of the 4 PHY LEDs */
-#define RG_GPIO_MISC_TPBANK0			0x6f0
-#define   RG_GPIO_MISC_TPBANK0_BOOTMODE		GENMASK(11, 8)
-
-/* These macro privides efuse parsing for internal phy. */
-#define EFS_DA_TX_I2MPB_A(x)			(((x) >> 0) & GENMASK(5, 0))
-#define EFS_DA_TX_I2MPB_B(x)			(((x) >> 6) & GENMASK(5, 0))
-#define EFS_DA_TX_I2MPB_C(x)			(((x) >> 12) & GENMASK(5, 0))
-#define EFS_DA_TX_I2MPB_D(x)			(((x) >> 18) & GENMASK(5, 0))
-#define EFS_DA_TX_AMP_OFFSET_A(x)		(((x) >> 24) & GENMASK(5, 0))
-
-#define EFS_DA_TX_AMP_OFFSET_B(x)		(((x) >> 0) & GENMASK(5, 0))
-#define EFS_DA_TX_AMP_OFFSET_C(x)		(((x) >> 6) & GENMASK(5, 0))
-#define EFS_DA_TX_AMP_OFFSET_D(x)		(((x) >> 12) & GENMASK(5, 0))
-#define EFS_DA_TX_R50_A(x)			(((x) >> 18) & GENMASK(5, 0))
-#define EFS_DA_TX_R50_B(x)			(((x) >> 24) & GENMASK(5, 0))
-
-#define EFS_DA_TX_R50_C(x)			(((x) >> 0) & GENMASK(5, 0))
-#define EFS_DA_TX_R50_D(x)			(((x) >> 6) & GENMASK(5, 0))
-
-#define EFS_RG_BG_RASEL(x)			(((x) >> 4) & GENMASK(2, 0))
-#define EFS_RG_REXT_TRIM(x)			(((x) >> 7) & GENMASK(5, 0))
-
-enum {
-	NO_PAIR,
-	PAIR_A,
-	PAIR_B,
-	PAIR_C,
-	PAIR_D,
-};
-
-enum calibration_mode {
-	EFUSE_K,
-	SW_K
-};
-
-enum CAL_ITEM {
-	REXT,
-	TX_OFFSET,
-	TX_AMP,
-	TX_R50,
-	TX_VCM
-};
-
-enum CAL_MODE {
-	EFUSE_M,
-	SW_M
-};
-
-#define MTK_PHY_LED_STATE_FORCE_ON	0
-#define MTK_PHY_LED_STATE_FORCE_BLINK	1
-#define MTK_PHY_LED_STATE_NETDEV	2
-
-struct mtk_socphy_priv {
-	unsigned long		led_state;
-};
-
-struct mtk_socphy_shared {
-	u32			boottrap;
-	struct mtk_socphy_priv	priv[4];
-};
-
-static int mtk_socphy_read_page(struct phy_device *phydev)
-{
-	return __phy_read(phydev, MTK_EXT_PAGE_ACCESS);
-}
-
-static int mtk_socphy_write_page(struct phy_device *phydev, int page)
-{
-	return __phy_write(phydev, MTK_EXT_PAGE_ACCESS, page);
-}
-
-/* One calibration cycle consists of:
- * 1.Set DA_CALIN_FLAG high to start calibration. Keep it high
- *   until AD_CAL_COMP is ready to output calibration result.
- * 2.Wait until DA_CAL_CLK is available.
- * 3.Fetch AD_CAL_COMP_OUT.
- */
-static int cal_cycle(struct phy_device *phydev, int devad,
-		     u32 regnum, u16 mask, u16 cal_val)
-{
-	int reg_val;
-	int ret;
-
-	phy_modify_mmd(phydev, devad, regnum,
-		       mask, cal_val);
-	phy_set_bits_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_RG_AD_CALIN,
-			 MTK_PHY_DA_CALIN_FLAG);
-
-	ret = phy_read_mmd_poll_timeout(phydev, MDIO_MMD_VEND1,
-					MTK_PHY_RG_AD_CAL_CLK, reg_val,
-					reg_val & MTK_PHY_DA_CAL_CLK, 500,
-					ANALOG_INTERNAL_OPERATION_MAX_US,
-					false);
-	if (ret) {
-		phydev_err(phydev, "Calibration cycle timeout\n");
-		return ret;
-	}
-
-	phy_clear_bits_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_RG_AD_CALIN,
-			   MTK_PHY_DA_CALIN_FLAG);
-	ret = phy_read_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_RG_AD_CAL_COMP);
-	if (ret < 0)
-		return ret;
-	ret = FIELD_GET(MTK_PHY_AD_CAL_COMP_OUT_MASK, ret);
-	phydev_dbg(phydev, "cal_val: 0x%x, ret: %d\n", cal_val, ret);
-
-	return ret;
-}
-
-static int rext_fill_result(struct phy_device *phydev, u16 *buf)
-{
-	phy_modify_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_RG_ANA_CAL_RG5,
-		       MTK_PHY_RG_REXT_TRIM_MASK, buf[0] << 8);
-	phy_modify_mmd(phydev, MDIO_MMD_VEND2, MTK_PHY_RG_BG_RASEL,
-		       MTK_PHY_RG_BG_RASEL_MASK, buf[1]);
-
-	return 0;
-}
-
-static int rext_cal_efuse(struct phy_device *phydev, u32 *buf)
-{
-	u16 rext_cal_val[2];
-
-	rext_cal_val[0] = EFS_RG_REXT_TRIM(buf[3]);
-	rext_cal_val[1] = EFS_RG_BG_RASEL(buf[3]);
-	rext_fill_result(phydev, rext_cal_val);
-
-	return 0;
-}
-
-static int tx_offset_fill_result(struct phy_device *phydev, u16 *buf)
-{
-	phy_modify_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_RG_CR_TX_AMP_OFFSET_A_B,
-		       MTK_PHY_CR_TX_AMP_OFFSET_A_MASK, buf[0] << 8);
-	phy_modify_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_RG_CR_TX_AMP_OFFSET_A_B,
-		       MTK_PHY_CR_TX_AMP_OFFSET_B_MASK, buf[1]);
-	phy_modify_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_RG_CR_TX_AMP_OFFSET_C_D,
-		       MTK_PHY_CR_TX_AMP_OFFSET_C_MASK, buf[2] << 8);
-	phy_modify_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_RG_CR_TX_AMP_OFFSET_C_D,
-		       MTK_PHY_CR_TX_AMP_OFFSET_D_MASK, buf[3]);
-
-	return 0;
-}
-
-static int tx_offset_cal_efuse(struct phy_device *phydev, u32 *buf)
-{
-	u16 tx_offset_cal_val[4];
-
-	tx_offset_cal_val[0] = EFS_DA_TX_AMP_OFFSET_A(buf[0]);
-	tx_offset_cal_val[1] = EFS_DA_TX_AMP_OFFSET_B(buf[1]);
-	tx_offset_cal_val[2] = EFS_DA_TX_AMP_OFFSET_C(buf[1]);
-	tx_offset_cal_val[3] = EFS_DA_TX_AMP_OFFSET_D(buf[1]);
-
-	tx_offset_fill_result(phydev, tx_offset_cal_val);
-
-	return 0;
-}
-
-static int tx_amp_fill_result(struct phy_device *phydev, u16 *buf)
-{
-	const int vals_9481[16] = { 10, 6, 6, 10,
-				    10, 6, 6, 10,
-				    10, 6, 6, 10,
-				    10, 6, 6, 10 };
-	const int vals_9461[16] = { 7, 1, 4, 7,
-				    7, 1, 4, 7,
-				    7, 1, 4, 7,
-				    7, 1, 4, 7 };
-	int bias[16] = {};
-	int i;
-
-	switch (phydev->drv->phy_id) {
-	case MTK_GPHY_ID_MT7981:
-		/* We add some calibration to efuse values
-		 * due to board level influence.
-		 * GBE: +7, TBT: +1, HBT: +4, TST: +7
-		 */
-		memcpy(bias, (const void *)vals_9461, sizeof(bias));
-		break;
-	case MTK_GPHY_ID_MT7988:
-		memcpy(bias, (const void *)vals_9481, sizeof(bias));
-		break;
-	}
-
-	/* Prevent overflow */
-	for (i = 0; i < 12; i++) {
-		if (buf[i >> 2] + bias[i] > 63) {
-			buf[i >> 2] = 63;
-			bias[i] = 0;
-		}
-	}
-
-	phy_modify_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_TXVLD_DA_RG,
-		       MTK_PHY_DA_TX_I2MPB_A_GBE_MASK,
-		       FIELD_PREP(MTK_PHY_DA_TX_I2MPB_A_GBE_MASK,
-				  buf[0] + bias[0]));
-	phy_modify_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_TXVLD_DA_RG,
-		       MTK_PHY_DA_TX_I2MPB_A_TBT_MASK,
-		       FIELD_PREP(MTK_PHY_DA_TX_I2MPB_A_TBT_MASK,
-				  buf[0] + bias[1]));
-	phy_modify_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_TX_I2MPB_TEST_MODE_A2,
-		       MTK_PHY_DA_TX_I2MPB_A_HBT_MASK,
-		       FIELD_PREP(MTK_PHY_DA_TX_I2MPB_A_HBT_MASK,
-				  buf[0] + bias[2]));
-	phy_modify_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_TX_I2MPB_TEST_MODE_A2,
-		       MTK_PHY_DA_TX_I2MPB_A_TST_MASK,
-		       FIELD_PREP(MTK_PHY_DA_TX_I2MPB_A_TST_MASK,
-				  buf[0] + bias[3]));
-
-	phy_modify_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_TX_I2MPB_TEST_MODE_B1,
-		       MTK_PHY_DA_TX_I2MPB_B_GBE_MASK,
-		       FIELD_PREP(MTK_PHY_DA_TX_I2MPB_B_GBE_MASK,
-				  buf[1] + bias[4]));
-	phy_modify_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_TX_I2MPB_TEST_MODE_B1,
-		       MTK_PHY_DA_TX_I2MPB_B_TBT_MASK,
-		       FIELD_PREP(MTK_PHY_DA_TX_I2MPB_B_TBT_MASK,
-				  buf[1] + bias[5]));
-	phy_modify_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_TX_I2MPB_TEST_MODE_B2,
-		       MTK_PHY_DA_TX_I2MPB_B_HBT_MASK,
-		       FIELD_PREP(MTK_PHY_DA_TX_I2MPB_B_HBT_MASK,
-				  buf[1] + bias[6]));
-	phy_modify_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_TX_I2MPB_TEST_MODE_B2,
-		       MTK_PHY_DA_TX_I2MPB_B_TST_MASK,
-		       FIELD_PREP(MTK_PHY_DA_TX_I2MPB_B_TST_MASK,
-				  buf[1] + bias[7]));
-
-	phy_modify_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_TX_I2MPB_TEST_MODE_C1,
-		       MTK_PHY_DA_TX_I2MPB_C_GBE_MASK,
-		       FIELD_PREP(MTK_PHY_DA_TX_I2MPB_C_GBE_MASK,
-				  buf[2] + bias[8]));
-	phy_modify_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_TX_I2MPB_TEST_MODE_C1,
-		       MTK_PHY_DA_TX_I2MPB_C_TBT_MASK,
-		       FIELD_PREP(MTK_PHY_DA_TX_I2MPB_C_TBT_MASK,
-				  buf[2] + bias[9]));
-	phy_modify_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_TX_I2MPB_TEST_MODE_C2,
-		       MTK_PHY_DA_TX_I2MPB_C_HBT_MASK,
-		       FIELD_PREP(MTK_PHY_DA_TX_I2MPB_C_HBT_MASK,
-				  buf[2] + bias[10]));
-	phy_modify_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_TX_I2MPB_TEST_MODE_C2,
-		       MTK_PHY_DA_TX_I2MPB_C_TST_MASK,
-		       FIELD_PREP(MTK_PHY_DA_TX_I2MPB_C_TST_MASK,
-				  buf[2] + bias[11]));
-
-	phy_modify_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_TX_I2MPB_TEST_MODE_D1,
-		       MTK_PHY_DA_TX_I2MPB_D_GBE_MASK,
-		       FIELD_PREP(MTK_PHY_DA_TX_I2MPB_D_GBE_MASK,
-				  buf[3] + bias[12]));
-	phy_modify_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_TX_I2MPB_TEST_MODE_D1,
-		       MTK_PHY_DA_TX_I2MPB_D_TBT_MASK,
-		       FIELD_PREP(MTK_PHY_DA_TX_I2MPB_D_TBT_MASK,
-				  buf[3] + bias[13]));
-	phy_modify_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_TX_I2MPB_TEST_MODE_D2,
-		       MTK_PHY_DA_TX_I2MPB_D_HBT_MASK,
-		       FIELD_PREP(MTK_PHY_DA_TX_I2MPB_D_HBT_MASK,
-				  buf[3] + bias[14]));
-	phy_modify_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_TX_I2MPB_TEST_MODE_D2,
-		       MTK_PHY_DA_TX_I2MPB_D_TST_MASK,
-		       FIELD_PREP(MTK_PHY_DA_TX_I2MPB_D_TST_MASK,
-				  buf[3] + bias[15]));
-
-	return 0;
-}
-
-static int tx_amp_cal_efuse(struct phy_device *phydev, u32 *buf)
-{
-	u16 tx_amp_cal_val[4];
-
-	tx_amp_cal_val[0] = EFS_DA_TX_I2MPB_A(buf[0]);
-	tx_amp_cal_val[1] = EFS_DA_TX_I2MPB_B(buf[0]);
-	tx_amp_cal_val[2] = EFS_DA_TX_I2MPB_C(buf[0]);
-	tx_amp_cal_val[3] = EFS_DA_TX_I2MPB_D(buf[0]);
-	tx_amp_fill_result(phydev, tx_amp_cal_val);
-
-	return 0;
-}
-
-static int tx_r50_fill_result(struct phy_device *phydev, u16 tx_r50_cal_val,
-			      u8 txg_calen_x)
-{
-	int bias = 0;
-	u16 reg, val;
-
-	if (phydev->drv->phy_id == MTK_GPHY_ID_MT7988)
-		bias = -1;
-
-	val = clamp_val(bias + tx_r50_cal_val, 0, 63);
-
-	switch (txg_calen_x) {
-	case PAIR_A:
-		reg = MTK_PHY_DA_TX_R50_PAIR_A;
-		break;
-	case PAIR_B:
-		reg = MTK_PHY_DA_TX_R50_PAIR_B;
-		break;
-	case PAIR_C:
-		reg = MTK_PHY_DA_TX_R50_PAIR_C;
-		break;
-	case PAIR_D:
-		reg = MTK_PHY_DA_TX_R50_PAIR_D;
-		break;
-	default:
-		return -EINVAL;
-	}
-
-	phy_write_mmd(phydev, MDIO_MMD_VEND1, reg, val | val << 8);
-
-	return 0;
-}
-
-static int tx_r50_cal_efuse(struct phy_device *phydev, u32 *buf,
-			    u8 txg_calen_x)
-{
-	u16 tx_r50_cal_val;
-
-	switch (txg_calen_x) {
-	case PAIR_A:
-		tx_r50_cal_val = EFS_DA_TX_R50_A(buf[1]);
-		break;
-	case PAIR_B:
-		tx_r50_cal_val = EFS_DA_TX_R50_B(buf[1]);
-		break;
-	case PAIR_C:
-		tx_r50_cal_val = EFS_DA_TX_R50_C(buf[2]);
-		break;
-	case PAIR_D:
-		tx_r50_cal_val = EFS_DA_TX_R50_D(buf[2]);
-		break;
-	default:
-		return -EINVAL;
-	}
-	tx_r50_fill_result(phydev, tx_r50_cal_val, txg_calen_x);
-
-	return 0;
-}
-
-static int tx_vcm_cal_sw(struct phy_device *phydev, u8 rg_txreserve_x)
-{
-	u8 lower_idx, upper_idx, txreserve_val;
-	u8 lower_ret, upper_ret;
-	int ret;
-
-	phy_set_bits_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_RG_ANA_CAL_RG0,
-			 MTK_PHY_RG_ANA_CALEN);
-	phy_clear_bits_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_RG_ANA_CAL_RG0,
-			   MTK_PHY_RG_CAL_CKINV);
-	phy_set_bits_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_RG_ANA_CAL_RG1,
-			 MTK_PHY_RG_TXVOS_CALEN);
-
-	switch (rg_txreserve_x) {
-	case PAIR_A:
-		phy_clear_bits_mmd(phydev, MDIO_MMD_VEND1,
-				   MTK_PHY_RG_DASN_DAC_IN0_A,
-				   MTK_PHY_DASN_DAC_IN0_A_MASK);
-		phy_clear_bits_mmd(phydev, MDIO_MMD_VEND1,
-				   MTK_PHY_RG_DASN_DAC_IN1_A,
-				   MTK_PHY_DASN_DAC_IN1_A_MASK);
-		phy_set_bits_mmd(phydev, MDIO_MMD_VEND1,
-				 MTK_PHY_RG_ANA_CAL_RG0,
-				 MTK_PHY_RG_ZCALEN_A);
-		break;
-	case PAIR_B:
-		phy_clear_bits_mmd(phydev, MDIO_MMD_VEND1,
-				   MTK_PHY_RG_DASN_DAC_IN0_B,
-				   MTK_PHY_DASN_DAC_IN0_B_MASK);
-		phy_clear_bits_mmd(phydev, MDIO_MMD_VEND1,
-				   MTK_PHY_RG_DASN_DAC_IN1_B,
-				   MTK_PHY_DASN_DAC_IN1_B_MASK);
-		phy_set_bits_mmd(phydev, MDIO_MMD_VEND1,
-				 MTK_PHY_RG_ANA_CAL_RG1,
-				 MTK_PHY_RG_ZCALEN_B);
-		break;
-	case PAIR_C:
-		phy_clear_bits_mmd(phydev, MDIO_MMD_VEND1,
-				   MTK_PHY_RG_DASN_DAC_IN0_C,
-				   MTK_PHY_DASN_DAC_IN0_C_MASK);
-		phy_clear_bits_mmd(phydev, MDIO_MMD_VEND1,
-				   MTK_PHY_RG_DASN_DAC_IN1_C,
-				   MTK_PHY_DASN_DAC_IN1_C_MASK);
-		phy_set_bits_mmd(phydev, MDIO_MMD_VEND1,
-				 MTK_PHY_RG_ANA_CAL_RG1,
-				 MTK_PHY_RG_ZCALEN_C);
-		break;
-	case PAIR_D:
-		phy_clear_bits_mmd(phydev, MDIO_MMD_VEND1,
-				   MTK_PHY_RG_DASN_DAC_IN0_D,
-				   MTK_PHY_DASN_DAC_IN0_D_MASK);
-		phy_clear_bits_mmd(phydev, MDIO_MMD_VEND1,
-				   MTK_PHY_RG_DASN_DAC_IN1_D,
-				   MTK_PHY_DASN_DAC_IN1_D_MASK);
-		phy_set_bits_mmd(phydev, MDIO_MMD_VEND1,
-				 MTK_PHY_RG_ANA_CAL_RG1,
-				 MTK_PHY_RG_ZCALEN_D);
-		break;
-	default:
-		ret = -EINVAL;
-		goto restore;
-	}
-
-	lower_idx = TXRESERVE_MIN;
-	upper_idx = TXRESERVE_MAX;
-
-	phydev_dbg(phydev, "Start TX-VCM SW cal.\n");
-	while ((upper_idx - lower_idx) > 1) {
-		txreserve_val = DIV_ROUND_CLOSEST(lower_idx + upper_idx, 2);
-		ret = cal_cycle(phydev, MDIO_MMD_VEND1, MTK_PHY_RXADC_CTRL_RG9,
-				MTK_PHY_DA_RX_PSBN_TBT_MASK |
-				MTK_PHY_DA_RX_PSBN_HBT_MASK |
-				MTK_PHY_DA_RX_PSBN_GBE_MASK |
-				MTK_PHY_DA_RX_PSBN_LP_MASK,
-				txreserve_val << 12 | txreserve_val << 8 |
-				txreserve_val << 4 | txreserve_val);
-		if (ret == 1) {
-			upper_idx = txreserve_val;
-			upper_ret = ret;
-		} else if (ret == 0) {
-			lower_idx = txreserve_val;
-			lower_ret = ret;
-		} else {
-			goto restore;
-		}
-	}
-
-	if (lower_idx == TXRESERVE_MIN) {
-		lower_ret = cal_cycle(phydev, MDIO_MMD_VEND1,
-				      MTK_PHY_RXADC_CTRL_RG9,
-				      MTK_PHY_DA_RX_PSBN_TBT_MASK |
-				      MTK_PHY_DA_RX_PSBN_HBT_MASK |
-				      MTK_PHY_DA_RX_PSBN_GBE_MASK |
-				      MTK_PHY_DA_RX_PSBN_LP_MASK,
-				      lower_idx << 12 | lower_idx << 8 |
-				      lower_idx << 4 | lower_idx);
-		ret = lower_ret;
-	} else if (upper_idx == TXRESERVE_MAX) {
-		upper_ret = cal_cycle(phydev, MDIO_MMD_VEND1,
-				      MTK_PHY_RXADC_CTRL_RG9,
-				      MTK_PHY_DA_RX_PSBN_TBT_MASK |
-				      MTK_PHY_DA_RX_PSBN_HBT_MASK |
-				      MTK_PHY_DA_RX_PSBN_GBE_MASK |
-				      MTK_PHY_DA_RX_PSBN_LP_MASK,
-				      upper_idx << 12 | upper_idx << 8 |
-				      upper_idx << 4 | upper_idx);
-		ret = upper_ret;
-	}
-	if (ret < 0)
-		goto restore;
-
-	/* We calibrate TX-VCM in different logic. Check upper index and then
-	 * lower index. If this calibration is valid, apply lower index's
-	 * result.
-	 */
-	ret = upper_ret - lower_ret;
-	if (ret == 1) {
-		ret = 0;
-		/* Make sure we use upper_idx in our calibration system */
-		cal_cycle(phydev, MDIO_MMD_VEND1, MTK_PHY_RXADC_CTRL_RG9,
-			  MTK_PHY_DA_RX_PSBN_TBT_MASK |
-			  MTK_PHY_DA_RX_PSBN_HBT_MASK |
-			  MTK_PHY_DA_RX_PSBN_GBE_MASK |
-			  MTK_PHY_DA_RX_PSBN_LP_MASK,
-			  upper_idx << 12 | upper_idx << 8 |
-			  upper_idx << 4 | upper_idx);
-		phydev_dbg(phydev, "TX-VCM SW cal result: 0x%x\n", upper_idx);
-	} else if (lower_idx == TXRESERVE_MIN && upper_ret == 1 &&
-		   lower_ret == 1) {
-		ret = 0;
-		cal_cycle(phydev, MDIO_MMD_VEND1, MTK_PHY_RXADC_CTRL_RG9,
-			  MTK_PHY_DA_RX_PSBN_TBT_MASK |
-			  MTK_PHY_DA_RX_PSBN_HBT_MASK |
-			  MTK_PHY_DA_RX_PSBN_GBE_MASK |
-			  MTK_PHY_DA_RX_PSBN_LP_MASK,
-			  lower_idx << 12 | lower_idx << 8 |
-			  lower_idx << 4 | lower_idx);
-		phydev_warn(phydev, "TX-VCM SW cal result at low margin 0x%x\n",
-			    lower_idx);
-	} else if (upper_idx == TXRESERVE_MAX && upper_ret == 0 &&
-		   lower_ret == 0) {
-		ret = 0;
-		phydev_warn(phydev,
-			    "TX-VCM SW cal result at high margin 0x%x\n",
-			    upper_idx);
-	} else {
-		ret = -EINVAL;
-	}
-
-restore:
-	phy_clear_bits_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_RG_ANA_CAL_RG0,
-			   MTK_PHY_RG_ANA_CALEN);
-	phy_clear_bits_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_RG_ANA_CAL_RG1,
-			   MTK_PHY_RG_TXVOS_CALEN);
-	phy_clear_bits_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_RG_ANA_CAL_RG0,
-			   MTK_PHY_RG_ZCALEN_A);
-	phy_clear_bits_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_RG_ANA_CAL_RG1,
-			   MTK_PHY_RG_ZCALEN_B | MTK_PHY_RG_ZCALEN_C |
-			   MTK_PHY_RG_ZCALEN_D);
-
-	return ret;
-}
-
-static void mt798x_phy_common_finetune(struct phy_device *phydev)
-{
-	phy_select_page(phydev, MTK_PHY_PAGE_EXTENDED_52B5);
-	/* SlvDSPreadyTime = 24, MasDSPreadyTime = 24 */
-	__phy_write(phydev, 0x11, 0xc71);
-	__phy_write(phydev, 0x12, 0xc);
-	__phy_write(phydev, 0x10, 0x8fae);
-
-	/* EnabRandUpdTrig = 1 */
-	__phy_write(phydev, 0x11, 0x2f00);
-	__phy_write(phydev, 0x12, 0xe);
-	__phy_write(phydev, 0x10, 0x8fb0);
-
-	/* NormMseLoThresh = 85 */
-	__phy_write(phydev, 0x11, 0x55a0);
-	__phy_write(phydev, 0x12, 0x0);
-	__phy_write(phydev, 0x10, 0x83aa);
-
-	/* FfeUpdGainForce = 1(Enable), FfeUpdGainForceVal = 4 */
-	__phy_write(phydev, 0x11, 0x240);
-	__phy_write(phydev, 0x12, 0x0);
-	__phy_write(phydev, 0x10, 0x9680);
-
-	/* TrFreeze = 0 (mt7988 default) */
-	__phy_write(phydev, 0x11, 0x0);
-	__phy_write(phydev, 0x12, 0x0);
-	__phy_write(phydev, 0x10, 0x9686);
-
-	/* SSTrKp100 = 5 */
-	/* SSTrKf100 = 6 */
-	/* SSTrKp1000Mas = 5 */
-	/* SSTrKf1000Mas = 6 */
-	/* SSTrKp1000Slv = 5 */
-	/* SSTrKf1000Slv = 6 */
-	__phy_write(phydev, 0x11, 0xbaef);
-	__phy_write(phydev, 0x12, 0x2e);
-	__phy_write(phydev, 0x10, 0x968c);
-	phy_restore_page(phydev, MTK_PHY_PAGE_STANDARD, 0);
-}
-
-static void mt7981_phy_finetune(struct phy_device *phydev)
-{
-	u16 val[8] = { 0x01ce, 0x01c1,
-		       0x020f, 0x0202,
-		       0x03d0, 0x03c0,
-		       0x0013, 0x0005 };
-	int i, k;
-
-	/* 100M eye finetune:
-	 * Keep middle level of TX MLT3 shapper as default.
-	 * Only change TX MLT3 overshoot level here.
-	 */
-	for (k = 0, i = 1; i < 12; i++) {
-		if (i % 3 == 0)
-			continue;
-		phy_write_mmd(phydev, MDIO_MMD_VEND1, i, val[k++]);
-	}
-
-	phy_select_page(phydev, MTK_PHY_PAGE_EXTENDED_52B5);
-	/* ResetSyncOffset = 6 */
-	__phy_write(phydev, 0x11, 0x600);
-	__phy_write(phydev, 0x12, 0x0);
-	__phy_write(phydev, 0x10, 0x8fc0);
-
-	/* VgaDecRate = 1 */
-	__phy_write(phydev, 0x11, 0x4c2a);
-	__phy_write(phydev, 0x12, 0x3e);
-	__phy_write(phydev, 0x10, 0x8fa4);
-
-	/* MrvlTrFix100Kp = 3, MrvlTrFix100Kf = 2,
-	 * MrvlTrFix1000Kp = 3, MrvlTrFix1000Kf = 2
-	 */
-	__phy_write(phydev, 0x11, 0xd10a);
-	__phy_write(phydev, 0x12, 0x34);
-	__phy_write(phydev, 0x10, 0x8f82);
-
-	/* VcoSlicerThreshBitsHigh */
-	__phy_write(phydev, 0x11, 0x5555);
-	__phy_write(phydev, 0x12, 0x55);
-	__phy_write(phydev, 0x10, 0x8ec0);
-	phy_restore_page(phydev, MTK_PHY_PAGE_STANDARD, 0);
-
-	/* TR_OPEN_LOOP_EN = 1, lpf_x_average = 9 */
-	phy_modify_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_RG_DEV1E_REG234,
-		       MTK_PHY_TR_OPEN_LOOP_EN_MASK |
-		       MTK_PHY_LPF_X_AVERAGE_MASK,
-		       BIT(0) | FIELD_PREP(MTK_PHY_LPF_X_AVERAGE_MASK, 0x9));
-
-	/* rg_tr_lpf_cnt_val = 512 */
-	phy_write_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_RG_LPF_CNT_VAL, 0x200);
-
-	/* IIR2 related */
-	phy_write_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_RG_LP_IIR2_K1_L, 0x82);
-	phy_write_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_RG_LP_IIR2_K1_U, 0x0);
-	phy_write_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_RG_LP_IIR2_K2_L, 0x103);
-	phy_write_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_RG_LP_IIR2_K2_U, 0x0);
-	phy_write_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_RG_LP_IIR2_K3_L, 0x82);
-	phy_write_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_RG_LP_IIR2_K3_U, 0x0);
-	phy_write_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_RG_LP_IIR2_K4_L, 0xd177);
-	phy_write_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_RG_LP_IIR2_K4_U, 0x3);
-	phy_write_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_RG_LP_IIR2_K5_L, 0x2c82);
-	phy_write_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_RG_LP_IIR2_K5_U, 0xe);
-
-	/* FFE peaking */
-	phy_modify_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_RG_DEV1E_REG27C,
-		       MTK_PHY_VGASTATE_FFE_THR_ST1_MASK, 0x1b << 8);
-	phy_modify_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_RG_DEV1E_REG27D,
-		       MTK_PHY_VGASTATE_FFE_THR_ST2_MASK, 0x1e);
-
-	/* Disable LDO pump */
-	phy_write_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_LDO_PUMP_EN_PAIRAB, 0x0);
-	phy_write_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_LDO_PUMP_EN_PAIRCD, 0x0);
-	/* Adjust LDO output voltage */
-	phy_write_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_LDO_OUTPUT_V, 0x2222);
-}
-
-static void mt7988_phy_finetune(struct phy_device *phydev)
-{
-	u16 val[12] = { 0x0187, 0x01cd, 0x01c8, 0x0182,
-			0x020d, 0x0206, 0x0384, 0x03d0,
-			0x03c6, 0x030a, 0x0011, 0x0005 };
-	int i;
-
-	/* Set default MLT3 shaper first */
-	for (i = 0; i < 12; i++)
-		phy_write_mmd(phydev, MDIO_MMD_VEND1, i, val[i]);
-
-	/* TCT finetune */
-	phy_write_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_RG_TX_FILTER, 0x5);
-
-	phy_select_page(phydev, MTK_PHY_PAGE_EXTENDED_52B5);
-	/* ResetSyncOffset = 5 */
-	__phy_write(phydev, 0x11, 0x500);
-	__phy_write(phydev, 0x12, 0x0);
-	__phy_write(phydev, 0x10, 0x8fc0);
-
-	/* VgaDecRate is 1 at default on mt7988 */
-
-	/* MrvlTrFix100Kp = 6, MrvlTrFix100Kf = 7,
-	 * MrvlTrFix1000Kp = 6, MrvlTrFix1000Kf = 7
-	 */
-	__phy_write(phydev, 0x11, 0xb90a);
-	__phy_write(phydev, 0x12, 0x6f);
-	__phy_write(phydev, 0x10, 0x8f82);
-
-	/* RemAckCntLimitCtrl = 1 */
-	__phy_write(phydev, 0x11, 0xfbba);
-	__phy_write(phydev, 0x12, 0xc3);
-	__phy_write(phydev, 0x10, 0x87f8);
-
-	phy_restore_page(phydev, MTK_PHY_PAGE_STANDARD, 0);
-
-	/* TR_OPEN_LOOP_EN = 1, lpf_x_average = 10 */
-	phy_modify_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_RG_DEV1E_REG234,
-		       MTK_PHY_TR_OPEN_LOOP_EN_MASK |
-		       MTK_PHY_LPF_X_AVERAGE_MASK,
-		       BIT(0) | FIELD_PREP(MTK_PHY_LPF_X_AVERAGE_MASK, 0xa));
-
-	/* rg_tr_lpf_cnt_val = 1023 */
-	phy_write_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_RG_LPF_CNT_VAL, 0x3ff);
-}
-
-static void mt798x_phy_eee(struct phy_device *phydev)
-{
-	phy_modify_mmd(phydev, MDIO_MMD_VEND1,
-		       MTK_PHY_RG_LPI_PCS_DSP_CTRL_REG120,
-		       MTK_PHY_LPI_SIG_EN_LO_THRESH1000_MASK |
-		       MTK_PHY_LPI_SIG_EN_HI_THRESH1000_MASK,
-		       FIELD_PREP(MTK_PHY_LPI_SIG_EN_LO_THRESH1000_MASK, 0x0) |
-		       FIELD_PREP(MTK_PHY_LPI_SIG_EN_HI_THRESH1000_MASK, 0x14));
-
-	phy_modify_mmd(phydev, MDIO_MMD_VEND1,
-		       MTK_PHY_RG_LPI_PCS_DSP_CTRL_REG122,
-		       MTK_PHY_LPI_NORM_MSE_HI_THRESH1000_MASK,
-		       FIELD_PREP(MTK_PHY_LPI_NORM_MSE_HI_THRESH1000_MASK,
-				  0xff));
-
-	phy_clear_bits_mmd(phydev, MDIO_MMD_VEND1,
-			   MTK_PHY_RG_TESTMUX_ADC_CTRL,
-			   MTK_PHY_RG_TXEN_DIG_MASK);
-
-	phy_set_bits_mmd(phydev, MDIO_MMD_VEND1,
-			 MTK_PHY_RG_DEV1E_REG19b, MTK_PHY_BYPASS_DSP_LPI_READY);
-
-	phy_clear_bits_mmd(phydev, MDIO_MMD_VEND1,
-			   MTK_PHY_RG_DEV1E_REG234, MTK_PHY_TR_LP_IIR_EEE_EN);
-
-	phy_modify_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_RG_DEV1E_REG238,
-		       MTK_PHY_LPI_SLV_SEND_TX_TIMER_MASK |
-		       MTK_PHY_LPI_SLV_SEND_TX_EN,
-		       FIELD_PREP(MTK_PHY_LPI_SLV_SEND_TX_TIMER_MASK, 0x120));
-
-	/* Keep MTK_PHY_LPI_SEND_LOC_TIMER as 375 */
-	phy_clear_bits_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_RG_DEV1E_REG239,
-			   MTK_PHY_LPI_TXPCS_LOC_RCV);
-
-	/* This also fixes some IoT issues, such as CH340 */
-	phy_modify_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_RG_DEV1E_REG2C7,
-		       MTK_PHY_MAX_GAIN_MASK | MTK_PHY_MIN_GAIN_MASK,
-		       FIELD_PREP(MTK_PHY_MAX_GAIN_MASK, 0x8) |
-		       FIELD_PREP(MTK_PHY_MIN_GAIN_MASK, 0x13));
-
-	phy_modify_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_RG_DEV1E_REG2D1,
-		       MTK_PHY_VCO_SLICER_THRESH_BITS_HIGH_EEE_MASK,
-		       FIELD_PREP(MTK_PHY_VCO_SLICER_THRESH_BITS_HIGH_EEE_MASK,
-				  0x33) |
-		       MTK_PHY_LPI_SKIP_SD_SLV_TR | MTK_PHY_LPI_TR_READY |
-		       MTK_PHY_LPI_VCO_EEE_STG0_EN);
-
-	phy_set_bits_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_RG_DEV1E_REG323,
-			 MTK_PHY_EEE_WAKE_MAS_INT_DC |
-			 MTK_PHY_EEE_WAKE_SLV_INT_DC);
-
-	phy_modify_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_RG_DEV1E_REG324,
-		       MTK_PHY_SMI_DETCNT_MAX_MASK,
-		       FIELD_PREP(MTK_PHY_SMI_DETCNT_MAX_MASK, 0x3f) |
-		       MTK_PHY_SMI_DET_MAX_EN);
-
-	phy_set_bits_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_RG_DEV1E_REG326,
-			 MTK_PHY_LPI_MODE_SD_ON | MTK_PHY_RESET_RANDUPD_CNT |
-			 MTK_PHY_TREC_UPDATE_ENAB_CLR |
-			 MTK_PHY_LPI_QUIT_WAIT_DFE_SIG_DET_OFF |
-			 MTK_PHY_TR_READY_SKIP_AFE_WAKEUP);
-
-	phy_select_page(phydev, MTK_PHY_PAGE_EXTENDED_52B5);
-	/* Regsigdet_sel_1000 = 0 */
-	__phy_write(phydev, 0x11, 0xb);
-	__phy_write(phydev, 0x12, 0x0);
-	__phy_write(phydev, 0x10, 0x9690);
-
-	/* REG_EEE_st2TrKf1000 = 2 */
-	__phy_write(phydev, 0x11, 0x114f);
-	__phy_write(phydev, 0x12, 0x2);
-	__phy_write(phydev, 0x10, 0x969a);
-
-	/* RegEEE_slv_wake_tr_timer_tar = 6, RegEEE_slv_remtx_timer_tar = 20 */
-	__phy_write(phydev, 0x11, 0x3028);
-	__phy_write(phydev, 0x12, 0x0);
-	__phy_write(phydev, 0x10, 0x969e);
-
-	/* RegEEE_slv_wake_int_timer_tar = 8 */
-	__phy_write(phydev, 0x11, 0x5010);
-	__phy_write(phydev, 0x12, 0x0);
-	__phy_write(phydev, 0x10, 0x96a0);
-
-	/* RegEEE_trfreeze_timer2 = 586 */
-	__phy_write(phydev, 0x11, 0x24a);
-	__phy_write(phydev, 0x12, 0x0);
-	__phy_write(phydev, 0x10, 0x96a8);
-
-	/* RegEEE100Stg1_tar = 16 */
-	__phy_write(phydev, 0x11, 0x3210);
-	__phy_write(phydev, 0x12, 0x0);
-	__phy_write(phydev, 0x10, 0x96b8);
-
-	/* REGEEE_wake_slv_tr_wait_dfesigdet_en = 0 */
-	__phy_write(phydev, 0x11, 0x1463);
-	__phy_write(phydev, 0x12, 0x0);
-	__phy_write(phydev, 0x10, 0x96ca);
-
-	/* DfeTailEnableVgaThresh1000 = 27 */
-	__phy_write(phydev, 0x11, 0x36);
-	__phy_write(phydev, 0x12, 0x0);
-	__phy_write(phydev, 0x10, 0x8f80);
-	phy_restore_page(phydev, MTK_PHY_PAGE_STANDARD, 0);
-
-	phy_select_page(phydev, MTK_PHY_PAGE_EXTENDED_3);
-	__phy_modify(phydev, MTK_PHY_LPI_REG_14,
-		     MTK_PHY_LPI_WAKE_TIMER_1000_MASK,
-		     FIELD_PREP(MTK_PHY_LPI_WAKE_TIMER_1000_MASK, 0x19c));
-
-	__phy_modify(phydev, MTK_PHY_LPI_REG_1c, MTK_PHY_SMI_DET_ON_THRESH_MASK,
-		     FIELD_PREP(MTK_PHY_SMI_DET_ON_THRESH_MASK, 0xc));
-	phy_restore_page(phydev, MTK_PHY_PAGE_STANDARD, 0);
-
-	phy_modify_mmd(phydev, MDIO_MMD_VEND1,
-		       MTK_PHY_RG_LPI_PCS_DSP_CTRL_REG122,
-		       MTK_PHY_LPI_NORM_MSE_HI_THRESH1000_MASK,
-		       FIELD_PREP(MTK_PHY_LPI_NORM_MSE_HI_THRESH1000_MASK,
-				  0xff));
-}
-
-static int cal_sw(struct phy_device *phydev, enum CAL_ITEM cal_item,
-		  u8 start_pair, u8 end_pair)
-{
-	u8 pair_n;
-	int ret;
-
-	for (pair_n = start_pair; pair_n <= end_pair; pair_n++) {
-		/* TX_OFFSET & TX_AMP have no SW calibration. */
-		switch (cal_item) {
-		case TX_VCM:
-			ret = tx_vcm_cal_sw(phydev, pair_n);
-			break;
-		default:
-			return -EINVAL;
-		}
-		if (ret)
-			return ret;
-	}
-	return 0;
-}
-
-static int cal_efuse(struct phy_device *phydev, enum CAL_ITEM cal_item,
-		     u8 start_pair, u8 end_pair, u32 *buf)
-{
-	u8 pair_n;
-	int ret;
-
-	for (pair_n = start_pair; pair_n <= end_pair; pair_n++) {
-		/* TX_VCM has no efuse calibration. */
-		switch (cal_item) {
-		case REXT:
-			ret = rext_cal_efuse(phydev, buf);
-			break;
-		case TX_OFFSET:
-			ret = tx_offset_cal_efuse(phydev, buf);
-			break;
-		case TX_AMP:
-			ret = tx_amp_cal_efuse(phydev, buf);
-			break;
-		case TX_R50:
-			ret = tx_r50_cal_efuse(phydev, buf, pair_n);
-			break;
-		default:
-			return -EINVAL;
-		}
-		if (ret)
-			return ret;
-	}
-
-	return 0;
-}
-
-static int start_cal(struct phy_device *phydev, enum CAL_ITEM cal_item,
-		     enum CAL_MODE cal_mode, u8 start_pair,
-		     u8 end_pair, u32 *buf)
-{
-	int ret;
-
-	switch (cal_mode) {
-	case EFUSE_M:
-		ret = cal_efuse(phydev, cal_item, start_pair,
-				end_pair, buf);
-		break;
-	case SW_M:
-		ret = cal_sw(phydev, cal_item, start_pair, end_pair);
-		break;
-	default:
-		return -EINVAL;
-	}
-
-	if (ret) {
-		phydev_err(phydev, "cal %d failed\n", cal_item);
-		return -EIO;
-	}
-
-	return 0;
-}
-
-static int mt798x_phy_calibration(struct phy_device *phydev)
-{
-	struct nvmem_cell *cell;
-	int ret = 0;
-	size_t len;
-	u32 *buf;
-
-	cell = nvmem_cell_get(&phydev->mdio.dev, "phy-cal-data");
-	if (IS_ERR(cell)) {
-		if (PTR_ERR(cell) == -EPROBE_DEFER)
-			return PTR_ERR(cell);
-		return 0;
-	}
-
-	buf = (u32 *)nvmem_cell_read(cell, &len);
-	if (IS_ERR(buf))
-		return PTR_ERR(buf);
-	nvmem_cell_put(cell);
-
-	if (!buf[0] || !buf[1] || !buf[2] || !buf[3] || len < 4 * sizeof(u32)) {
-		phydev_err(phydev, "invalid efuse data\n");
-		ret = -EINVAL;
-		goto out;
-	}
-
-	ret = start_cal(phydev, REXT, EFUSE_M, NO_PAIR, NO_PAIR, buf);
-	if (ret)
-		goto out;
-	ret = start_cal(phydev, TX_OFFSET, EFUSE_M, NO_PAIR, NO_PAIR, buf);
-	if (ret)
-		goto out;
-	ret = start_cal(phydev, TX_AMP, EFUSE_M, NO_PAIR, NO_PAIR, buf);
-	if (ret)
-		goto out;
-	ret = start_cal(phydev, TX_R50, EFUSE_M, PAIR_A, PAIR_D, buf);
-	if (ret)
-		goto out;
-	ret = start_cal(phydev, TX_VCM, SW_M, PAIR_A, PAIR_A, buf);
-	if (ret)
-		goto out;
-
-out:
-	kfree(buf);
-	return ret;
-}
-
-static int mt798x_phy_config_init(struct phy_device *phydev)
-{
-	switch (phydev->drv->phy_id) {
-	case MTK_GPHY_ID_MT7981:
-		mt7981_phy_finetune(phydev);
-		break;
-	case MTK_GPHY_ID_MT7988:
-		mt7988_phy_finetune(phydev);
-		break;
-	}
-
-	mt798x_phy_common_finetune(phydev);
-	mt798x_phy_eee(phydev);
-
-	return mt798x_phy_calibration(phydev);
-}
-
-static int mt798x_phy_hw_led_on_set(struct phy_device *phydev, u8 index,
-				    bool on)
-{
-	unsigned int bit_on = MTK_PHY_LED_STATE_FORCE_ON + (index ? 16 : 0);
-	struct mtk_socphy_priv *priv = phydev->priv;
-	bool changed;
-
-	if (on)
-		changed = !test_and_set_bit(bit_on, &priv->led_state);
-	else
-		changed = !!test_and_clear_bit(bit_on, &priv->led_state);
-
-	changed |= !!test_and_clear_bit(MTK_PHY_LED_STATE_NETDEV +
-					(index ? 16 : 0), &priv->led_state);
-	if (changed)
-		return phy_modify_mmd(phydev, MDIO_MMD_VEND2, index ?
-				      MTK_PHY_LED1_ON_CTRL :
-				      MTK_PHY_LED0_ON_CTRL,
-				      MTK_PHY_LED_ON_MASK,
-				      on ? MTK_PHY_LED_ON_FORCE_ON : 0);
-	else
-		return 0;
-}
-
-static int mt798x_phy_hw_led_blink_set(struct phy_device *phydev, u8 index,
-				       bool blinking)
-{
-	unsigned int bit_blink = MTK_PHY_LED_STATE_FORCE_BLINK +
-				 (index ? 16 : 0);
-	struct mtk_socphy_priv *priv = phydev->priv;
-	bool changed;
-
-	if (blinking)
-		changed = !test_and_set_bit(bit_blink, &priv->led_state);
-	else
-		changed = !!test_and_clear_bit(bit_blink, &priv->led_state);
-
-	changed |= !!test_bit(MTK_PHY_LED_STATE_NETDEV +
-			      (index ? 16 : 0), &priv->led_state);
-	if (changed)
-		return phy_write_mmd(phydev, MDIO_MMD_VEND2, index ?
-				     MTK_PHY_LED1_BLINK_CTRL :
-				     MTK_PHY_LED0_BLINK_CTRL,
-				     blinking ?
-				     MTK_PHY_LED_BLINK_FORCE_BLINK : 0);
-	else
-		return 0;
-}
-
-static int mt798x_phy_led_blink_set(struct phy_device *phydev, u8 index,
-				    unsigned long *delay_on,
-				    unsigned long *delay_off)
-{
-	bool blinking = false;
-	int err = 0;
-
-	if (index > 1)
-		return -EINVAL;
-
-	if (delay_on && delay_off && (*delay_on > 0) && (*delay_off > 0)) {
-		blinking = true;
-		*delay_on = 50;
-		*delay_off = 50;
-	}
-
-	err = mt798x_phy_hw_led_blink_set(phydev, index, blinking);
-	if (err)
-		return err;
-
-	return mt798x_phy_hw_led_on_set(phydev, index, false);
-}
-
-static int mt798x_phy_led_brightness_set(struct phy_device *phydev,
-					 u8 index, enum led_brightness value)
-{
-	int err;
-
-	err = mt798x_phy_hw_led_blink_set(phydev, index, false);
-	if (err)
-		return err;
-
-	return mt798x_phy_hw_led_on_set(phydev, index, (value != LED_OFF));
-}
-
-static const unsigned long supported_triggers =
-	BIT(TRIGGER_NETDEV_FULL_DUPLEX) |
-	BIT(TRIGGER_NETDEV_HALF_DUPLEX) |
-	BIT(TRIGGER_NETDEV_LINK)        |
-	BIT(TRIGGER_NETDEV_LINK_10)     |
-	BIT(TRIGGER_NETDEV_LINK_100)    |
-	BIT(TRIGGER_NETDEV_LINK_1000)   |
-	BIT(TRIGGER_NETDEV_RX)          |
-	BIT(TRIGGER_NETDEV_TX);
-
-static int mt798x_phy_led_hw_is_supported(struct phy_device *phydev, u8 index,
-					  unsigned long rules)
-{
-	if (index > 1)
-		return -EINVAL;
-
-	/* All combinations of the supported triggers are allowed */
-	if (rules & ~supported_triggers)
-		return -EOPNOTSUPP;
-
-	return 0;
-};
-
-static int mt798x_phy_led_hw_control_get(struct phy_device *phydev, u8 index,
-					 unsigned long *rules)
-{
-	unsigned int bit_blink = MTK_PHY_LED_STATE_FORCE_BLINK +
-				 (index ? 16 : 0);
-	unsigned int bit_netdev = MTK_PHY_LED_STATE_NETDEV + (index ? 16 : 0);
-	unsigned int bit_on = MTK_PHY_LED_STATE_FORCE_ON + (index ? 16 : 0);
-	struct mtk_socphy_priv *priv = phydev->priv;
-	int on, blink;
-
-	if (index > 1)
-		return -EINVAL;
-
-	on = phy_read_mmd(phydev, MDIO_MMD_VEND2,
-			  index ? MTK_PHY_LED1_ON_CTRL : MTK_PHY_LED0_ON_CTRL);
-
-	if (on < 0)
-		return -EIO;
-
-	blink = phy_read_mmd(phydev, MDIO_MMD_VEND2,
-			     index ? MTK_PHY_LED1_BLINK_CTRL :
-				     MTK_PHY_LED0_BLINK_CTRL);
-	if (blink < 0)
-		return -EIO;
-
-	if ((on & (MTK_PHY_LED_ON_LINK | MTK_PHY_LED_ON_FDX |
-		   MTK_PHY_LED_ON_HDX | MTK_PHY_LED_ON_LINKDOWN)) ||
-	    (blink & (MTK_PHY_LED_BLINK_RX | MTK_PHY_LED_BLINK_TX)))
-		set_bit(bit_netdev, &priv->led_state);
-	else
-		clear_bit(bit_netdev, &priv->led_state);
-
-	if (on & MTK_PHY_LED_ON_FORCE_ON)
-		set_bit(bit_on, &priv->led_state);
-	else
-		clear_bit(bit_on, &priv->led_state);
-
-	if (blink & MTK_PHY_LED_BLINK_FORCE_BLINK)
-		set_bit(bit_blink, &priv->led_state);
-	else
-		clear_bit(bit_blink, &priv->led_state);
-
-	if (!rules)
-		return 0;
-
-	if (on & MTK_PHY_LED_ON_LINK)
-		*rules |= BIT(TRIGGER_NETDEV_LINK);
-
-	if (on & MTK_PHY_LED_ON_LINK10)
-		*rules |= BIT(TRIGGER_NETDEV_LINK_10);
-
-	if (on & MTK_PHY_LED_ON_LINK100)
-		*rules |= BIT(TRIGGER_NETDEV_LINK_100);
-
-	if (on & MTK_PHY_LED_ON_LINK1000)
-		*rules |= BIT(TRIGGER_NETDEV_LINK_1000);
-
-	if (on & MTK_PHY_LED_ON_FDX)
-		*rules |= BIT(TRIGGER_NETDEV_FULL_DUPLEX);
-
-	if (on & MTK_PHY_LED_ON_HDX)
-		*rules |= BIT(TRIGGER_NETDEV_HALF_DUPLEX);
-
-	if (blink & MTK_PHY_LED_BLINK_RX)
-		*rules |= BIT(TRIGGER_NETDEV_RX);
-
-	if (blink & MTK_PHY_LED_BLINK_TX)
-		*rules |= BIT(TRIGGER_NETDEV_TX);
-
-	return 0;
-};
-
-static int mt798x_phy_led_hw_control_set(struct phy_device *phydev, u8 index,
-					 unsigned long rules)
-{
-	unsigned int bit_netdev = MTK_PHY_LED_STATE_NETDEV + (index ? 16 : 0);
-	struct mtk_socphy_priv *priv = phydev->priv;
-	u16 on = 0, blink = 0;
-	int ret;
-
-	if (index > 1)
-		return -EINVAL;
-
-	if (rules & BIT(TRIGGER_NETDEV_FULL_DUPLEX))
-		on |= MTK_PHY_LED_ON_FDX;
-
-	if (rules & BIT(TRIGGER_NETDEV_HALF_DUPLEX))
-		on |= MTK_PHY_LED_ON_HDX;
-
-	if (rules & (BIT(TRIGGER_NETDEV_LINK_10) | BIT(TRIGGER_NETDEV_LINK)))
-		on |= MTK_PHY_LED_ON_LINK10;
-
-	if (rules & (BIT(TRIGGER_NETDEV_LINK_100) | BIT(TRIGGER_NETDEV_LINK)))
-		on |= MTK_PHY_LED_ON_LINK100;
-
-	if (rules & (BIT(TRIGGER_NETDEV_LINK_1000) | BIT(TRIGGER_NETDEV_LINK)))
-		on |= MTK_PHY_LED_ON_LINK1000;
-
-	if (rules & BIT(TRIGGER_NETDEV_RX)) {
-		blink |= (on & MTK_PHY_LED_ON_LINK) ?
-			  (((on & MTK_PHY_LED_ON_LINK10) ?
-			    MTK_PHY_LED_BLINK_10RX : 0) |
-			   ((on & MTK_PHY_LED_ON_LINK100) ?
-			    MTK_PHY_LED_BLINK_100RX : 0) |
-			   ((on & MTK_PHY_LED_ON_LINK1000) ?
-			    MTK_PHY_LED_BLINK_1000RX : 0)) :
-			  MTK_PHY_LED_BLINK_RX;
-	}
-
-	if (rules & BIT(TRIGGER_NETDEV_TX)) {
-		blink |= (on & MTK_PHY_LED_ON_LINK) ?
-			  (((on & MTK_PHY_LED_ON_LINK10) ?
-			    MTK_PHY_LED_BLINK_10TX : 0) |
-			   ((on & MTK_PHY_LED_ON_LINK100) ?
-			    MTK_PHY_LED_BLINK_100TX : 0) |
-			   ((on & MTK_PHY_LED_ON_LINK1000) ?
-			    MTK_PHY_LED_BLINK_1000TX : 0)) :
-			  MTK_PHY_LED_BLINK_TX;
-	}
-
-	if (blink || on)
-		set_bit(bit_netdev, &priv->led_state);
-	else
-		clear_bit(bit_netdev, &priv->led_state);
-
-	ret = phy_modify_mmd(phydev, MDIO_MMD_VEND2, index ?
-				MTK_PHY_LED1_ON_CTRL :
-				MTK_PHY_LED0_ON_CTRL,
-			     MTK_PHY_LED_ON_FDX     |
-			     MTK_PHY_LED_ON_HDX     |
-			     MTK_PHY_LED_ON_LINK,
-			     on);
-
-	if (ret)
-		return ret;
-
-	return phy_write_mmd(phydev, MDIO_MMD_VEND2, index ?
-				MTK_PHY_LED1_BLINK_CTRL :
-				MTK_PHY_LED0_BLINK_CTRL, blink);
-};
-
-static bool mt7988_phy_led_get_polarity(struct phy_device *phydev, int led_num)
-{
-	struct mtk_socphy_shared *priv = phydev->shared->priv;
-	u32 polarities;
-
-	if (led_num == 0)
-		polarities = ~(priv->boottrap);
-	else
-		polarities = MTK_PHY_LED1_DEFAULT_POLARITIES;
-
-	if (polarities & BIT(phydev->mdio.addr))
-		return true;
-
-	return false;
-}
-
-static int mt7988_phy_fix_leds_polarities(struct phy_device *phydev)
-{
-	struct pinctrl *pinctrl;
-	int index;
-
-	/* Setup LED polarity according to bootstrap use of LED pins */
-	for (index = 0; index < 2; ++index)
-		phy_modify_mmd(phydev, MDIO_MMD_VEND2, index ?
-				MTK_PHY_LED1_ON_CTRL : MTK_PHY_LED0_ON_CTRL,
-			       MTK_PHY_LED_ON_POLARITY,
-			       mt7988_phy_led_get_polarity(phydev, index) ?
-				MTK_PHY_LED_ON_POLARITY : 0);
-
-	/* Only now setup pinctrl to avoid bogus blinking */
-	pinctrl = devm_pinctrl_get_select(&phydev->mdio.dev, "gbe-led");
-	if (IS_ERR(pinctrl))
-		dev_err(&phydev->mdio.bus->dev,
-			"Failed to setup PHY LED pinctrl\n");
-
-	return 0;
-}
-
-static int mt7988_phy_probe_shared(struct phy_device *phydev)
-{
-	struct device_node *np = dev_of_node(&phydev->mdio.bus->dev);
-	struct mtk_socphy_shared *shared = phydev->shared->priv;
-	struct regmap *regmap;
-	u32 reg;
-	int ret;
-
-	/* The LED0 of the 4 PHYs in MT7988 are wired to SoC pins LED_A, LED_B,
-	 * LED_C and LED_D respectively. At the same time those pins are used to
-	 * bootstrap configuration of the reference clock source (LED_A),
-	 * DRAM DDRx16b x2/x1 (LED_B) and boot device (LED_C, LED_D).
-	 * In practice this is done using a LED and a resistor pulling the pin
-	 * either to GND or to VIO.
-	 * The detected value at boot time is accessible at run-time using the
-	 * TPBANK0 register located in the gpio base of the pinctrl, in order
-	 * to read it here it needs to be referenced by a phandle called
-	 * 'mediatek,pio' in the MDIO bus hosting the PHY.
-	 * The 4 bits in TPBANK0 are kept as package shared data and are used to
-	 * set LED polarity for each of the LED0.
-	 */
-	regmap = syscon_regmap_lookup_by_phandle(np, "mediatek,pio");
-	if (IS_ERR(regmap))
-		return PTR_ERR(regmap);
-
-	ret = regmap_read(regmap, RG_GPIO_MISC_TPBANK0, &reg);
-	if (ret)
-		return ret;
-
-	shared->boottrap = FIELD_GET(RG_GPIO_MISC_TPBANK0_BOOTMODE, reg);
-
-	return 0;
-}
-
-static void mt798x_phy_leds_state_init(struct phy_device *phydev)
-{
-	int i;
-
-	for (i = 0; i < 2; ++i)
-		mt798x_phy_led_hw_control_get(phydev, i, NULL);
-}
-
-static int mt7988_phy_probe(struct phy_device *phydev)
-{
-	struct mtk_socphy_shared *shared;
-	struct mtk_socphy_priv *priv;
-	int err;
-
-	if (phydev->mdio.addr > 3)
-		return -EINVAL;
-
-	err = devm_phy_package_join(&phydev->mdio.dev, phydev, 0,
-				    sizeof(struct mtk_socphy_shared));
-	if (err)
-		return err;
-
-	if (phy_package_probe_once(phydev)) {
-		err = mt7988_phy_probe_shared(phydev);
-		if (err)
-			return err;
-	}
-
-	shared = phydev->shared->priv;
-	priv = &shared->priv[phydev->mdio.addr];
-
-	phydev->priv = priv;
-
-	mt798x_phy_leds_state_init(phydev);
-
-	err = mt7988_phy_fix_leds_polarities(phydev);
-	if (err)
-		return err;
-
-	/* Disable TX power saving at probing to:
-	 * 1. Meet common mode compliance test criteria
-	 * 2. Make sure that TX-VCM calibration works fine
-	 */
-	phy_modify_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_RXADC_CTRL_RG7,
-		       MTK_PHY_DA_AD_BUF_BIAS_LP_MASK, 0x3 << 8);
-
-	return mt798x_phy_calibration(phydev);
-}
-
-static int mt7981_phy_probe(struct phy_device *phydev)
-{
-	struct mtk_socphy_priv *priv;
-
-	priv = devm_kzalloc(&phydev->mdio.dev, sizeof(struct mtk_socphy_priv),
-			    GFP_KERNEL);
-	if (!priv)
-		return -ENOMEM;
-
-	phydev->priv = priv;
-
-	mt798x_phy_leds_state_init(phydev);
-
-	return mt798x_phy_calibration(phydev);
-}
-
-static struct phy_driver mtk_socphy_driver[] = {
-	{
-		PHY_ID_MATCH_EXACT(MTK_GPHY_ID_MT7981),
-		.name		= "MediaTek MT7981 PHY",
-		.config_init	= mt798x_phy_config_init,
-		.config_intr	= genphy_no_config_intr,
-		.handle_interrupt = genphy_handle_interrupt_no_ack,
-		.probe		= mt7981_phy_probe,
-		.suspend	= genphy_suspend,
-		.resume		= genphy_resume,
-		.read_page	= mtk_socphy_read_page,
-		.write_page	= mtk_socphy_write_page,
-		.led_blink_set	= mt798x_phy_led_blink_set,
-		.led_brightness_set = mt798x_phy_led_brightness_set,
-		.led_hw_is_supported = mt798x_phy_led_hw_is_supported,
-		.led_hw_control_set = mt798x_phy_led_hw_control_set,
-		.led_hw_control_get = mt798x_phy_led_hw_control_get,
-	},
-	{
-		PHY_ID_MATCH_EXACT(MTK_GPHY_ID_MT7988),
-		.name		= "MediaTek MT7988 PHY",
-		.config_init	= mt798x_phy_config_init,
-		.config_intr	= genphy_no_config_intr,
-		.handle_interrupt = genphy_handle_interrupt_no_ack,
-		.probe		= mt7988_phy_probe,
-		.suspend	= genphy_suspend,
-		.resume		= genphy_resume,
-		.read_page	= mtk_socphy_read_page,
-		.write_page	= mtk_socphy_write_page,
-		.led_blink_set	= mt798x_phy_led_blink_set,
-		.led_brightness_set = mt798x_phy_led_brightness_set,
-		.led_hw_is_supported = mt798x_phy_led_hw_is_supported,
-		.led_hw_control_set = mt798x_phy_led_hw_control_set,
-		.led_hw_control_get = mt798x_phy_led_hw_control_get,
-	},
-};
-
-module_phy_driver(mtk_socphy_driver);
-
-static struct mdio_device_id __maybe_unused mtk_socphy_tbl[] = {
-	{ PHY_ID_MATCH_EXACT(MTK_GPHY_ID_MT7981) },
-	{ PHY_ID_MATCH_EXACT(MTK_GPHY_ID_MT7988) },
-	{ }
-};
-
-MODULE_DESCRIPTION("MediaTek SoC Gigabit Ethernet PHY driver");
-MODULE_AUTHOR("Daniel Golle <daniel@makrotopia.org>");
-MODULE_AUTHOR("SkyLake Huang <SkyLake.Huang@mediatek.com>");
-MODULE_LICENSE("GPL");
-
-MODULE_DEVICE_TABLE(mdio, mtk_socphy_tbl);
--- a/drivers/net/phy/mediatek-ge.c
+++ /dev/null
@@ -1,114 +0,0 @@
-// SPDX-License-Identifier: GPL-2.0+
-#include <linux/bitfield.h>
-#include <linux/module.h>
-#include <linux/phy.h>
-
-#define MTK_EXT_PAGE_ACCESS		0x1f
-#define MTK_PHY_PAGE_STANDARD		0x0000
-#define MTK_PHY_PAGE_EXTENDED		0x0001
-#define MTK_PHY_PAGE_EXTENDED_2		0x0002
-#define MTK_PHY_PAGE_EXTENDED_3		0x0003
-#define MTK_PHY_PAGE_EXTENDED_2A30	0x2a30
-#define MTK_PHY_PAGE_EXTENDED_52B5	0x52b5
-
-static int mtk_gephy_read_page(struct phy_device *phydev)
-{
-	return __phy_read(phydev, MTK_EXT_PAGE_ACCESS);
-}
-
-static int mtk_gephy_write_page(struct phy_device *phydev, int page)
-{
-	return __phy_write(phydev, MTK_EXT_PAGE_ACCESS, page);
-}
-
-static void mtk_gephy_config_init(struct phy_device *phydev)
-{
-	/* Disable EEE */
-	phy_write_mmd(phydev, MDIO_MMD_AN, MDIO_AN_EEE_ADV, 0);
-
-	/* Enable HW auto downshift */
-	phy_modify_paged(phydev, MTK_PHY_PAGE_EXTENDED, 0x14, 0, BIT(4));
-
-	/* Increase SlvDPSready time */
-	phy_select_page(phydev, MTK_PHY_PAGE_EXTENDED_52B5);
-	__phy_write(phydev, 0x10, 0xafae);
-	__phy_write(phydev, 0x12, 0x2f);
-	__phy_write(phydev, 0x10, 0x8fae);
-	phy_restore_page(phydev, MTK_PHY_PAGE_STANDARD, 0);
-
-	/* Adjust 100_mse_threshold */
-	phy_write_mmd(phydev, MDIO_MMD_VEND1, 0x123, 0xffff);
-
-	/* Disable mcc */
-	phy_write_mmd(phydev, MDIO_MMD_VEND1, 0xa6, 0x300);
-}
-
-static int mt7530_phy_config_init(struct phy_device *phydev)
-{
-	mtk_gephy_config_init(phydev);
-
-	/* Increase post_update_timer */
-	phy_write_paged(phydev, MTK_PHY_PAGE_EXTENDED_3, 0x11, 0x4b);
-
-	return 0;
-}
-
-static int mt7531_phy_config_init(struct phy_device *phydev)
-{
-	mtk_gephy_config_init(phydev);
-
-	/* PHY link down power saving enable */
-	phy_set_bits(phydev, 0x17, BIT(4));
-	phy_clear_bits_mmd(phydev, MDIO_MMD_VEND1, 0xc6, 0x300);
-
-	/* Set TX Pair delay selection */
-	phy_write_mmd(phydev, MDIO_MMD_VEND1, 0x13, 0x404);
-	phy_write_mmd(phydev, MDIO_MMD_VEND1, 0x14, 0x404);
-
-	return 0;
-}
-
-static struct phy_driver mtk_gephy_driver[] = {
-	{
-		PHY_ID_MATCH_EXACT(0x03a29412),
-		.name		= "MediaTek MT7530 PHY",
-		.config_init	= mt7530_phy_config_init,
-		/* Interrupts are handled by the switch, not the PHY
-		 * itself.
-		 */
-		.config_intr	= genphy_no_config_intr,
-		.handle_interrupt = genphy_handle_interrupt_no_ack,
-		.suspend	= genphy_suspend,
-		.resume		= genphy_resume,
-		.read_page	= mtk_gephy_read_page,
-		.write_page	= mtk_gephy_write_page,
-	},
-	{
-		PHY_ID_MATCH_EXACT(0x03a29441),
-		.name		= "MediaTek MT7531 PHY",
-		.config_init	= mt7531_phy_config_init,
-		/* Interrupts are handled by the switch, not the PHY
-		 * itself.
-		 */
-		.config_intr	= genphy_no_config_intr,
-		.handle_interrupt = genphy_handle_interrupt_no_ack,
-		.suspend	= genphy_suspend,
-		.resume		= genphy_resume,
-		.read_page	= mtk_gephy_read_page,
-		.write_page	= mtk_gephy_write_page,
-	},
-};
-
-module_phy_driver(mtk_gephy_driver);
-
-static struct mdio_device_id __maybe_unused mtk_gephy_tbl[] = {
-	{ PHY_ID_MATCH_EXACT(0x03a29441) },
-	{ PHY_ID_MATCH_EXACT(0x03a29412) },
-	{ }
-};
-
-MODULE_DESCRIPTION("MediaTek Gigabit Ethernet PHY driver");
-MODULE_AUTHOR("DENG, Qingfang <dqfext@gmail.com>");
-MODULE_LICENSE("GPL");
-
-MODULE_DEVICE_TABLE(mdio, mtk_gephy_tbl);
--- /dev/null
+++ b/drivers/net/phy/mediatek/mtk-ge-soc.c
@@ -0,0 +1,1610 @@
+// SPDX-License-Identifier: GPL-2.0+
+#include <linux/bitfield.h>
+#include <linux/bitmap.h>
+#include <linux/mfd/syscon.h>
+#include <linux/module.h>
+#include <linux/nvmem-consumer.h>
+#include <linux/pinctrl/consumer.h>
+#include <linux/phy.h>
+#include <linux/regmap.h>
+
+#define MTK_GPHY_ID_MT7981			0x03a29461
+#define MTK_GPHY_ID_MT7988			0x03a29481
+
+#define MTK_EXT_PAGE_ACCESS			0x1f
+#define MTK_PHY_PAGE_STANDARD			0x0000
+#define MTK_PHY_PAGE_EXTENDED_3			0x0003
+
+#define MTK_PHY_LPI_REG_14			0x14
+#define MTK_PHY_LPI_WAKE_TIMER_1000_MASK	GENMASK(8, 0)
+
+#define MTK_PHY_LPI_REG_1c			0x1c
+#define MTK_PHY_SMI_DET_ON_THRESH_MASK		GENMASK(13, 8)
+
+#define MTK_PHY_PAGE_EXTENDED_2A30		0x2a30
+#define MTK_PHY_PAGE_EXTENDED_52B5		0x52b5
+
+#define ANALOG_INTERNAL_OPERATION_MAX_US	20
+#define TXRESERVE_MIN				0
+#define TXRESERVE_MAX				7
+
+#define MTK_PHY_ANARG_RG			0x10
+#define   MTK_PHY_TCLKOFFSET_MASK		GENMASK(12, 8)
+
+/* Registers on MDIO_MMD_VEND1 */
+#define MTK_PHY_TXVLD_DA_RG			0x12
+#define   MTK_PHY_DA_TX_I2MPB_A_GBE_MASK	GENMASK(15, 10)
+#define   MTK_PHY_DA_TX_I2MPB_A_TBT_MASK	GENMASK(5, 0)
+
+#define MTK_PHY_TX_I2MPB_TEST_MODE_A2		0x16
+#define   MTK_PHY_DA_TX_I2MPB_A_HBT_MASK	GENMASK(15, 10)
+#define   MTK_PHY_DA_TX_I2MPB_A_TST_MASK	GENMASK(5, 0)
+
+#define MTK_PHY_TX_I2MPB_TEST_MODE_B1		0x17
+#define   MTK_PHY_DA_TX_I2MPB_B_GBE_MASK	GENMASK(13, 8)
+#define   MTK_PHY_DA_TX_I2MPB_B_TBT_MASK	GENMASK(5, 0)
+
+#define MTK_PHY_TX_I2MPB_TEST_MODE_B2		0x18
+#define   MTK_PHY_DA_TX_I2MPB_B_HBT_MASK	GENMASK(13, 8)
+#define   MTK_PHY_DA_TX_I2MPB_B_TST_MASK	GENMASK(5, 0)
+
+#define MTK_PHY_TX_I2MPB_TEST_MODE_C1		0x19
+#define   MTK_PHY_DA_TX_I2MPB_C_GBE_MASK	GENMASK(13, 8)
+#define   MTK_PHY_DA_TX_I2MPB_C_TBT_MASK	GENMASK(5, 0)
+
+#define MTK_PHY_TX_I2MPB_TEST_MODE_C2		0x20
+#define   MTK_PHY_DA_TX_I2MPB_C_HBT_MASK	GENMASK(13, 8)
+#define   MTK_PHY_DA_TX_I2MPB_C_TST_MASK	GENMASK(5, 0)
+
+#define MTK_PHY_TX_I2MPB_TEST_MODE_D1		0x21
+#define   MTK_PHY_DA_TX_I2MPB_D_GBE_MASK	GENMASK(13, 8)
+#define   MTK_PHY_DA_TX_I2MPB_D_TBT_MASK	GENMASK(5, 0)
+
+#define MTK_PHY_TX_I2MPB_TEST_MODE_D2		0x22
+#define   MTK_PHY_DA_TX_I2MPB_D_HBT_MASK	GENMASK(13, 8)
+#define   MTK_PHY_DA_TX_I2MPB_D_TST_MASK	GENMASK(5, 0)
+
+#define MTK_PHY_RXADC_CTRL_RG7			0xc6
+#define   MTK_PHY_DA_AD_BUF_BIAS_LP_MASK	GENMASK(9, 8)
+
+#define MTK_PHY_RXADC_CTRL_RG9			0xc8
+#define   MTK_PHY_DA_RX_PSBN_TBT_MASK		GENMASK(14, 12)
+#define   MTK_PHY_DA_RX_PSBN_HBT_MASK		GENMASK(10, 8)
+#define   MTK_PHY_DA_RX_PSBN_GBE_MASK		GENMASK(6, 4)
+#define   MTK_PHY_DA_RX_PSBN_LP_MASK		GENMASK(2, 0)
+
+#define MTK_PHY_LDO_OUTPUT_V			0xd7
+
+#define MTK_PHY_RG_ANA_CAL_RG0			0xdb
+#define   MTK_PHY_RG_CAL_CKINV			BIT(12)
+#define   MTK_PHY_RG_ANA_CALEN			BIT(8)
+#define   MTK_PHY_RG_ZCALEN_A			BIT(0)
+
+#define MTK_PHY_RG_ANA_CAL_RG1			0xdc
+#define   MTK_PHY_RG_ZCALEN_B			BIT(12)
+#define   MTK_PHY_RG_ZCALEN_C			BIT(8)
+#define   MTK_PHY_RG_ZCALEN_D			BIT(4)
+#define   MTK_PHY_RG_TXVOS_CALEN		BIT(0)
+
+#define MTK_PHY_RG_ANA_CAL_RG5			0xe0
+#define   MTK_PHY_RG_REXT_TRIM_MASK		GENMASK(13, 8)
+
+#define MTK_PHY_RG_TX_FILTER			0xfe
+
+#define MTK_PHY_RG_LPI_PCS_DSP_CTRL_REG120	0x120
+#define   MTK_PHY_LPI_SIG_EN_LO_THRESH1000_MASK	GENMASK(12, 8)
+#define   MTK_PHY_LPI_SIG_EN_HI_THRESH1000_MASK	GENMASK(4, 0)
+
+#define MTK_PHY_RG_LPI_PCS_DSP_CTRL_REG122	0x122
+#define   MTK_PHY_LPI_NORM_MSE_HI_THRESH1000_MASK	GENMASK(7, 0)
+
+#define MTK_PHY_RG_TESTMUX_ADC_CTRL		0x144
+#define   MTK_PHY_RG_TXEN_DIG_MASK		GENMASK(5, 5)
+
+#define MTK_PHY_RG_CR_TX_AMP_OFFSET_A_B		0x172
+#define   MTK_PHY_CR_TX_AMP_OFFSET_A_MASK	GENMASK(13, 8)
+#define   MTK_PHY_CR_TX_AMP_OFFSET_B_MASK	GENMASK(6, 0)
+
+#define MTK_PHY_RG_CR_TX_AMP_OFFSET_C_D		0x173
+#define   MTK_PHY_CR_TX_AMP_OFFSET_C_MASK	GENMASK(13, 8)
+#define   MTK_PHY_CR_TX_AMP_OFFSET_D_MASK	GENMASK(6, 0)
+
+#define MTK_PHY_RG_AD_CAL_COMP			0x17a
+#define   MTK_PHY_AD_CAL_COMP_OUT_MASK		GENMASK(8, 8)
+
+#define MTK_PHY_RG_AD_CAL_CLK			0x17b
+#define   MTK_PHY_DA_CAL_CLK			BIT(0)
+
+#define MTK_PHY_RG_AD_CALIN			0x17c
+#define   MTK_PHY_DA_CALIN_FLAG			BIT(0)
+
+#define MTK_PHY_RG_DASN_DAC_IN0_A		0x17d
+#define   MTK_PHY_DASN_DAC_IN0_A_MASK		GENMASK(9, 0)
+
+#define MTK_PHY_RG_DASN_DAC_IN0_B		0x17e
+#define   MTK_PHY_DASN_DAC_IN0_B_MASK		GENMASK(9, 0)
+
+#define MTK_PHY_RG_DASN_DAC_IN0_C		0x17f
+#define   MTK_PHY_DASN_DAC_IN0_C_MASK		GENMASK(9, 0)
+
+#define MTK_PHY_RG_DASN_DAC_IN0_D		0x180
+#define   MTK_PHY_DASN_DAC_IN0_D_MASK		GENMASK(9, 0)
+
+#define MTK_PHY_RG_DASN_DAC_IN1_A		0x181
+#define   MTK_PHY_DASN_DAC_IN1_A_MASK		GENMASK(9, 0)
+
+#define MTK_PHY_RG_DASN_DAC_IN1_B		0x182
+#define   MTK_PHY_DASN_DAC_IN1_B_MASK		GENMASK(9, 0)
+
+#define MTK_PHY_RG_DASN_DAC_IN1_C		0x183
+#define   MTK_PHY_DASN_DAC_IN1_C_MASK		GENMASK(9, 0)
+
+#define MTK_PHY_RG_DASN_DAC_IN1_D		0x184
+#define   MTK_PHY_DASN_DAC_IN1_D_MASK		GENMASK(9, 0)
+
+#define MTK_PHY_RG_DEV1E_REG19b			0x19b
+#define   MTK_PHY_BYPASS_DSP_LPI_READY		BIT(8)
+
+#define MTK_PHY_RG_LP_IIR2_K1_L			0x22a
+#define MTK_PHY_RG_LP_IIR2_K1_U			0x22b
+#define MTK_PHY_RG_LP_IIR2_K2_L			0x22c
+#define MTK_PHY_RG_LP_IIR2_K2_U			0x22d
+#define MTK_PHY_RG_LP_IIR2_K3_L			0x22e
+#define MTK_PHY_RG_LP_IIR2_K3_U			0x22f
+#define MTK_PHY_RG_LP_IIR2_K4_L			0x230
+#define MTK_PHY_RG_LP_IIR2_K4_U			0x231
+#define MTK_PHY_RG_LP_IIR2_K5_L			0x232
+#define MTK_PHY_RG_LP_IIR2_K5_U			0x233
+
+#define MTK_PHY_RG_DEV1E_REG234			0x234
+#define   MTK_PHY_TR_OPEN_LOOP_EN_MASK		GENMASK(0, 0)
+#define   MTK_PHY_LPF_X_AVERAGE_MASK		GENMASK(7, 4)
+#define   MTK_PHY_TR_LP_IIR_EEE_EN		BIT(12)
+
+#define MTK_PHY_RG_LPF_CNT_VAL			0x235
+
+#define MTK_PHY_RG_DEV1E_REG238			0x238
+#define   MTK_PHY_LPI_SLV_SEND_TX_TIMER_MASK	GENMASK(8, 0)
+#define   MTK_PHY_LPI_SLV_SEND_TX_EN		BIT(12)
+
+#define MTK_PHY_RG_DEV1E_REG239			0x239
+#define   MTK_PHY_LPI_SEND_LOC_TIMER_MASK	GENMASK(8, 0)
+#define   MTK_PHY_LPI_TXPCS_LOC_RCV		BIT(12)
+
+#define MTK_PHY_RG_DEV1E_REG27C			0x27c
+#define   MTK_PHY_VGASTATE_FFE_THR_ST1_MASK	GENMASK(12, 8)
+#define MTK_PHY_RG_DEV1E_REG27D			0x27d
+#define   MTK_PHY_VGASTATE_FFE_THR_ST2_MASK	GENMASK(4, 0)
+
+#define MTK_PHY_RG_DEV1E_REG2C7			0x2c7
+#define   MTK_PHY_MAX_GAIN_MASK			GENMASK(4, 0)
+#define   MTK_PHY_MIN_GAIN_MASK			GENMASK(12, 8)
+
+#define MTK_PHY_RG_DEV1E_REG2D1			0x2d1
+#define   MTK_PHY_VCO_SLICER_THRESH_BITS_HIGH_EEE_MASK	GENMASK(7, 0)
+#define   MTK_PHY_LPI_SKIP_SD_SLV_TR		BIT(8)
+#define   MTK_PHY_LPI_TR_READY			BIT(9)
+#define   MTK_PHY_LPI_VCO_EEE_STG0_EN		BIT(10)
+
+#define MTK_PHY_RG_DEV1E_REG323			0x323
+#define   MTK_PHY_EEE_WAKE_MAS_INT_DC		BIT(0)
+#define   MTK_PHY_EEE_WAKE_SLV_INT_DC		BIT(4)
+
+#define MTK_PHY_RG_DEV1E_REG324			0x324
+#define   MTK_PHY_SMI_DETCNT_MAX_MASK		GENMASK(5, 0)
+#define   MTK_PHY_SMI_DET_MAX_EN		BIT(8)
+
+#define MTK_PHY_RG_DEV1E_REG326			0x326
+#define   MTK_PHY_LPI_MODE_SD_ON		BIT(0)
+#define   MTK_PHY_RESET_RANDUPD_CNT		BIT(1)
+#define   MTK_PHY_TREC_UPDATE_ENAB_CLR		BIT(2)
+#define   MTK_PHY_LPI_QUIT_WAIT_DFE_SIG_DET_OFF	BIT(4)
+#define   MTK_PHY_TR_READY_SKIP_AFE_WAKEUP	BIT(5)
+
+#define MTK_PHY_LDO_PUMP_EN_PAIRAB		0x502
+#define MTK_PHY_LDO_PUMP_EN_PAIRCD		0x503
+
+#define MTK_PHY_DA_TX_R50_PAIR_A		0x53d
+#define MTK_PHY_DA_TX_R50_PAIR_B		0x53e
+#define MTK_PHY_DA_TX_R50_PAIR_C		0x53f
+#define MTK_PHY_DA_TX_R50_PAIR_D		0x540
+
+/* Registers on MDIO_MMD_VEND2 */
+#define MTK_PHY_LED0_ON_CTRL			0x24
+#define MTK_PHY_LED1_ON_CTRL			0x26
+#define   MTK_PHY_LED_ON_MASK			GENMASK(6, 0)
+#define   MTK_PHY_LED_ON_LINK1000		BIT(0)
+#define   MTK_PHY_LED_ON_LINK100		BIT(1)
+#define   MTK_PHY_LED_ON_LINK10			BIT(2)
+#define   MTK_PHY_LED_ON_LINK			(MTK_PHY_LED_ON_LINK10 |\
+						 MTK_PHY_LED_ON_LINK100 |\
+						 MTK_PHY_LED_ON_LINK1000)
+#define   MTK_PHY_LED_ON_LINKDOWN		BIT(3)
+#define   MTK_PHY_LED_ON_FDX			BIT(4) /* Full duplex */
+#define   MTK_PHY_LED_ON_HDX			BIT(5) /* Half duplex */
+#define   MTK_PHY_LED_ON_FORCE_ON		BIT(6)
+#define   MTK_PHY_LED_ON_POLARITY		BIT(14)
+#define   MTK_PHY_LED_ON_ENABLE			BIT(15)
+
+#define MTK_PHY_LED0_BLINK_CTRL			0x25
+#define MTK_PHY_LED1_BLINK_CTRL			0x27
+#define   MTK_PHY_LED_BLINK_1000TX		BIT(0)
+#define   MTK_PHY_LED_BLINK_1000RX		BIT(1)
+#define   MTK_PHY_LED_BLINK_100TX		BIT(2)
+#define   MTK_PHY_LED_BLINK_100RX		BIT(3)
+#define   MTK_PHY_LED_BLINK_10TX		BIT(4)
+#define   MTK_PHY_LED_BLINK_10RX		BIT(5)
+#define   MTK_PHY_LED_BLINK_RX			(MTK_PHY_LED_BLINK_10RX |\
+						 MTK_PHY_LED_BLINK_100RX |\
+						 MTK_PHY_LED_BLINK_1000RX)
+#define   MTK_PHY_LED_BLINK_TX			(MTK_PHY_LED_BLINK_10TX |\
+						 MTK_PHY_LED_BLINK_100TX |\
+						 MTK_PHY_LED_BLINK_1000TX)
+#define   MTK_PHY_LED_BLINK_COLLISION		BIT(6)
+#define   MTK_PHY_LED_BLINK_RX_CRC_ERR		BIT(7)
+#define   MTK_PHY_LED_BLINK_RX_IDLE_ERR		BIT(8)
+#define   MTK_PHY_LED_BLINK_FORCE_BLINK		BIT(9)
+
+#define MTK_PHY_LED1_DEFAULT_POLARITIES		BIT(1)
+
+#define MTK_PHY_RG_BG_RASEL			0x115
+#define   MTK_PHY_RG_BG_RASEL_MASK		GENMASK(2, 0)
+
+/* 'boottrap' register reflecting the configuration of the 4 PHY LEDs */
+#define RG_GPIO_MISC_TPBANK0			0x6f0
+#define   RG_GPIO_MISC_TPBANK0_BOOTMODE		GENMASK(11, 8)
+
+/* These macro privides efuse parsing for internal phy. */
+#define EFS_DA_TX_I2MPB_A(x)			(((x) >> 0) & GENMASK(5, 0))
+#define EFS_DA_TX_I2MPB_B(x)			(((x) >> 6) & GENMASK(5, 0))
+#define EFS_DA_TX_I2MPB_C(x)			(((x) >> 12) & GENMASK(5, 0))
+#define EFS_DA_TX_I2MPB_D(x)			(((x) >> 18) & GENMASK(5, 0))
+#define EFS_DA_TX_AMP_OFFSET_A(x)		(((x) >> 24) & GENMASK(5, 0))
+
+#define EFS_DA_TX_AMP_OFFSET_B(x)		(((x) >> 0) & GENMASK(5, 0))
+#define EFS_DA_TX_AMP_OFFSET_C(x)		(((x) >> 6) & GENMASK(5, 0))
+#define EFS_DA_TX_AMP_OFFSET_D(x)		(((x) >> 12) & GENMASK(5, 0))
+#define EFS_DA_TX_R50_A(x)			(((x) >> 18) & GENMASK(5, 0))
+#define EFS_DA_TX_R50_B(x)			(((x) >> 24) & GENMASK(5, 0))
+
+#define EFS_DA_TX_R50_C(x)			(((x) >> 0) & GENMASK(5, 0))
+#define EFS_DA_TX_R50_D(x)			(((x) >> 6) & GENMASK(5, 0))
+
+#define EFS_RG_BG_RASEL(x)			(((x) >> 4) & GENMASK(2, 0))
+#define EFS_RG_REXT_TRIM(x)			(((x) >> 7) & GENMASK(5, 0))
+
+enum {
+	NO_PAIR,
+	PAIR_A,
+	PAIR_B,
+	PAIR_C,
+	PAIR_D,
+};
+
+enum calibration_mode {
+	EFUSE_K,
+	SW_K
+};
+
+enum CAL_ITEM {
+	REXT,
+	TX_OFFSET,
+	TX_AMP,
+	TX_R50,
+	TX_VCM
+};
+
+enum CAL_MODE {
+	EFUSE_M,
+	SW_M
+};
+
+#define MTK_PHY_LED_STATE_FORCE_ON	0
+#define MTK_PHY_LED_STATE_FORCE_BLINK	1
+#define MTK_PHY_LED_STATE_NETDEV	2
+
+struct mtk_socphy_priv {
+	unsigned long		led_state;
+};
+
+struct mtk_socphy_shared {
+	u32			boottrap;
+	struct mtk_socphy_priv	priv[4];
+};
+
+static int mtk_socphy_read_page(struct phy_device *phydev)
+{
+	return __phy_read(phydev, MTK_EXT_PAGE_ACCESS);
+}
+
+static int mtk_socphy_write_page(struct phy_device *phydev, int page)
+{
+	return __phy_write(phydev, MTK_EXT_PAGE_ACCESS, page);
+}
+
+/* One calibration cycle consists of:
+ * 1.Set DA_CALIN_FLAG high to start calibration. Keep it high
+ *   until AD_CAL_COMP is ready to output calibration result.
+ * 2.Wait until DA_CAL_CLK is available.
+ * 3.Fetch AD_CAL_COMP_OUT.
+ */
+static int cal_cycle(struct phy_device *phydev, int devad,
+		     u32 regnum, u16 mask, u16 cal_val)
+{
+	int reg_val;
+	int ret;
+
+	phy_modify_mmd(phydev, devad, regnum,
+		       mask, cal_val);
+	phy_set_bits_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_RG_AD_CALIN,
+			 MTK_PHY_DA_CALIN_FLAG);
+
+	ret = phy_read_mmd_poll_timeout(phydev, MDIO_MMD_VEND1,
+					MTK_PHY_RG_AD_CAL_CLK, reg_val,
+					reg_val & MTK_PHY_DA_CAL_CLK, 500,
+					ANALOG_INTERNAL_OPERATION_MAX_US,
+					false);
+	if (ret) {
+		phydev_err(phydev, "Calibration cycle timeout\n");
+		return ret;
+	}
+
+	phy_clear_bits_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_RG_AD_CALIN,
+			   MTK_PHY_DA_CALIN_FLAG);
+	ret = phy_read_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_RG_AD_CAL_COMP);
+	if (ret < 0)
+		return ret;
+	ret = FIELD_GET(MTK_PHY_AD_CAL_COMP_OUT_MASK, ret);
+	phydev_dbg(phydev, "cal_val: 0x%x, ret: %d\n", cal_val, ret);
+
+	return ret;
+}
+
+static int rext_fill_result(struct phy_device *phydev, u16 *buf)
+{
+	phy_modify_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_RG_ANA_CAL_RG5,
+		       MTK_PHY_RG_REXT_TRIM_MASK, buf[0] << 8);
+	phy_modify_mmd(phydev, MDIO_MMD_VEND2, MTK_PHY_RG_BG_RASEL,
+		       MTK_PHY_RG_BG_RASEL_MASK, buf[1]);
+
+	return 0;
+}
+
+static int rext_cal_efuse(struct phy_device *phydev, u32 *buf)
+{
+	u16 rext_cal_val[2];
+
+	rext_cal_val[0] = EFS_RG_REXT_TRIM(buf[3]);
+	rext_cal_val[1] = EFS_RG_BG_RASEL(buf[3]);
+	rext_fill_result(phydev, rext_cal_val);
+
+	return 0;
+}
+
+static int tx_offset_fill_result(struct phy_device *phydev, u16 *buf)
+{
+	phy_modify_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_RG_CR_TX_AMP_OFFSET_A_B,
+		       MTK_PHY_CR_TX_AMP_OFFSET_A_MASK, buf[0] << 8);
+	phy_modify_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_RG_CR_TX_AMP_OFFSET_A_B,
+		       MTK_PHY_CR_TX_AMP_OFFSET_B_MASK, buf[1]);
+	phy_modify_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_RG_CR_TX_AMP_OFFSET_C_D,
+		       MTK_PHY_CR_TX_AMP_OFFSET_C_MASK, buf[2] << 8);
+	phy_modify_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_RG_CR_TX_AMP_OFFSET_C_D,
+		       MTK_PHY_CR_TX_AMP_OFFSET_D_MASK, buf[3]);
+
+	return 0;
+}
+
+static int tx_offset_cal_efuse(struct phy_device *phydev, u32 *buf)
+{
+	u16 tx_offset_cal_val[4];
+
+	tx_offset_cal_val[0] = EFS_DA_TX_AMP_OFFSET_A(buf[0]);
+	tx_offset_cal_val[1] = EFS_DA_TX_AMP_OFFSET_B(buf[1]);
+	tx_offset_cal_val[2] = EFS_DA_TX_AMP_OFFSET_C(buf[1]);
+	tx_offset_cal_val[3] = EFS_DA_TX_AMP_OFFSET_D(buf[1]);
+
+	tx_offset_fill_result(phydev, tx_offset_cal_val);
+
+	return 0;
+}
+
+static int tx_amp_fill_result(struct phy_device *phydev, u16 *buf)
+{
+	const int vals_9481[16] = { 10, 6, 6, 10,
+				    10, 6, 6, 10,
+				    10, 6, 6, 10,
+				    10, 6, 6, 10 };
+	const int vals_9461[16] = { 7, 1, 4, 7,
+				    7, 1, 4, 7,
+				    7, 1, 4, 7,
+				    7, 1, 4, 7 };
+	int bias[16] = {};
+	int i;
+
+	switch (phydev->drv->phy_id) {
+	case MTK_GPHY_ID_MT7981:
+		/* We add some calibration to efuse values
+		 * due to board level influence.
+		 * GBE: +7, TBT: +1, HBT: +4, TST: +7
+		 */
+		memcpy(bias, (const void *)vals_9461, sizeof(bias));
+		break;
+	case MTK_GPHY_ID_MT7988:
+		memcpy(bias, (const void *)vals_9481, sizeof(bias));
+		break;
+	}
+
+	/* Prevent overflow */
+	for (i = 0; i < 12; i++) {
+		if (buf[i >> 2] + bias[i] > 63) {
+			buf[i >> 2] = 63;
+			bias[i] = 0;
+		}
+	}
+
+	phy_modify_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_TXVLD_DA_RG,
+		       MTK_PHY_DA_TX_I2MPB_A_GBE_MASK,
+		       FIELD_PREP(MTK_PHY_DA_TX_I2MPB_A_GBE_MASK,
+				  buf[0] + bias[0]));
+	phy_modify_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_TXVLD_DA_RG,
+		       MTK_PHY_DA_TX_I2MPB_A_TBT_MASK,
+		       FIELD_PREP(MTK_PHY_DA_TX_I2MPB_A_TBT_MASK,
+				  buf[0] + bias[1]));
+	phy_modify_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_TX_I2MPB_TEST_MODE_A2,
+		       MTK_PHY_DA_TX_I2MPB_A_HBT_MASK,
+		       FIELD_PREP(MTK_PHY_DA_TX_I2MPB_A_HBT_MASK,
+				  buf[0] + bias[2]));
+	phy_modify_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_TX_I2MPB_TEST_MODE_A2,
+		       MTK_PHY_DA_TX_I2MPB_A_TST_MASK,
+		       FIELD_PREP(MTK_PHY_DA_TX_I2MPB_A_TST_MASK,
+				  buf[0] + bias[3]));
+
+	phy_modify_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_TX_I2MPB_TEST_MODE_B1,
+		       MTK_PHY_DA_TX_I2MPB_B_GBE_MASK,
+		       FIELD_PREP(MTK_PHY_DA_TX_I2MPB_B_GBE_MASK,
+				  buf[1] + bias[4]));
+	phy_modify_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_TX_I2MPB_TEST_MODE_B1,
+		       MTK_PHY_DA_TX_I2MPB_B_TBT_MASK,
+		       FIELD_PREP(MTK_PHY_DA_TX_I2MPB_B_TBT_MASK,
+				  buf[1] + bias[5]));
+	phy_modify_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_TX_I2MPB_TEST_MODE_B2,
+		       MTK_PHY_DA_TX_I2MPB_B_HBT_MASK,
+		       FIELD_PREP(MTK_PHY_DA_TX_I2MPB_B_HBT_MASK,
+				  buf[1] + bias[6]));
+	phy_modify_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_TX_I2MPB_TEST_MODE_B2,
+		       MTK_PHY_DA_TX_I2MPB_B_TST_MASK,
+		       FIELD_PREP(MTK_PHY_DA_TX_I2MPB_B_TST_MASK,
+				  buf[1] + bias[7]));
+
+	phy_modify_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_TX_I2MPB_TEST_MODE_C1,
+		       MTK_PHY_DA_TX_I2MPB_C_GBE_MASK,
+		       FIELD_PREP(MTK_PHY_DA_TX_I2MPB_C_GBE_MASK,
+				  buf[2] + bias[8]));
+	phy_modify_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_TX_I2MPB_TEST_MODE_C1,
+		       MTK_PHY_DA_TX_I2MPB_C_TBT_MASK,
+		       FIELD_PREP(MTK_PHY_DA_TX_I2MPB_C_TBT_MASK,
+				  buf[2] + bias[9]));
+	phy_modify_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_TX_I2MPB_TEST_MODE_C2,
+		       MTK_PHY_DA_TX_I2MPB_C_HBT_MASK,
+		       FIELD_PREP(MTK_PHY_DA_TX_I2MPB_C_HBT_MASK,
+				  buf[2] + bias[10]));
+	phy_modify_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_TX_I2MPB_TEST_MODE_C2,
+		       MTK_PHY_DA_TX_I2MPB_C_TST_MASK,
+		       FIELD_PREP(MTK_PHY_DA_TX_I2MPB_C_TST_MASK,
+				  buf[2] + bias[11]));
+
+	phy_modify_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_TX_I2MPB_TEST_MODE_D1,
+		       MTK_PHY_DA_TX_I2MPB_D_GBE_MASK,
+		       FIELD_PREP(MTK_PHY_DA_TX_I2MPB_D_GBE_MASK,
+				  buf[3] + bias[12]));
+	phy_modify_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_TX_I2MPB_TEST_MODE_D1,
+		       MTK_PHY_DA_TX_I2MPB_D_TBT_MASK,
+		       FIELD_PREP(MTK_PHY_DA_TX_I2MPB_D_TBT_MASK,
+				  buf[3] + bias[13]));
+	phy_modify_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_TX_I2MPB_TEST_MODE_D2,
+		       MTK_PHY_DA_TX_I2MPB_D_HBT_MASK,
+		       FIELD_PREP(MTK_PHY_DA_TX_I2MPB_D_HBT_MASK,
+				  buf[3] + bias[14]));
+	phy_modify_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_TX_I2MPB_TEST_MODE_D2,
+		       MTK_PHY_DA_TX_I2MPB_D_TST_MASK,
+		       FIELD_PREP(MTK_PHY_DA_TX_I2MPB_D_TST_MASK,
+				  buf[3] + bias[15]));
+
+	return 0;
+}
+
+static int tx_amp_cal_efuse(struct phy_device *phydev, u32 *buf)
+{
+	u16 tx_amp_cal_val[4];
+
+	tx_amp_cal_val[0] = EFS_DA_TX_I2MPB_A(buf[0]);
+	tx_amp_cal_val[1] = EFS_DA_TX_I2MPB_B(buf[0]);
+	tx_amp_cal_val[2] = EFS_DA_TX_I2MPB_C(buf[0]);
+	tx_amp_cal_val[3] = EFS_DA_TX_I2MPB_D(buf[0]);
+	tx_amp_fill_result(phydev, tx_amp_cal_val);
+
+	return 0;
+}
+
+static int tx_r50_fill_result(struct phy_device *phydev, u16 tx_r50_cal_val,
+			      u8 txg_calen_x)
+{
+	int bias = 0;
+	u16 reg, val;
+
+	if (phydev->drv->phy_id == MTK_GPHY_ID_MT7988)
+		bias = -1;
+
+	val = clamp_val(bias + tx_r50_cal_val, 0, 63);
+
+	switch (txg_calen_x) {
+	case PAIR_A:
+		reg = MTK_PHY_DA_TX_R50_PAIR_A;
+		break;
+	case PAIR_B:
+		reg = MTK_PHY_DA_TX_R50_PAIR_B;
+		break;
+	case PAIR_C:
+		reg = MTK_PHY_DA_TX_R50_PAIR_C;
+		break;
+	case PAIR_D:
+		reg = MTK_PHY_DA_TX_R50_PAIR_D;
+		break;
+	default:
+		return -EINVAL;
+	}
+
+	phy_write_mmd(phydev, MDIO_MMD_VEND1, reg, val | val << 8);
+
+	return 0;
+}
+
+static int tx_r50_cal_efuse(struct phy_device *phydev, u32 *buf,
+			    u8 txg_calen_x)
+{
+	u16 tx_r50_cal_val;
+
+	switch (txg_calen_x) {
+	case PAIR_A:
+		tx_r50_cal_val = EFS_DA_TX_R50_A(buf[1]);
+		break;
+	case PAIR_B:
+		tx_r50_cal_val = EFS_DA_TX_R50_B(buf[1]);
+		break;
+	case PAIR_C:
+		tx_r50_cal_val = EFS_DA_TX_R50_C(buf[2]);
+		break;
+	case PAIR_D:
+		tx_r50_cal_val = EFS_DA_TX_R50_D(buf[2]);
+		break;
+	default:
+		return -EINVAL;
+	}
+	tx_r50_fill_result(phydev, tx_r50_cal_val, txg_calen_x);
+
+	return 0;
+}
+
+static int tx_vcm_cal_sw(struct phy_device *phydev, u8 rg_txreserve_x)
+{
+	u8 lower_idx, upper_idx, txreserve_val;
+	u8 lower_ret, upper_ret;
+	int ret;
+
+	phy_set_bits_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_RG_ANA_CAL_RG0,
+			 MTK_PHY_RG_ANA_CALEN);
+	phy_clear_bits_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_RG_ANA_CAL_RG0,
+			   MTK_PHY_RG_CAL_CKINV);
+	phy_set_bits_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_RG_ANA_CAL_RG1,
+			 MTK_PHY_RG_TXVOS_CALEN);
+
+	switch (rg_txreserve_x) {
+	case PAIR_A:
+		phy_clear_bits_mmd(phydev, MDIO_MMD_VEND1,
+				   MTK_PHY_RG_DASN_DAC_IN0_A,
+				   MTK_PHY_DASN_DAC_IN0_A_MASK);
+		phy_clear_bits_mmd(phydev, MDIO_MMD_VEND1,
+				   MTK_PHY_RG_DASN_DAC_IN1_A,
+				   MTK_PHY_DASN_DAC_IN1_A_MASK);
+		phy_set_bits_mmd(phydev, MDIO_MMD_VEND1,
+				 MTK_PHY_RG_ANA_CAL_RG0,
+				 MTK_PHY_RG_ZCALEN_A);
+		break;
+	case PAIR_B:
+		phy_clear_bits_mmd(phydev, MDIO_MMD_VEND1,
+				   MTK_PHY_RG_DASN_DAC_IN0_B,
+				   MTK_PHY_DASN_DAC_IN0_B_MASK);
+		phy_clear_bits_mmd(phydev, MDIO_MMD_VEND1,
+				   MTK_PHY_RG_DASN_DAC_IN1_B,
+				   MTK_PHY_DASN_DAC_IN1_B_MASK);
+		phy_set_bits_mmd(phydev, MDIO_MMD_VEND1,
+				 MTK_PHY_RG_ANA_CAL_RG1,
+				 MTK_PHY_RG_ZCALEN_B);
+		break;
+	case PAIR_C:
+		phy_clear_bits_mmd(phydev, MDIO_MMD_VEND1,
+				   MTK_PHY_RG_DASN_DAC_IN0_C,
+				   MTK_PHY_DASN_DAC_IN0_C_MASK);
+		phy_clear_bits_mmd(phydev, MDIO_MMD_VEND1,
+				   MTK_PHY_RG_DASN_DAC_IN1_C,
+				   MTK_PHY_DASN_DAC_IN1_C_MASK);
+		phy_set_bits_mmd(phydev, MDIO_MMD_VEND1,
+				 MTK_PHY_RG_ANA_CAL_RG1,
+				 MTK_PHY_RG_ZCALEN_C);
+		break;
+	case PAIR_D:
+		phy_clear_bits_mmd(phydev, MDIO_MMD_VEND1,
+				   MTK_PHY_RG_DASN_DAC_IN0_D,
+				   MTK_PHY_DASN_DAC_IN0_D_MASK);
+		phy_clear_bits_mmd(phydev, MDIO_MMD_VEND1,
+				   MTK_PHY_RG_DASN_DAC_IN1_D,
+				   MTK_PHY_DASN_DAC_IN1_D_MASK);
+		phy_set_bits_mmd(phydev, MDIO_MMD_VEND1,
+				 MTK_PHY_RG_ANA_CAL_RG1,
+				 MTK_PHY_RG_ZCALEN_D);
+		break;
+	default:
+		ret = -EINVAL;
+		goto restore;
+	}
+
+	lower_idx = TXRESERVE_MIN;
+	upper_idx = TXRESERVE_MAX;
+
+	phydev_dbg(phydev, "Start TX-VCM SW cal.\n");
+	while ((upper_idx - lower_idx) > 1) {
+		txreserve_val = DIV_ROUND_CLOSEST(lower_idx + upper_idx, 2);
+		ret = cal_cycle(phydev, MDIO_MMD_VEND1, MTK_PHY_RXADC_CTRL_RG9,
+				MTK_PHY_DA_RX_PSBN_TBT_MASK |
+				MTK_PHY_DA_RX_PSBN_HBT_MASK |
+				MTK_PHY_DA_RX_PSBN_GBE_MASK |
+				MTK_PHY_DA_RX_PSBN_LP_MASK,
+				txreserve_val << 12 | txreserve_val << 8 |
+				txreserve_val << 4 | txreserve_val);
+		if (ret == 1) {
+			upper_idx = txreserve_val;
+			upper_ret = ret;
+		} else if (ret == 0) {
+			lower_idx = txreserve_val;
+			lower_ret = ret;
+		} else {
+			goto restore;
+		}
+	}
+
+	if (lower_idx == TXRESERVE_MIN) {
+		lower_ret = cal_cycle(phydev, MDIO_MMD_VEND1,
+				      MTK_PHY_RXADC_CTRL_RG9,
+				      MTK_PHY_DA_RX_PSBN_TBT_MASK |
+				      MTK_PHY_DA_RX_PSBN_HBT_MASK |
+				      MTK_PHY_DA_RX_PSBN_GBE_MASK |
+				      MTK_PHY_DA_RX_PSBN_LP_MASK,
+				      lower_idx << 12 | lower_idx << 8 |
+				      lower_idx << 4 | lower_idx);
+		ret = lower_ret;
+	} else if (upper_idx == TXRESERVE_MAX) {
+		upper_ret = cal_cycle(phydev, MDIO_MMD_VEND1,
+				      MTK_PHY_RXADC_CTRL_RG9,
+				      MTK_PHY_DA_RX_PSBN_TBT_MASK |
+				      MTK_PHY_DA_RX_PSBN_HBT_MASK |
+				      MTK_PHY_DA_RX_PSBN_GBE_MASK |
+				      MTK_PHY_DA_RX_PSBN_LP_MASK,
+				      upper_idx << 12 | upper_idx << 8 |
+				      upper_idx << 4 | upper_idx);
+		ret = upper_ret;
+	}
+	if (ret < 0)
+		goto restore;
+
+	/* We calibrate TX-VCM in different logic. Check upper index and then
+	 * lower index. If this calibration is valid, apply lower index's
+	 * result.
+	 */
+	ret = upper_ret - lower_ret;
+	if (ret == 1) {
+		ret = 0;
+		/* Make sure we use upper_idx in our calibration system */
+		cal_cycle(phydev, MDIO_MMD_VEND1, MTK_PHY_RXADC_CTRL_RG9,
+			  MTK_PHY_DA_RX_PSBN_TBT_MASK |
+			  MTK_PHY_DA_RX_PSBN_HBT_MASK |
+			  MTK_PHY_DA_RX_PSBN_GBE_MASK |
+			  MTK_PHY_DA_RX_PSBN_LP_MASK,
+			  upper_idx << 12 | upper_idx << 8 |
+			  upper_idx << 4 | upper_idx);
+		phydev_dbg(phydev, "TX-VCM SW cal result: 0x%x\n", upper_idx);
+	} else if (lower_idx == TXRESERVE_MIN && upper_ret == 1 &&
+		   lower_ret == 1) {
+		ret = 0;
+		cal_cycle(phydev, MDIO_MMD_VEND1, MTK_PHY_RXADC_CTRL_RG9,
+			  MTK_PHY_DA_RX_PSBN_TBT_MASK |
+			  MTK_PHY_DA_RX_PSBN_HBT_MASK |
+			  MTK_PHY_DA_RX_PSBN_GBE_MASK |
+			  MTK_PHY_DA_RX_PSBN_LP_MASK,
+			  lower_idx << 12 | lower_idx << 8 |
+			  lower_idx << 4 | lower_idx);
+		phydev_warn(phydev, "TX-VCM SW cal result at low margin 0x%x\n",
+			    lower_idx);
+	} else if (upper_idx == TXRESERVE_MAX && upper_ret == 0 &&
+		   lower_ret == 0) {
+		ret = 0;
+		phydev_warn(phydev,
+			    "TX-VCM SW cal result at high margin 0x%x\n",
+			    upper_idx);
+	} else {
+		ret = -EINVAL;
+	}
+
+restore:
+	phy_clear_bits_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_RG_ANA_CAL_RG0,
+			   MTK_PHY_RG_ANA_CALEN);
+	phy_clear_bits_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_RG_ANA_CAL_RG1,
+			   MTK_PHY_RG_TXVOS_CALEN);
+	phy_clear_bits_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_RG_ANA_CAL_RG0,
+			   MTK_PHY_RG_ZCALEN_A);
+	phy_clear_bits_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_RG_ANA_CAL_RG1,
+			   MTK_PHY_RG_ZCALEN_B | MTK_PHY_RG_ZCALEN_C |
+			   MTK_PHY_RG_ZCALEN_D);
+
+	return ret;
+}
+
+static void mt798x_phy_common_finetune(struct phy_device *phydev)
+{
+	phy_select_page(phydev, MTK_PHY_PAGE_EXTENDED_52B5);
+	/* SlvDSPreadyTime = 24, MasDSPreadyTime = 24 */
+	__phy_write(phydev, 0x11, 0xc71);
+	__phy_write(phydev, 0x12, 0xc);
+	__phy_write(phydev, 0x10, 0x8fae);
+
+	/* EnabRandUpdTrig = 1 */
+	__phy_write(phydev, 0x11, 0x2f00);
+	__phy_write(phydev, 0x12, 0xe);
+	__phy_write(phydev, 0x10, 0x8fb0);
+
+	/* NormMseLoThresh = 85 */
+	__phy_write(phydev, 0x11, 0x55a0);
+	__phy_write(phydev, 0x12, 0x0);
+	__phy_write(phydev, 0x10, 0x83aa);
+
+	/* FfeUpdGainForce = 1(Enable), FfeUpdGainForceVal = 4 */
+	__phy_write(phydev, 0x11, 0x240);
+	__phy_write(phydev, 0x12, 0x0);
+	__phy_write(phydev, 0x10, 0x9680);
+
+	/* TrFreeze = 0 (mt7988 default) */
+	__phy_write(phydev, 0x11, 0x0);
+	__phy_write(phydev, 0x12, 0x0);
+	__phy_write(phydev, 0x10, 0x9686);
+
+	/* SSTrKp100 = 5 */
+	/* SSTrKf100 = 6 */
+	/* SSTrKp1000Mas = 5 */
+	/* SSTrKf1000Mas = 6 */
+	/* SSTrKp1000Slv = 5 */
+	/* SSTrKf1000Slv = 6 */
+	__phy_write(phydev, 0x11, 0xbaef);
+	__phy_write(phydev, 0x12, 0x2e);
+	__phy_write(phydev, 0x10, 0x968c);
+	phy_restore_page(phydev, MTK_PHY_PAGE_STANDARD, 0);
+}
+
+static void mt7981_phy_finetune(struct phy_device *phydev)
+{
+	u16 val[8] = { 0x01ce, 0x01c1,
+		       0x020f, 0x0202,
+		       0x03d0, 0x03c0,
+		       0x0013, 0x0005 };
+	int i, k;
+
+	/* 100M eye finetune:
+	 * Keep middle level of TX MLT3 shapper as default.
+	 * Only change TX MLT3 overshoot level here.
+	 */
+	for (k = 0, i = 1; i < 12; i++) {
+		if (i % 3 == 0)
+			continue;
+		phy_write_mmd(phydev, MDIO_MMD_VEND1, i, val[k++]);
+	}
+
+	phy_select_page(phydev, MTK_PHY_PAGE_EXTENDED_52B5);
+	/* ResetSyncOffset = 6 */
+	__phy_write(phydev, 0x11, 0x600);
+	__phy_write(phydev, 0x12, 0x0);
+	__phy_write(phydev, 0x10, 0x8fc0);
+
+	/* VgaDecRate = 1 */
+	__phy_write(phydev, 0x11, 0x4c2a);
+	__phy_write(phydev, 0x12, 0x3e);
+	__phy_write(phydev, 0x10, 0x8fa4);
+
+	/* MrvlTrFix100Kp = 3, MrvlTrFix100Kf = 2,
+	 * MrvlTrFix1000Kp = 3, MrvlTrFix1000Kf = 2
+	 */
+	__phy_write(phydev, 0x11, 0xd10a);
+	__phy_write(phydev, 0x12, 0x34);
+	__phy_write(phydev, 0x10, 0x8f82);
+
+	/* VcoSlicerThreshBitsHigh */
+	__phy_write(phydev, 0x11, 0x5555);
+	__phy_write(phydev, 0x12, 0x55);
+	__phy_write(phydev, 0x10, 0x8ec0);
+	phy_restore_page(phydev, MTK_PHY_PAGE_STANDARD, 0);
+
+	/* TR_OPEN_LOOP_EN = 1, lpf_x_average = 9 */
+	phy_modify_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_RG_DEV1E_REG234,
+		       MTK_PHY_TR_OPEN_LOOP_EN_MASK |
+		       MTK_PHY_LPF_X_AVERAGE_MASK,
+		       BIT(0) | FIELD_PREP(MTK_PHY_LPF_X_AVERAGE_MASK, 0x9));
+
+	/* rg_tr_lpf_cnt_val = 512 */
+	phy_write_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_RG_LPF_CNT_VAL, 0x200);
+
+	/* IIR2 related */
+	phy_write_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_RG_LP_IIR2_K1_L, 0x82);
+	phy_write_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_RG_LP_IIR2_K1_U, 0x0);
+	phy_write_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_RG_LP_IIR2_K2_L, 0x103);
+	phy_write_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_RG_LP_IIR2_K2_U, 0x0);
+	phy_write_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_RG_LP_IIR2_K3_L, 0x82);
+	phy_write_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_RG_LP_IIR2_K3_U, 0x0);
+	phy_write_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_RG_LP_IIR2_K4_L, 0xd177);
+	phy_write_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_RG_LP_IIR2_K4_U, 0x3);
+	phy_write_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_RG_LP_IIR2_K5_L, 0x2c82);
+	phy_write_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_RG_LP_IIR2_K5_U, 0xe);
+
+	/* FFE peaking */
+	phy_modify_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_RG_DEV1E_REG27C,
+		       MTK_PHY_VGASTATE_FFE_THR_ST1_MASK, 0x1b << 8);
+	phy_modify_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_RG_DEV1E_REG27D,
+		       MTK_PHY_VGASTATE_FFE_THR_ST2_MASK, 0x1e);
+
+	/* Disable LDO pump */
+	phy_write_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_LDO_PUMP_EN_PAIRAB, 0x0);
+	phy_write_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_LDO_PUMP_EN_PAIRCD, 0x0);
+	/* Adjust LDO output voltage */
+	phy_write_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_LDO_OUTPUT_V, 0x2222);
+}
+
+static void mt7988_phy_finetune(struct phy_device *phydev)
+{
+	u16 val[12] = { 0x0187, 0x01cd, 0x01c8, 0x0182,
+			0x020d, 0x0206, 0x0384, 0x03d0,
+			0x03c6, 0x030a, 0x0011, 0x0005 };
+	int i;
+
+	/* Set default MLT3 shaper first */
+	for (i = 0; i < 12; i++)
+		phy_write_mmd(phydev, MDIO_MMD_VEND1, i, val[i]);
+
+	/* TCT finetune */
+	phy_write_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_RG_TX_FILTER, 0x5);
+
+	phy_select_page(phydev, MTK_PHY_PAGE_EXTENDED_52B5);
+	/* ResetSyncOffset = 5 */
+	__phy_write(phydev, 0x11, 0x500);
+	__phy_write(phydev, 0x12, 0x0);
+	__phy_write(phydev, 0x10, 0x8fc0);
+
+	/* VgaDecRate is 1 at default on mt7988 */
+
+	/* MrvlTrFix100Kp = 6, MrvlTrFix100Kf = 7,
+	 * MrvlTrFix1000Kp = 6, MrvlTrFix1000Kf = 7
+	 */
+	__phy_write(phydev, 0x11, 0xb90a);
+	__phy_write(phydev, 0x12, 0x6f);
+	__phy_write(phydev, 0x10, 0x8f82);
+
+	/* RemAckCntLimitCtrl = 1 */
+	__phy_write(phydev, 0x11, 0xfbba);
+	__phy_write(phydev, 0x12, 0xc3);
+	__phy_write(phydev, 0x10, 0x87f8);
+
+	phy_restore_page(phydev, MTK_PHY_PAGE_STANDARD, 0);
+
+	/* TR_OPEN_LOOP_EN = 1, lpf_x_average = 10 */
+	phy_modify_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_RG_DEV1E_REG234,
+		       MTK_PHY_TR_OPEN_LOOP_EN_MASK |
+		       MTK_PHY_LPF_X_AVERAGE_MASK,
+		       BIT(0) | FIELD_PREP(MTK_PHY_LPF_X_AVERAGE_MASK, 0xa));
+
+	/* rg_tr_lpf_cnt_val = 1023 */
+	phy_write_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_RG_LPF_CNT_VAL, 0x3ff);
+}
+
+static void mt798x_phy_eee(struct phy_device *phydev)
+{
+	phy_modify_mmd(phydev, MDIO_MMD_VEND1,
+		       MTK_PHY_RG_LPI_PCS_DSP_CTRL_REG120,
+		       MTK_PHY_LPI_SIG_EN_LO_THRESH1000_MASK |
+		       MTK_PHY_LPI_SIG_EN_HI_THRESH1000_MASK,
+		       FIELD_PREP(MTK_PHY_LPI_SIG_EN_LO_THRESH1000_MASK, 0x0) |
+		       FIELD_PREP(MTK_PHY_LPI_SIG_EN_HI_THRESH1000_MASK, 0x14));
+
+	phy_modify_mmd(phydev, MDIO_MMD_VEND1,
+		       MTK_PHY_RG_LPI_PCS_DSP_CTRL_REG122,
+		       MTK_PHY_LPI_NORM_MSE_HI_THRESH1000_MASK,
+		       FIELD_PREP(MTK_PHY_LPI_NORM_MSE_HI_THRESH1000_MASK,
+				  0xff));
+
+	phy_clear_bits_mmd(phydev, MDIO_MMD_VEND1,
+			   MTK_PHY_RG_TESTMUX_ADC_CTRL,
+			   MTK_PHY_RG_TXEN_DIG_MASK);
+
+	phy_set_bits_mmd(phydev, MDIO_MMD_VEND1,
+			 MTK_PHY_RG_DEV1E_REG19b, MTK_PHY_BYPASS_DSP_LPI_READY);
+
+	phy_clear_bits_mmd(phydev, MDIO_MMD_VEND1,
+			   MTK_PHY_RG_DEV1E_REG234, MTK_PHY_TR_LP_IIR_EEE_EN);
+
+	phy_modify_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_RG_DEV1E_REG238,
+		       MTK_PHY_LPI_SLV_SEND_TX_TIMER_MASK |
+		       MTK_PHY_LPI_SLV_SEND_TX_EN,
+		       FIELD_PREP(MTK_PHY_LPI_SLV_SEND_TX_TIMER_MASK, 0x120));
+
+	/* Keep MTK_PHY_LPI_SEND_LOC_TIMER as 375 */
+	phy_clear_bits_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_RG_DEV1E_REG239,
+			   MTK_PHY_LPI_TXPCS_LOC_RCV);
+
+	/* This also fixes some IoT issues, such as CH340 */
+	phy_modify_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_RG_DEV1E_REG2C7,
+		       MTK_PHY_MAX_GAIN_MASK | MTK_PHY_MIN_GAIN_MASK,
+		       FIELD_PREP(MTK_PHY_MAX_GAIN_MASK, 0x8) |
+		       FIELD_PREP(MTK_PHY_MIN_GAIN_MASK, 0x13));
+
+	phy_modify_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_RG_DEV1E_REG2D1,
+		       MTK_PHY_VCO_SLICER_THRESH_BITS_HIGH_EEE_MASK,
+		       FIELD_PREP(MTK_PHY_VCO_SLICER_THRESH_BITS_HIGH_EEE_MASK,
+				  0x33) |
+		       MTK_PHY_LPI_SKIP_SD_SLV_TR | MTK_PHY_LPI_TR_READY |
+		       MTK_PHY_LPI_VCO_EEE_STG0_EN);
+
+	phy_set_bits_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_RG_DEV1E_REG323,
+			 MTK_PHY_EEE_WAKE_MAS_INT_DC |
+			 MTK_PHY_EEE_WAKE_SLV_INT_DC);
+
+	phy_modify_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_RG_DEV1E_REG324,
+		       MTK_PHY_SMI_DETCNT_MAX_MASK,
+		       FIELD_PREP(MTK_PHY_SMI_DETCNT_MAX_MASK, 0x3f) |
+		       MTK_PHY_SMI_DET_MAX_EN);
+
+	phy_set_bits_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_RG_DEV1E_REG326,
+			 MTK_PHY_LPI_MODE_SD_ON | MTK_PHY_RESET_RANDUPD_CNT |
+			 MTK_PHY_TREC_UPDATE_ENAB_CLR |
+			 MTK_PHY_LPI_QUIT_WAIT_DFE_SIG_DET_OFF |
+			 MTK_PHY_TR_READY_SKIP_AFE_WAKEUP);
+
+	phy_select_page(phydev, MTK_PHY_PAGE_EXTENDED_52B5);
+	/* Regsigdet_sel_1000 = 0 */
+	__phy_write(phydev, 0x11, 0xb);
+	__phy_write(phydev, 0x12, 0x0);
+	__phy_write(phydev, 0x10, 0x9690);
+
+	/* REG_EEE_st2TrKf1000 = 2 */
+	__phy_write(phydev, 0x11, 0x114f);
+	__phy_write(phydev, 0x12, 0x2);
+	__phy_write(phydev, 0x10, 0x969a);
+
+	/* RegEEE_slv_wake_tr_timer_tar = 6, RegEEE_slv_remtx_timer_tar = 20 */
+	__phy_write(phydev, 0x11, 0x3028);
+	__phy_write(phydev, 0x12, 0x0);
+	__phy_write(phydev, 0x10, 0x969e);
+
+	/* RegEEE_slv_wake_int_timer_tar = 8 */
+	__phy_write(phydev, 0x11, 0x5010);
+	__phy_write(phydev, 0x12, 0x0);
+	__phy_write(phydev, 0x10, 0x96a0);
+
+	/* RegEEE_trfreeze_timer2 = 586 */
+	__phy_write(phydev, 0x11, 0x24a);
+	__phy_write(phydev, 0x12, 0x0);
+	__phy_write(phydev, 0x10, 0x96a8);
+
+	/* RegEEE100Stg1_tar = 16 */
+	__phy_write(phydev, 0x11, 0x3210);
+	__phy_write(phydev, 0x12, 0x0);
+	__phy_write(phydev, 0x10, 0x96b8);
+
+	/* REGEEE_wake_slv_tr_wait_dfesigdet_en = 0 */
+	__phy_write(phydev, 0x11, 0x1463);
+	__phy_write(phydev, 0x12, 0x0);
+	__phy_write(phydev, 0x10, 0x96ca);
+
+	/* DfeTailEnableVgaThresh1000 = 27 */
+	__phy_write(phydev, 0x11, 0x36);
+	__phy_write(phydev, 0x12, 0x0);
+	__phy_write(phydev, 0x10, 0x8f80);
+	phy_restore_page(phydev, MTK_PHY_PAGE_STANDARD, 0);
+
+	phy_select_page(phydev, MTK_PHY_PAGE_EXTENDED_3);
+	__phy_modify(phydev, MTK_PHY_LPI_REG_14,
+		     MTK_PHY_LPI_WAKE_TIMER_1000_MASK,
+		     FIELD_PREP(MTK_PHY_LPI_WAKE_TIMER_1000_MASK, 0x19c));
+
+	__phy_modify(phydev, MTK_PHY_LPI_REG_1c, MTK_PHY_SMI_DET_ON_THRESH_MASK,
+		     FIELD_PREP(MTK_PHY_SMI_DET_ON_THRESH_MASK, 0xc));
+	phy_restore_page(phydev, MTK_PHY_PAGE_STANDARD, 0);
+
+	phy_modify_mmd(phydev, MDIO_MMD_VEND1,
+		       MTK_PHY_RG_LPI_PCS_DSP_CTRL_REG122,
+		       MTK_PHY_LPI_NORM_MSE_HI_THRESH1000_MASK,
+		       FIELD_PREP(MTK_PHY_LPI_NORM_MSE_HI_THRESH1000_MASK,
+				  0xff));
+}
+
+static int cal_sw(struct phy_device *phydev, enum CAL_ITEM cal_item,
+		  u8 start_pair, u8 end_pair)
+{
+	u8 pair_n;
+	int ret;
+
+	for (pair_n = start_pair; pair_n <= end_pair; pair_n++) {
+		/* TX_OFFSET & TX_AMP have no SW calibration. */
+		switch (cal_item) {
+		case TX_VCM:
+			ret = tx_vcm_cal_sw(phydev, pair_n);
+			break;
+		default:
+			return -EINVAL;
+		}
+		if (ret)
+			return ret;
+	}
+	return 0;
+}
+
+static int cal_efuse(struct phy_device *phydev, enum CAL_ITEM cal_item,
+		     u8 start_pair, u8 end_pair, u32 *buf)
+{
+	u8 pair_n;
+	int ret;
+
+	for (pair_n = start_pair; pair_n <= end_pair; pair_n++) {
+		/* TX_VCM has no efuse calibration. */
+		switch (cal_item) {
+		case REXT:
+			ret = rext_cal_efuse(phydev, buf);
+			break;
+		case TX_OFFSET:
+			ret = tx_offset_cal_efuse(phydev, buf);
+			break;
+		case TX_AMP:
+			ret = tx_amp_cal_efuse(phydev, buf);
+			break;
+		case TX_R50:
+			ret = tx_r50_cal_efuse(phydev, buf, pair_n);
+			break;
+		default:
+			return -EINVAL;
+		}
+		if (ret)
+			return ret;
+	}
+
+	return 0;
+}
+
+static int start_cal(struct phy_device *phydev, enum CAL_ITEM cal_item,
+		     enum CAL_MODE cal_mode, u8 start_pair,
+		     u8 end_pair, u32 *buf)
+{
+	int ret;
+
+	switch (cal_mode) {
+	case EFUSE_M:
+		ret = cal_efuse(phydev, cal_item, start_pair,
+				end_pair, buf);
+		break;
+	case SW_M:
+		ret = cal_sw(phydev, cal_item, start_pair, end_pair);
+		break;
+	default:
+		return -EINVAL;
+	}
+
+	if (ret) {
+		phydev_err(phydev, "cal %d failed\n", cal_item);
+		return -EIO;
+	}
+
+	return 0;
+}
+
+static int mt798x_phy_calibration(struct phy_device *phydev)
+{
+	struct nvmem_cell *cell;
+	int ret = 0;
+	size_t len;
+	u32 *buf;
+
+	cell = nvmem_cell_get(&phydev->mdio.dev, "phy-cal-data");
+	if (IS_ERR(cell)) {
+		if (PTR_ERR(cell) == -EPROBE_DEFER)
+			return PTR_ERR(cell);
+		return 0;
+	}
+
+	buf = (u32 *)nvmem_cell_read(cell, &len);
+	if (IS_ERR(buf))
+		return PTR_ERR(buf);
+	nvmem_cell_put(cell);
+
+	if (!buf[0] || !buf[1] || !buf[2] || !buf[3] || len < 4 * sizeof(u32)) {
+		phydev_err(phydev, "invalid efuse data\n");
+		ret = -EINVAL;
+		goto out;
+	}
+
+	ret = start_cal(phydev, REXT, EFUSE_M, NO_PAIR, NO_PAIR, buf);
+	if (ret)
+		goto out;
+	ret = start_cal(phydev, TX_OFFSET, EFUSE_M, NO_PAIR, NO_PAIR, buf);
+	if (ret)
+		goto out;
+	ret = start_cal(phydev, TX_AMP, EFUSE_M, NO_PAIR, NO_PAIR, buf);
+	if (ret)
+		goto out;
+	ret = start_cal(phydev, TX_R50, EFUSE_M, PAIR_A, PAIR_D, buf);
+	if (ret)
+		goto out;
+	ret = start_cal(phydev, TX_VCM, SW_M, PAIR_A, PAIR_A, buf);
+	if (ret)
+		goto out;
+
+out:
+	kfree(buf);
+	return ret;
+}
+
+static int mt798x_phy_config_init(struct phy_device *phydev)
+{
+	switch (phydev->drv->phy_id) {
+	case MTK_GPHY_ID_MT7981:
+		mt7981_phy_finetune(phydev);
+		break;
+	case MTK_GPHY_ID_MT7988:
+		mt7988_phy_finetune(phydev);
+		break;
+	}
+
+	mt798x_phy_common_finetune(phydev);
+	mt798x_phy_eee(phydev);
+
+	return mt798x_phy_calibration(phydev);
+}
+
+static int mt798x_phy_hw_led_on_set(struct phy_device *phydev, u8 index,
+				    bool on)
+{
+	unsigned int bit_on = MTK_PHY_LED_STATE_FORCE_ON + (index ? 16 : 0);
+	struct mtk_socphy_priv *priv = phydev->priv;
+	bool changed;
+
+	if (on)
+		changed = !test_and_set_bit(bit_on, &priv->led_state);
+	else
+		changed = !!test_and_clear_bit(bit_on, &priv->led_state);
+
+	changed |= !!test_and_clear_bit(MTK_PHY_LED_STATE_NETDEV +
+					(index ? 16 : 0), &priv->led_state);
+	if (changed)
+		return phy_modify_mmd(phydev, MDIO_MMD_VEND2, index ?
+				      MTK_PHY_LED1_ON_CTRL :
+				      MTK_PHY_LED0_ON_CTRL,
+				      MTK_PHY_LED_ON_MASK,
+				      on ? MTK_PHY_LED_ON_FORCE_ON : 0);
+	else
+		return 0;
+}
+
+static int mt798x_phy_hw_led_blink_set(struct phy_device *phydev, u8 index,
+				       bool blinking)
+{
+	unsigned int bit_blink = MTK_PHY_LED_STATE_FORCE_BLINK +
+				 (index ? 16 : 0);
+	struct mtk_socphy_priv *priv = phydev->priv;
+	bool changed;
+
+	if (blinking)
+		changed = !test_and_set_bit(bit_blink, &priv->led_state);
+	else
+		changed = !!test_and_clear_bit(bit_blink, &priv->led_state);
+
+	changed |= !!test_bit(MTK_PHY_LED_STATE_NETDEV +
+			      (index ? 16 : 0), &priv->led_state);
+	if (changed)
+		return phy_write_mmd(phydev, MDIO_MMD_VEND2, index ?
+				     MTK_PHY_LED1_BLINK_CTRL :
+				     MTK_PHY_LED0_BLINK_CTRL,
+				     blinking ?
+				     MTK_PHY_LED_BLINK_FORCE_BLINK : 0);
+	else
+		return 0;
+}
+
+static int mt798x_phy_led_blink_set(struct phy_device *phydev, u8 index,
+				    unsigned long *delay_on,
+				    unsigned long *delay_off)
+{
+	bool blinking = false;
+	int err = 0;
+
+	if (index > 1)
+		return -EINVAL;
+
+	if (delay_on && delay_off && (*delay_on > 0) && (*delay_off > 0)) {
+		blinking = true;
+		*delay_on = 50;
+		*delay_off = 50;
+	}
+
+	err = mt798x_phy_hw_led_blink_set(phydev, index, blinking);
+	if (err)
+		return err;
+
+	return mt798x_phy_hw_led_on_set(phydev, index, false);
+}
+
+static int mt798x_phy_led_brightness_set(struct phy_device *phydev,
+					 u8 index, enum led_brightness value)
+{
+	int err;
+
+	err = mt798x_phy_hw_led_blink_set(phydev, index, false);
+	if (err)
+		return err;
+
+	return mt798x_phy_hw_led_on_set(phydev, index, (value != LED_OFF));
+}
+
+static const unsigned long supported_triggers =
+	BIT(TRIGGER_NETDEV_FULL_DUPLEX) |
+	BIT(TRIGGER_NETDEV_HALF_DUPLEX) |
+	BIT(TRIGGER_NETDEV_LINK)        |
+	BIT(TRIGGER_NETDEV_LINK_10)     |
+	BIT(TRIGGER_NETDEV_LINK_100)    |
+	BIT(TRIGGER_NETDEV_LINK_1000)   |
+	BIT(TRIGGER_NETDEV_RX)          |
+	BIT(TRIGGER_NETDEV_TX);
+
+static int mt798x_phy_led_hw_is_supported(struct phy_device *phydev, u8 index,
+					  unsigned long rules)
+{
+	if (index > 1)
+		return -EINVAL;
+
+	/* All combinations of the supported triggers are allowed */
+	if (rules & ~supported_triggers)
+		return -EOPNOTSUPP;
+
+	return 0;
+};
+
+static int mt798x_phy_led_hw_control_get(struct phy_device *phydev, u8 index,
+					 unsigned long *rules)
+{
+	unsigned int bit_blink = MTK_PHY_LED_STATE_FORCE_BLINK +
+				 (index ? 16 : 0);
+	unsigned int bit_netdev = MTK_PHY_LED_STATE_NETDEV + (index ? 16 : 0);
+	unsigned int bit_on = MTK_PHY_LED_STATE_FORCE_ON + (index ? 16 : 0);
+	struct mtk_socphy_priv *priv = phydev->priv;
+	int on, blink;
+
+	if (index > 1)
+		return -EINVAL;
+
+	on = phy_read_mmd(phydev, MDIO_MMD_VEND2,
+			  index ? MTK_PHY_LED1_ON_CTRL : MTK_PHY_LED0_ON_CTRL);
+
+	if (on < 0)
+		return -EIO;
+
+	blink = phy_read_mmd(phydev, MDIO_MMD_VEND2,
+			     index ? MTK_PHY_LED1_BLINK_CTRL :
+				     MTK_PHY_LED0_BLINK_CTRL);
+	if (blink < 0)
+		return -EIO;
+
+	if ((on & (MTK_PHY_LED_ON_LINK | MTK_PHY_LED_ON_FDX |
+		   MTK_PHY_LED_ON_HDX | MTK_PHY_LED_ON_LINKDOWN)) ||
+	    (blink & (MTK_PHY_LED_BLINK_RX | MTK_PHY_LED_BLINK_TX)))
+		set_bit(bit_netdev, &priv->led_state);
+	else
+		clear_bit(bit_netdev, &priv->led_state);
+
+	if (on & MTK_PHY_LED_ON_FORCE_ON)
+		set_bit(bit_on, &priv->led_state);
+	else
+		clear_bit(bit_on, &priv->led_state);
+
+	if (blink & MTK_PHY_LED_BLINK_FORCE_BLINK)
+		set_bit(bit_blink, &priv->led_state);
+	else
+		clear_bit(bit_blink, &priv->led_state);
+
+	if (!rules)
+		return 0;
+
+	if (on & MTK_PHY_LED_ON_LINK)
+		*rules |= BIT(TRIGGER_NETDEV_LINK);
+
+	if (on & MTK_PHY_LED_ON_LINK10)
+		*rules |= BIT(TRIGGER_NETDEV_LINK_10);
+
+	if (on & MTK_PHY_LED_ON_LINK100)
+		*rules |= BIT(TRIGGER_NETDEV_LINK_100);
+
+	if (on & MTK_PHY_LED_ON_LINK1000)
+		*rules |= BIT(TRIGGER_NETDEV_LINK_1000);
+
+	if (on & MTK_PHY_LED_ON_FDX)
+		*rules |= BIT(TRIGGER_NETDEV_FULL_DUPLEX);
+
+	if (on & MTK_PHY_LED_ON_HDX)
+		*rules |= BIT(TRIGGER_NETDEV_HALF_DUPLEX);
+
+	if (blink & MTK_PHY_LED_BLINK_RX)
+		*rules |= BIT(TRIGGER_NETDEV_RX);
+
+	if (blink & MTK_PHY_LED_BLINK_TX)
+		*rules |= BIT(TRIGGER_NETDEV_TX);
+
+	return 0;
+};
+
+static int mt798x_phy_led_hw_control_set(struct phy_device *phydev, u8 index,
+					 unsigned long rules)
+{
+	unsigned int bit_netdev = MTK_PHY_LED_STATE_NETDEV + (index ? 16 : 0);
+	struct mtk_socphy_priv *priv = phydev->priv;
+	u16 on = 0, blink = 0;
+	int ret;
+
+	if (index > 1)
+		return -EINVAL;
+
+	if (rules & BIT(TRIGGER_NETDEV_FULL_DUPLEX))
+		on |= MTK_PHY_LED_ON_FDX;
+
+	if (rules & BIT(TRIGGER_NETDEV_HALF_DUPLEX))
+		on |= MTK_PHY_LED_ON_HDX;
+
+	if (rules & (BIT(TRIGGER_NETDEV_LINK_10) | BIT(TRIGGER_NETDEV_LINK)))
+		on |= MTK_PHY_LED_ON_LINK10;
+
+	if (rules & (BIT(TRIGGER_NETDEV_LINK_100) | BIT(TRIGGER_NETDEV_LINK)))
+		on |= MTK_PHY_LED_ON_LINK100;
+
+	if (rules & (BIT(TRIGGER_NETDEV_LINK_1000) | BIT(TRIGGER_NETDEV_LINK)))
+		on |= MTK_PHY_LED_ON_LINK1000;
+
+	if (rules & BIT(TRIGGER_NETDEV_RX)) {
+		blink |= (on & MTK_PHY_LED_ON_LINK) ?
+			  (((on & MTK_PHY_LED_ON_LINK10) ?
+			    MTK_PHY_LED_BLINK_10RX : 0) |
+			   ((on & MTK_PHY_LED_ON_LINK100) ?
+			    MTK_PHY_LED_BLINK_100RX : 0) |
+			   ((on & MTK_PHY_LED_ON_LINK1000) ?
+			    MTK_PHY_LED_BLINK_1000RX : 0)) :
+			  MTK_PHY_LED_BLINK_RX;
+	}
+
+	if (rules & BIT(TRIGGER_NETDEV_TX)) {
+		blink |= (on & MTK_PHY_LED_ON_LINK) ?
+			  (((on & MTK_PHY_LED_ON_LINK10) ?
+			    MTK_PHY_LED_BLINK_10TX : 0) |
+			   ((on & MTK_PHY_LED_ON_LINK100) ?
+			    MTK_PHY_LED_BLINK_100TX : 0) |
+			   ((on & MTK_PHY_LED_ON_LINK1000) ?
+			    MTK_PHY_LED_BLINK_1000TX : 0)) :
+			  MTK_PHY_LED_BLINK_TX;
+	}
+
+	if (blink || on)
+		set_bit(bit_netdev, &priv->led_state);
+	else
+		clear_bit(bit_netdev, &priv->led_state);
+
+	ret = phy_modify_mmd(phydev, MDIO_MMD_VEND2, index ?
+				MTK_PHY_LED1_ON_CTRL :
+				MTK_PHY_LED0_ON_CTRL,
+			     MTK_PHY_LED_ON_FDX     |
+			     MTK_PHY_LED_ON_HDX     |
+			     MTK_PHY_LED_ON_LINK,
+			     on);
+
+	if (ret)
+		return ret;
+
+	return phy_write_mmd(phydev, MDIO_MMD_VEND2, index ?
+				MTK_PHY_LED1_BLINK_CTRL :
+				MTK_PHY_LED0_BLINK_CTRL, blink);
+};
+
+static bool mt7988_phy_led_get_polarity(struct phy_device *phydev, int led_num)
+{
+	struct mtk_socphy_shared *priv = phydev->shared->priv;
+	u32 polarities;
+
+	if (led_num == 0)
+		polarities = ~(priv->boottrap);
+	else
+		polarities = MTK_PHY_LED1_DEFAULT_POLARITIES;
+
+	if (polarities & BIT(phydev->mdio.addr))
+		return true;
+
+	return false;
+}
+
+static int mt7988_phy_fix_leds_polarities(struct phy_device *phydev)
+{
+	struct pinctrl *pinctrl;
+	int index;
+
+	/* Setup LED polarity according to bootstrap use of LED pins */
+	for (index = 0; index < 2; ++index)
+		phy_modify_mmd(phydev, MDIO_MMD_VEND2, index ?
+				MTK_PHY_LED1_ON_CTRL : MTK_PHY_LED0_ON_CTRL,
+			       MTK_PHY_LED_ON_POLARITY,
+			       mt7988_phy_led_get_polarity(phydev, index) ?
+				MTK_PHY_LED_ON_POLARITY : 0);
+
+	/* Only now setup pinctrl to avoid bogus blinking */
+	pinctrl = devm_pinctrl_get_select(&phydev->mdio.dev, "gbe-led");
+	if (IS_ERR(pinctrl))
+		dev_err(&phydev->mdio.bus->dev,
+			"Failed to setup PHY LED pinctrl\n");
+
+	return 0;
+}
+
+static int mt7988_phy_probe_shared(struct phy_device *phydev)
+{
+	struct device_node *np = dev_of_node(&phydev->mdio.bus->dev);
+	struct mtk_socphy_shared *shared = phydev->shared->priv;
+	struct regmap *regmap;
+	u32 reg;
+	int ret;
+
+	/* The LED0 of the 4 PHYs in MT7988 are wired to SoC pins LED_A, LED_B,
+	 * LED_C and LED_D respectively. At the same time those pins are used to
+	 * bootstrap configuration of the reference clock source (LED_A),
+	 * DRAM DDRx16b x2/x1 (LED_B) and boot device (LED_C, LED_D).
+	 * In practice this is done using a LED and a resistor pulling the pin
+	 * either to GND or to VIO.
+	 * The detected value at boot time is accessible at run-time using the
+	 * TPBANK0 register located in the gpio base of the pinctrl, in order
+	 * to read it here it needs to be referenced by a phandle called
+	 * 'mediatek,pio' in the MDIO bus hosting the PHY.
+	 * The 4 bits in TPBANK0 are kept as package shared data and are used to
+	 * set LED polarity for each of the LED0.
+	 */
+	regmap = syscon_regmap_lookup_by_phandle(np, "mediatek,pio");
+	if (IS_ERR(regmap))
+		return PTR_ERR(regmap);
+
+	ret = regmap_read(regmap, RG_GPIO_MISC_TPBANK0, &reg);
+	if (ret)
+		return ret;
+
+	shared->boottrap = FIELD_GET(RG_GPIO_MISC_TPBANK0_BOOTMODE, reg);
+
+	return 0;
+}
+
+static void mt798x_phy_leds_state_init(struct phy_device *phydev)
+{
+	int i;
+
+	for (i = 0; i < 2; ++i)
+		mt798x_phy_led_hw_control_get(phydev, i, NULL);
+}
+
+static int mt7988_phy_probe(struct phy_device *phydev)
+{
+	struct mtk_socphy_shared *shared;
+	struct mtk_socphy_priv *priv;
+	int err;
+
+	if (phydev->mdio.addr > 3)
+		return -EINVAL;
+
+	err = devm_phy_package_join(&phydev->mdio.dev, phydev, 0,
+				    sizeof(struct mtk_socphy_shared));
+	if (err)
+		return err;
+
+	if (phy_package_probe_once(phydev)) {
+		err = mt7988_phy_probe_shared(phydev);
+		if (err)
+			return err;
+	}
+
+	shared = phydev->shared->priv;
+	priv = &shared->priv[phydev->mdio.addr];
+
+	phydev->priv = priv;
+
+	mt798x_phy_leds_state_init(phydev);
+
+	err = mt7988_phy_fix_leds_polarities(phydev);
+	if (err)
+		return err;
+
+	/* Disable TX power saving at probing to:
+	 * 1. Meet common mode compliance test criteria
+	 * 2. Make sure that TX-VCM calibration works fine
+	 */
+	phy_modify_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_RXADC_CTRL_RG7,
+		       MTK_PHY_DA_AD_BUF_BIAS_LP_MASK, 0x3 << 8);
+
+	return mt798x_phy_calibration(phydev);
+}
+
+static int mt7981_phy_probe(struct phy_device *phydev)
+{
+	struct mtk_socphy_priv *priv;
+
+	priv = devm_kzalloc(&phydev->mdio.dev, sizeof(struct mtk_socphy_priv),
+			    GFP_KERNEL);
+	if (!priv)
+		return -ENOMEM;
+
+	phydev->priv = priv;
+
+	mt798x_phy_leds_state_init(phydev);
+
+	return mt798x_phy_calibration(phydev);
+}
+
+static struct phy_driver mtk_socphy_driver[] = {
+	{
+		PHY_ID_MATCH_EXACT(MTK_GPHY_ID_MT7981),
+		.name		= "MediaTek MT7981 PHY",
+		.config_init	= mt798x_phy_config_init,
+		.config_intr	= genphy_no_config_intr,
+		.handle_interrupt = genphy_handle_interrupt_no_ack,
+		.probe		= mt7981_phy_probe,
+		.suspend	= genphy_suspend,
+		.resume		= genphy_resume,
+		.read_page	= mtk_socphy_read_page,
+		.write_page	= mtk_socphy_write_page,
+		.led_blink_set	= mt798x_phy_led_blink_set,
+		.led_brightness_set = mt798x_phy_led_brightness_set,
+		.led_hw_is_supported = mt798x_phy_led_hw_is_supported,
+		.led_hw_control_set = mt798x_phy_led_hw_control_set,
+		.led_hw_control_get = mt798x_phy_led_hw_control_get,
+	},
+	{
+		PHY_ID_MATCH_EXACT(MTK_GPHY_ID_MT7988),
+		.name		= "MediaTek MT7988 PHY",
+		.config_init	= mt798x_phy_config_init,
+		.config_intr	= genphy_no_config_intr,
+		.handle_interrupt = genphy_handle_interrupt_no_ack,
+		.probe		= mt7988_phy_probe,
+		.suspend	= genphy_suspend,
+		.resume		= genphy_resume,
+		.read_page	= mtk_socphy_read_page,
+		.write_page	= mtk_socphy_write_page,
+		.led_blink_set	= mt798x_phy_led_blink_set,
+		.led_brightness_set = mt798x_phy_led_brightness_set,
+		.led_hw_is_supported = mt798x_phy_led_hw_is_supported,
+		.led_hw_control_set = mt798x_phy_led_hw_control_set,
+		.led_hw_control_get = mt798x_phy_led_hw_control_get,
+	},
+};
+
+module_phy_driver(mtk_socphy_driver);
+
+static struct mdio_device_id __maybe_unused mtk_socphy_tbl[] = {
+	{ PHY_ID_MATCH_EXACT(MTK_GPHY_ID_MT7981) },
+	{ PHY_ID_MATCH_EXACT(MTK_GPHY_ID_MT7988) },
+	{ }
+};
+
+MODULE_DESCRIPTION("MediaTek SoC Gigabit Ethernet PHY driver");
+MODULE_AUTHOR("Daniel Golle <daniel@makrotopia.org>");
+MODULE_AUTHOR("SkyLake Huang <SkyLake.Huang@mediatek.com>");
+MODULE_LICENSE("GPL");
+
+MODULE_DEVICE_TABLE(mdio, mtk_socphy_tbl);
--- /dev/null
+++ b/drivers/net/phy/mediatek/mtk-ge.c
@@ -0,0 +1,114 @@
+// SPDX-License-Identifier: GPL-2.0+
+#include <linux/bitfield.h>
+#include <linux/module.h>
+#include <linux/phy.h>
+
+#define MTK_EXT_PAGE_ACCESS		0x1f
+#define MTK_PHY_PAGE_STANDARD		0x0000
+#define MTK_PHY_PAGE_EXTENDED		0x0001
+#define MTK_PHY_PAGE_EXTENDED_2		0x0002
+#define MTK_PHY_PAGE_EXTENDED_3		0x0003
+#define MTK_PHY_PAGE_EXTENDED_2A30	0x2a30
+#define MTK_PHY_PAGE_EXTENDED_52B5	0x52b5
+
+static int mtk_gephy_read_page(struct phy_device *phydev)
+{
+	return __phy_read(phydev, MTK_EXT_PAGE_ACCESS);
+}
+
+static int mtk_gephy_write_page(struct phy_device *phydev, int page)
+{
+	return __phy_write(phydev, MTK_EXT_PAGE_ACCESS, page);
+}
+
+static void mtk_gephy_config_init(struct phy_device *phydev)
+{
+	/* Disable EEE */
+	phy_write_mmd(phydev, MDIO_MMD_AN, MDIO_AN_EEE_ADV, 0);
+
+	/* Enable HW auto downshift */
+	phy_modify_paged(phydev, MTK_PHY_PAGE_EXTENDED, 0x14, 0, BIT(4));
+
+	/* Increase SlvDPSready time */
+	phy_select_page(phydev, MTK_PHY_PAGE_EXTENDED_52B5);
+	__phy_write(phydev, 0x10, 0xafae);
+	__phy_write(phydev, 0x12, 0x2f);
+	__phy_write(phydev, 0x10, 0x8fae);
+	phy_restore_page(phydev, MTK_PHY_PAGE_STANDARD, 0);
+
+	/* Adjust 100_mse_threshold */
+	phy_write_mmd(phydev, MDIO_MMD_VEND1, 0x123, 0xffff);
+
+	/* Disable mcc */
+	phy_write_mmd(phydev, MDIO_MMD_VEND1, 0xa6, 0x300);
+}
+
+static int mt7530_phy_config_init(struct phy_device *phydev)
+{
+	mtk_gephy_config_init(phydev);
+
+	/* Increase post_update_timer */
+	phy_write_paged(phydev, MTK_PHY_PAGE_EXTENDED_3, 0x11, 0x4b);
+
+	return 0;
+}
+
+static int mt7531_phy_config_init(struct phy_device *phydev)
+{
+	mtk_gephy_config_init(phydev);
+
+	/* PHY link down power saving enable */
+	phy_set_bits(phydev, 0x17, BIT(4));
+	phy_clear_bits_mmd(phydev, MDIO_MMD_VEND1, 0xc6, 0x300);
+
+	/* Set TX Pair delay selection */
+	phy_write_mmd(phydev, MDIO_MMD_VEND1, 0x13, 0x404);
+	phy_write_mmd(phydev, MDIO_MMD_VEND1, 0x14, 0x404);
+
+	return 0;
+}
+
+static struct phy_driver mtk_gephy_driver[] = {
+	{
+		PHY_ID_MATCH_EXACT(0x03a29412),
+		.name		= "MediaTek MT7530 PHY",
+		.config_init	= mt7530_phy_config_init,
+		/* Interrupts are handled by the switch, not the PHY
+		 * itself.
+		 */
+		.config_intr	= genphy_no_config_intr,
+		.handle_interrupt = genphy_handle_interrupt_no_ack,
+		.suspend	= genphy_suspend,
+		.resume		= genphy_resume,
+		.read_page	= mtk_gephy_read_page,
+		.write_page	= mtk_gephy_write_page,
+	},
+	{
+		PHY_ID_MATCH_EXACT(0x03a29441),
+		.name		= "MediaTek MT7531 PHY",
+		.config_init	= mt7531_phy_config_init,
+		/* Interrupts are handled by the switch, not the PHY
+		 * itself.
+		 */
+		.config_intr	= genphy_no_config_intr,
+		.handle_interrupt = genphy_handle_interrupt_no_ack,
+		.suspend	= genphy_suspend,
+		.resume		= genphy_resume,
+		.read_page	= mtk_gephy_read_page,
+		.write_page	= mtk_gephy_write_page,
+	},
+};
+
+module_phy_driver(mtk_gephy_driver);
+
+static struct mdio_device_id __maybe_unused mtk_gephy_tbl[] = {
+	{ PHY_ID_MATCH_EXACT(0x03a29441) },
+	{ PHY_ID_MATCH_EXACT(0x03a29412) },
+	{ }
+};
+
+MODULE_DESCRIPTION("MediaTek Gigabit Ethernet PHY driver");
+MODULE_AUTHOR("DENG, Qingfang <dqfext@gmail.com>");
+MODULE_LICENSE("GPL");
+
+MODULE_DEVICE_TABLE(mdio, mtk_gephy_tbl);
