// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

/dts-v1/;

#include "ipq5018.dtsi"
#include "ipq5018-ess.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>
#include <dt-bindings/leds/common.h>

/ {
	model = "I-O DATA WN-DAX3000GR";
	compatible = "iodata,wn-dax3000gr", "qcom,ipq5018";

	aliases {
		serial0 = &blsp1_uart1;
		led-boot = &led_status_green;
		led-failsafe = &led_status_red;
		led-upgrade = &led_status_green;
		label-mac-device = <&dp1>;
	};

	chosen {
		bootargs-append = " root=/dev/ubiblock0_1 coherent_pool=2M";
		stdout-path = "serial0:115200n8";
	};

	keys {
		compatible = "gpio-keys";
		pinctrl-0 = <&button_pins>;
		pinctrl-names = "default";

		button-reset {
			label = "reset";
			gpios = <&tlmm 22 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
		};

		switch-led-on {
			label = "led-on";
			gpios = <&tlmm 23 GPIO_ACTIVE_LOW>;
			linux,code = <BTN_0>;
			linux,input-type = <EV_SW>;
		};

		switch-repeater {
			label = "repeater";
			gpios = <&tlmm 31 GPIO_ACTIVE_LOW>;
			linux,code = <BTN_1>;
			linux,input-type = <EV_SW>;
		};

		switch-ap {
			label = "ap";
			gpios = <&tlmm 32 GPIO_ACTIVE_LOW>;
			linux,code = <BTN_2>;
			linux,input-type = <EV_SW>;
		};

		button-wps {
			label = "wps";
			gpios = <&tlmm 38 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_WPS_BUTTON>;
		};
	};

	leds {
		compatible = "gpio-leds";
		pinctrl-0 = <&led_pins>;
		pinctrl-names = "default";

		led-0 {
			gpios = <&tlmm 12 GPIO_ACTIVE_HIGH>;
			color = <LED_COLOR_ID_GREEN>;
			function = LED_FUNCTION_WPS;
		};

		led_status_green: led-1 {
			gpios = <&tlmm 13 GPIO_ACTIVE_HIGH>;
			color = <LED_COLOR_ID_GREEN>;
			function = LED_FUNCTION_STATUS;
		};

		led_status_red: led-2 {
			gpios = <&tlmm 16 GPIO_ACTIVE_HIGH>;
			color = <LED_COLOR_ID_ORANGE>;
			function = LED_FUNCTION_STATUS;
		};

		led-3 {
			gpios = <&tlmm 24 GPIO_ACTIVE_HIGH>;
			color = <LED_COLOR_ID_GREEN>;
			function = LED_FUNCTION_WAN_ONLINE;
		};

		led-4 {
			gpios = <&tlmm 25 GPIO_ACTIVE_HIGH>;
			color = <LED_COLOR_ID_GREEN>;
			function = "router";
		};

		led-5 {
			gpios = <&tlmm 26 GPIO_ACTIVE_HIGH>;
			color = <LED_COLOR_ID_GREEN>;
			function = LED_FUNCTION_POWER;
			default-state = "on";
		};

		led-6 {
			gpios = <&tlmm 28 GPIO_ACTIVE_HIGH>;
			color = <LED_COLOR_ID_GREEN>;
			function = LED_FUNCTION_WAN;
		};
	};

	reserved-memory {
		q6_mem_regions: q6_mem_regions@4b000000 {
			no-map;
			reg = <0x0 0x4b000000 0x0 0x3000000>;
		};
	};
};

&sleep_clk {
	clock-frequency = <32000>;
};

&xo_board_clk {
	clock-div = <4>;
	clock-mult = <1>;
};

&blsp1_uart1 {
	status = "okay";

	pinctrl-0 = <&serial_0_pins>;
	pinctrl-names = "default";
};

&crypto {
	status = "okay";
};

&cryptobam {
	status = "okay";
};

&prng {
	status = "okay";
};

&qfprom {
	status = "okay";
};

&qpic_bam {
	status = "okay";
};

&qpic_nand {
	pinctrl-0 = <&qpic_pins>;
	pinctrl-names = "default";
	status = "okay";

	flash@0 {
		compatible = "spi-nand";
		reg = <0>;
		#address-cells = <1>;
		#size-cells = <1>;

		nand-ecc-engine = <&qpic_nand>;

		/* strength=8 breaks NAND I/O, use 4 instead */
		nand-ecc-strength = <4>;
		nand-ecc-step-size = <512>;
		nand-bus-width = <8>;

		partitions {
			compatible = "qcom,smem-part";

			partition-0-appsblenv {
				compatible = "fixed-partitions";
				label = "0:appsblenv";
				#address-cells = <1>;
				#size-cells = <1>;

				partition@0 {
					label = "env-data";
					reg = <0x0 0x40000>;

					nvmem-layout {
						compatible = "u-boot,env";

						macaddr_appsblenv_ethaddr: ethaddr {
							compatible = "mac-base";
							#nvmem-cell-cells = <1>;
						};
					};
				};
			};
		};
	};
};

&switch {
	status = "okay";

	switch_mac_mode = <MAC_MODE_SGMII_CHANNEL0>;

	qcom,port_phyinfo {
		port@0 {
			port_id = <1>;
			mdiobus = <&mdio0>;
			phy_address = <7>;
		};

		port@1 {
			port_id = <2>;
			forced-speed = <1000>;
			forced-duplex = <1>;
		};
	};
};

&dp1 {
	status = "okay";

	label = "wan";
	nvmem-cells = <&macaddr_appsblenv_ethaddr 2>;
	nvmem-cell-names = "mac-address";
};

&dp2 {
	status = "okay";

	nvmem-cells = <&macaddr_appsblenv_ethaddr 0>;
	nvmem-cell-names = "mac-address";

	fixed-link {
		speed = <1000>;
		full-duplex;
	};
};

&mdio0 {
	status = "okay";
};

&mdio1 {
	status = "okay";

	pinctrl-0 = <&mdio1_pins>, <&switch_reset_pins>;
	pinctrl-names = "default";
	reset-gpios = <&tlmm 39 GPIO_ACTIVE_LOW>;

	qca8337_0: ethernet-phy@0 {
		reg = <0>;
	};

	qca8337_1: ethernet-phy@1 {
		reg = <1>;
	};

	qca8337_2: ethernet-phy@2 {
		reg = <2>;
	};

	qca8337_3: ethernet-phy@3 {
		reg = <3>;
	};

	ethernet-switch@18 {
		compatible = "qca,qca8337";
		reg = <0x18>;
		#address-cells = <1>;
		#size-cells = <0>;

		ports {
			#address-cells = <1>;
			#size-cells = <0>;

			port@1 {
				reg = <1>;
				label = "lan1";
				phy-handle = <&qca8337_0>;
			};

			port@2 {
				reg = <2>;
				label = "lan2";
				phy-handle = <&qca8337_1>;
			};

			port@3 {
				reg = <3>;
				label = "lan3";
				phy-handle = <&qca8337_2>;
			};

			port@4 {
				reg = <4>;
				label = "lan4";
				phy-handle = <&qca8337_3>;
			};

			port@6 {
				reg = <6>;
				phy-mode = "sgmii";
				ethernet = <&dp2>;
				qca,sgmii-enable-pll;

				fixed-link {
					speed = <1000>;
					full-duplex;
				};
			};
		};
	};
};

&tlmm {
	button_pins: button-state {
		key-pullup-pins {
			pins = "gpio22", "gpio23", "gpio38";
			function = "gpio";
			drive-strength = <8>;
			bias-pull-up;
		};

		key-pulldown-pins {
			pins = "gpio31", "gpio32";
			function = "gpio";
			drive-strength = <8>;
			bias-pull-down;
		};
	};

	led_pins: led-state {
		pins = "gpio12", "gpio13", "gpio16", "gpio24",
		       "gpio25", "gpio26", "gpio28";
		function = "gpio";
		drive-strength = <8>;
		bias-pull-down;
	};

	mdio1_pins: mdio-state {
		mdc-pins {
			pins = "gpio36";
			function = "mdc";
			drive-strength = <8>;
			bias-pull-up;
		};

		mdio-pins {
			pins = "gpio37";
			function = "mdio";
			drive-strength = <8>;
			bias-pull-up;
		};
	};

	qpic_pins: qpic-state {
		clock-pins {
			pins = "gpio9";
			function = "qspi_clk";
			drive-strength = <8>;
			bias-disable;
		};

		cs-pins {
			pins = "gpio8";
			function = "qspi_cs";
			drive-strength = <8>;
			bias-disable;
		};

		data-pins {
			pins = "gpio4", "gpio5", "gpio6", "gpio7";
			function = "qspi_data";
			drive-strength = <8>;
			bias-disable;
		};
	};

	serial_0_pins: uart0-state {
		pins = "gpio20", "gpio21";
		function = "blsp0_uart0";
		bias-disable;
	};

	switch_reset_pins: switch-reset-state {
		pins = "gpio39";
		function = "gpio";
		drive-strength = <8>;
		bias-pull-down;
	};
};

&q6v5_wcss {
	status = "okay";

	memory-region = <&q6_mem_regions>;
	firmware-name = "ath11k/IPQ5018/hw1.0/q6_fw.mdt",
			"ath11k/IPQ5018/hw1.0/m3_fw.mdt",
			"ath11k/QCN6122/hw1.0/m3_fw.mdt";

	boot-args = <0x2 4 2 18 0 0>; /* pcie:1, len:4, updid:2, reset:gpio18 */

	q6_wcss_pd1: pd-1 {
		firmware-name = "ath11k/IPQ5018/hw1.0/q6_fw.mdt";

		resets =
			<&gcc GCC_WCSSAON_RESET>,
			<&gcc GCC_WCSS_BCR>,
			<&gcc GCC_CE_BCR>;
		reset-names =
			"wcss_aon_reset",
			"wcss_reset",
			"ce_reset";

		clocks =
			<&gcc GCC_WCSS_AHB_S_CLK>,
			<&gcc GCC_WCSS_ACMT_CLK>,
			<&gcc GCC_WCSS_AXI_M_CLK>;
		clock-names =
			"gcc_wcss_ahb_s_clk",
			"gcc_wcss_acmt_clk",
			"gcc_wcss_axi_m_clk";

		interrupts-extended =
			<&wcss_smp2p_in 8 IRQ_TYPE_NONE>,
			<&wcss_smp2p_in 9 IRQ_TYPE_NONE>,
			<&wcss_smp2p_in 12 IRQ_TYPE_NONE>,
			<&wcss_smp2p_in 11 IRQ_TYPE_NONE>;
		interrupt-names =
			"fatal",
			"ready",
			"spawn-ack",
			"stop-ack";

		qcom,smem-states =
			<&wcss_smp2p_out 8>,
			<&wcss_smp2p_out 9>,
			<&wcss_smp2p_out 10>;
		qcom,smem-state-names =
			"shutdown",
			"stop",
			"spawn";
	};

	q6_wcss_pd2: pd-2 {
		firmware-name = "ath11k/IPQ5018/hw1.0/q6_fw.mdt";

		interrupts-extended =
			<&wcss_smp2p_in 16 IRQ_TYPE_NONE>,
			<&wcss_smp2p_in 17 IRQ_TYPE_NONE>,
			<&wcss_smp2p_in 20 IRQ_TYPE_NONE>,
			<&wcss_smp2p_in 19 IRQ_TYPE_NONE>;
		interrupt-names =
			"fatal",
			"ready",
			"spawn-ack",
			"stop-ack";

		qcom,smem-states =
			<&wcss_smp2p_out 16>,
			<&wcss_smp2p_out 17>,
			<&wcss_smp2p_out 18>;
		qcom,smem-state-names =
			"shutdown",
			"stop",
			"spawn";
	};
};

&wifi0 {
	status = "okay";

	qcom,rproc = <&q6_wcss_pd1>;
	qcom,ath11k-calibration-variant = "IODATA-WN-DAX3000GR";
	qcom,ath11k-fw-memory-mode = <2>;
	qcom,bdf-addr = <0x4c400000>;

	ieee80211-freq-limit = <2400000 2483000>;
};

&wifi1 {
	status = "okay";

	qcom,rproc = <&q6_wcss_pd2>;
	qcom,userpd-subsys-name = "q6v5_wcss_userpd2";
	qcom,ath11k-calibration-variant = "IODATA-WN-DAX3000GR";
	qcom,ath11k-fw-memory-mode = <2>;
	qcom,bdf-addr = <0x4d100000>;
	qcom,m3-dump-addr = <0x4df00000>;

	ieee80211-freq-limit = <5150000 5730000>;
};
