// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

#include "ar7240.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>
#include <dt-bindings/leds/common.h>

/ {
	aliases {
		led-boot = &led_system;
		led-failsafe = &led_system;
		led-running = &led_system;
		led-upgrade = &led_system;
		label-mac-device = &ath9k;
	};

	keys {
		compatible = "gpio-keys";

		reset {
			label = "reset";
			linux,code = <KEY_RESTART>;
			gpios = <&gpio 11 GPIO_ACTIVE_LOW>;
			debounce-interval = <60>;
		};

		wps {
			label = "wps";
			linux,code = <KEY_WPS_BUTTON>;
			gpios = <&gpio 12 GPIO_ACTIVE_LOW>;
			debounce-interval = <60>;
		};
	};

	leds: leds {
		compatible = "gpio-leds";

		pinctrl-names = "default";
		pinctrl-0 = <&pinmux_switch_led_pins>;

		led_system: system {
			label = "green:system";
			gpios = <&gpio 1 GPIO_ACTIVE_LOW>;
		};

		qss {
			label = "green:qss";
			gpios = <&gpio 0 GPIO_ACTIVE_LOW>;
		};
	};

	ath9k-leds {
		compatible = "gpio-leds";

		wlan {
			function = LED_FUNCTION_WLAN;
			color = <LED_COLOR_ID_GREEN>;
			gpios = <&ath9k 1 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "phy0tpt";
		};
	};
};

&spi {
	status = "okay";

	flash@0 {
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <25000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			uboot: partition@0 {
				reg = <0x0 0x20000>;
				label = "u-boot";
				read-only;

				nvmem-layout {
					compatible = "fixed-layout";
					#address-cells = <1>;
					#size-cells = <1>;

					macaddr_uboot_1fc00: macaddr@1fc00 {
						compatible = "mac-base";
						reg = <0x1fc00 0x6>;
						#nvmem-cell-cells = <1>;
					};
				};
			};

			partition@20000 {
				compatible = "tplink,firmware";
				reg = <0x20000 0x3d0000>;
				label = "firmware";
			};

			partition@3f0000 {
				reg = <0x3f0000 0x10000>;
				label = "art";
				read-only;

				nvmem-layout {
					compatible = "fixed-layout";
					#address-cells = <1>;
					#size-cells = <1>;

					calibration_art_1000: calibration@1000 {
					};
				};
			};
		};
	};
};

&eth1 {
	status = "okay";
};

&pcie {
	status = "okay";

	ath9k: wifi@0,0 {
		reg = <0x0000 0 0 0 0>;
		nvmem-cells = <&macaddr_uboot_1fc00 0>, <&calibration_art_1000>;
		nvmem-cell-names = "mac-address", "calibration";
		#gpio-cells = <2>;
		gpio-controller;
	};
};

&pinmux {
	pinmux_switch_led_pins: switch_led_pins {
		pinctrl-single,bits = <0x0 0x0 0xf8>;
	};
};
