From b544223bec9f710256543eadc1b8b8344f80d665 Mon Sep 17 00:00:00 2001
From: "SkyLake.Huang" <skylake.huang@mediatek.com>
Date: Thu, 17 Oct 2024 11:22:11 +0800
Subject: [PATCH 1/3] net: phy: mediatek-ge-soc: Fix coding style

This patch fixes spelling errors, re-arrange vars with
reverse Xmas tree and remove unnecessary parens in
mediatek-ge-soc.c.

Signed-off-by: SkyLake.Huang <skylake.huang@mediatek.com>
Reviewed-by: Simon Horman <horms@kernel.org>
Signed-off-by: Andrew Lunn <andrew@lunn.ch>
---
 drivers/net/phy/mediatek-ge-soc.c | 36 ++++++++++++++++---------------
 1 file changed, 19 insertions(+), 17 deletions(-)

--- a/drivers/net/phy/mediatek-ge-soc.c
+++ b/drivers/net/phy/mediatek-ge-soc.c
@@ -408,16 +408,17 @@ static int tx_offset_cal_efuse(struct ph
 
 static int tx_amp_fill_result(struct phy_device *phydev, u16 *buf)
 {
-	int i;
-	int bias[16] = {};
-	const int vals_9461[16] = { 7, 1, 4, 7,
-				    7, 1, 4, 7,
-				    7, 1, 4, 7,
-				    7, 1, 4, 7 };
 	const int vals_9481[16] = { 10, 6, 6, 10,
 				    10, 6, 6, 10,
 				    10, 6, 6, 10,
 				    10, 6, 6, 10 };
+	const int vals_9461[16] = { 7, 1, 4, 7,
+				    7, 1, 4, 7,
+				    7, 1, 4, 7,
+				    7, 1, 4, 7 };
+	int bias[16] = {};
+	int i;
+
 	switch (phydev->drv->phy_id) {
 	case MTK_GPHY_ID_MT7981:
 		/* We add some calibration to efuse values
@@ -1069,10 +1070,10 @@ static int start_cal(struct phy_device *
 
 static int mt798x_phy_calibration(struct phy_device *phydev)
 {
+	struct nvmem_cell *cell;
 	int ret = 0;
-	u32 *buf;
 	size_t len;
-	struct nvmem_cell *cell;
+	u32 *buf;
 
 	cell = nvmem_cell_get(&phydev->mdio.dev, "phy-cal-data");
 	if (IS_ERR(cell)) {
@@ -1210,14 +1211,15 @@ static int mt798x_phy_led_brightness_set
 	return mt798x_phy_hw_led_on_set(phydev, index, (value != LED_OFF));
 }
 
-static const unsigned long supported_triggers = (BIT(TRIGGER_NETDEV_FULL_DUPLEX) |
-						 BIT(TRIGGER_NETDEV_HALF_DUPLEX) |
-						 BIT(TRIGGER_NETDEV_LINK)        |
-						 BIT(TRIGGER_NETDEV_LINK_10)     |
-						 BIT(TRIGGER_NETDEV_LINK_100)    |
-						 BIT(TRIGGER_NETDEV_LINK_1000)   |
-						 BIT(TRIGGER_NETDEV_RX)          |
-						 BIT(TRIGGER_NETDEV_TX));
+static const unsigned long supported_triggers =
+	BIT(TRIGGER_NETDEV_FULL_DUPLEX) |
+	BIT(TRIGGER_NETDEV_HALF_DUPLEX) |
+	BIT(TRIGGER_NETDEV_LINK)        |
+	BIT(TRIGGER_NETDEV_LINK_10)     |
+	BIT(TRIGGER_NETDEV_LINK_100)    |
+	BIT(TRIGGER_NETDEV_LINK_1000)   |
+	BIT(TRIGGER_NETDEV_RX)          |
+	BIT(TRIGGER_NETDEV_TX);
 
 static int mt798x_phy_led_hw_is_supported(struct phy_device *phydev, u8 index,
 					  unsigned long rules)
@@ -1415,7 +1417,7 @@ static int mt7988_phy_probe_shared(struc
 	 * LED_C and LED_D respectively. At the same time those pins are used to
 	 * bootstrap configuration of the reference clock source (LED_A),
 	 * DRAM DDRx16b x2/x1 (LED_B) and boot device (LED_C, LED_D).
-	 * In practise this is done using a LED and a resistor pulling the pin
+	 * In practice this is done using a LED and a resistor pulling the pin
 	 * either to GND or to VIO.
 	 * The detected value at boot time is accessible at run-time using the
 	 * TPBANK0 register located in the gpio base of the pinctrl, in order
