From 71e79430117d56c409c5ea485a263bc0d8083390 Mon Sep 17 00:00:00 2001
From: Eric Woudstra <ericwouds@gmail.com>
Date: Tue, 26 Mar 2024 17:23:05 +0100
Subject: [PATCH] net: phy: air_en8811h: Add the Airoha EN8811H PHY driver

Add the driver for the Airoha EN8811H 2.5 Gigabit PHY. The phy supports
100/1000/2500 Mbps with auto negotiation only.

The driver uses two firmware files, for which updated versions are added to
linux-firmware already.

Note: At phy-address + 8 there is another device on the mdio bus, that
belongs to the EN881H. While the original driver writes to it, Airoha
has confirmed this is not needed. Therefore, communication with this
device is not included in this driver.

Signed-off-by: Eric Woudstra <ericwouds@gmail.com>
Reviewed-by: Andrew Lunn <andrew@lunn.ch>
Link: https://lore.kernel.org/r/20240326162305.303598-3-ericwouds@gmail.com
Signed-off-by: Jakub Kicinski <kuba@kernel.org>
---
 drivers/net/phy/Kconfig       |    5 +
 drivers/net/phy/Makefile      |    1 +
 drivers/net/phy/air_en8811h.c | 1086 +++++++++++++++++++++++++++++++++
 3 files changed, 1092 insertions(+)
 create mode 100644 drivers/net/phy/air_en8811h.c

--- a/drivers/net/phy/Kconfig
+++ b/drivers/net/phy/Kconfig
@@ -80,6 +80,11 @@ config AS21XXX_PHY
 	  AS21210PB1 that all register with the PHY ID 0x7500 0x7500
 	  before the firmware is loaded.
 
+config AIR_EN8811H_PHY
+	tristate "Airoha EN8811H 2.5 Gigabit PHY"
+	help
+	  Currently supports the Airoha EN8811H PHY.
+
 config AMD_PHY
 	tristate "AMD PHYs"
 	help
--- a/drivers/net/phy/Makefile
+++ b/drivers/net/phy/Makefile
@@ -34,6 +34,7 @@ obj-y				+= $(sfp-obj-y) $(sfp-obj-m)
 
 obj-$(CONFIG_ADIN_PHY)		+= adin.o
 obj-$(CONFIG_ADIN1100_PHY)	+= adin1100.o
+obj-$(CONFIG_AIR_EN8811H_PHY)   += air_en8811h.o
 obj-$(CONFIG_AMD_PHY)		+= amd.o
 obj-$(CONFIG_AQUANTIA_PHY)	+= aquantia/
 obj-$(CONFIG_AS21XXX_PHY)	+= as21xxx.o
--- /dev/null
+++ b/drivers/net/phy/air_en8811h.c
@@ -0,0 +1,1086 @@
+// SPDX-License-Identifier: GPL-2.0+
+/*
+ * Driver for the Airoha EN8811H 2.5 Gigabit PHY.
+ *
+ * Limitations of the EN8811H:
+ * - Only full duplex supported
+ * - Forced speed (AN off) is not supported by hardware (100Mbps)
+ *
+ * Source originated from airoha's en8811h.c and en8811h.h v1.2.1
+ *
+ * Copyright (C) 2023 Airoha Technology Corp.
+ */
+
+#include <linux/phy.h>
+#include <linux/firmware.h>
+#include <linux/property.h>
+#include <linux/wordpart.h>
+#include <asm/unaligned.h>
+
+#define EN8811H_PHY_ID		0x03a2a411
+
+#define EN8811H_MD32_DM		"airoha/EthMD32.dm.bin"
+#define EN8811H_MD32_DSP	"airoha/EthMD32.DSP.bin"
+
+#define AIR_FW_ADDR_DM	0x00000000
+#define AIR_FW_ADDR_DSP	0x00100000
+
+/* MII Registers */
+#define AIR_AUX_CTRL_STATUS		0x1d
+#define   AIR_AUX_CTRL_STATUS_SPEED_MASK	GENMASK(4, 2)
+#define   AIR_AUX_CTRL_STATUS_SPEED_100		0x4
+#define   AIR_AUX_CTRL_STATUS_SPEED_1000	0x8
+#define   AIR_AUX_CTRL_STATUS_SPEED_2500	0xc
+
+#define AIR_EXT_PAGE_ACCESS		0x1f
+#define   AIR_PHY_PAGE_STANDARD			0x0000
+#define   AIR_PHY_PAGE_EXTENDED_4		0x0004
+
+/* MII Registers Page 4*/
+#define AIR_BPBUS_MODE			0x10
+#define   AIR_BPBUS_MODE_ADDR_FIXED		0x0000
+#define   AIR_BPBUS_MODE_ADDR_INCR		BIT(15)
+#define AIR_BPBUS_WR_ADDR_HIGH		0x11
+#define AIR_BPBUS_WR_ADDR_LOW		0x12
+#define AIR_BPBUS_WR_DATA_HIGH		0x13
+#define AIR_BPBUS_WR_DATA_LOW		0x14
+#define AIR_BPBUS_RD_ADDR_HIGH		0x15
+#define AIR_BPBUS_RD_ADDR_LOW		0x16
+#define AIR_BPBUS_RD_DATA_HIGH		0x17
+#define AIR_BPBUS_RD_DATA_LOW		0x18
+
+/* Registers on MDIO_MMD_VEND1 */
+#define EN8811H_PHY_FW_STATUS		0x8009
+#define   EN8811H_PHY_READY			0x02
+
+#define AIR_PHY_MCU_CMD_1		0x800c
+#define AIR_PHY_MCU_CMD_1_MODE1			0x0
+#define AIR_PHY_MCU_CMD_2		0x800d
+#define AIR_PHY_MCU_CMD_2_MODE1			0x0
+#define AIR_PHY_MCU_CMD_3		0x800e
+#define AIR_PHY_MCU_CMD_3_MODE1			0x1101
+#define AIR_PHY_MCU_CMD_3_DOCMD			0x1100
+#define AIR_PHY_MCU_CMD_4		0x800f
+#define AIR_PHY_MCU_CMD_4_MODE1			0x0002
+#define AIR_PHY_MCU_CMD_4_INTCLR		0x00e4
+
+/* Registers on MDIO_MMD_VEND2 */
+#define AIR_PHY_LED_BCR			0x021
+#define   AIR_PHY_LED_BCR_MODE_MASK		GENMASK(1, 0)
+#define   AIR_PHY_LED_BCR_TIME_TEST		BIT(2)
+#define   AIR_PHY_LED_BCR_CLK_EN		BIT(3)
+#define   AIR_PHY_LED_BCR_EXT_CTRL		BIT(15)
+
+#define AIR_PHY_LED_DUR_ON		0x022
+
+#define AIR_PHY_LED_DUR_BLINK		0x023
+
+#define AIR_PHY_LED_ON(i)	       (0x024 + ((i) * 2))
+#define   AIR_PHY_LED_ON_MASK			(GENMASK(6, 0) | BIT(8))
+#define   AIR_PHY_LED_ON_LINK1000		BIT(0)
+#define   AIR_PHY_LED_ON_LINK100		BIT(1)
+#define   AIR_PHY_LED_ON_LINK10			BIT(2)
+#define   AIR_PHY_LED_ON_LINKDOWN		BIT(3)
+#define   AIR_PHY_LED_ON_FDX			BIT(4) /* Full duplex */
+#define   AIR_PHY_LED_ON_HDX			BIT(5) /* Half duplex */
+#define   AIR_PHY_LED_ON_FORCE_ON		BIT(6)
+#define   AIR_PHY_LED_ON_LINK2500		BIT(8)
+#define   AIR_PHY_LED_ON_POLARITY		BIT(14)
+#define   AIR_PHY_LED_ON_ENABLE			BIT(15)
+
+#define AIR_PHY_LED_BLINK(i)	       (0x025 + ((i) * 2))
+#define   AIR_PHY_LED_BLINK_1000TX		BIT(0)
+#define   AIR_PHY_LED_BLINK_1000RX		BIT(1)
+#define   AIR_PHY_LED_BLINK_100TX		BIT(2)
+#define   AIR_PHY_LED_BLINK_100RX		BIT(3)
+#define   AIR_PHY_LED_BLINK_10TX		BIT(4)
+#define   AIR_PHY_LED_BLINK_10RX		BIT(5)
+#define   AIR_PHY_LED_BLINK_COLLISION		BIT(6)
+#define   AIR_PHY_LED_BLINK_RX_CRC_ERR		BIT(7)
+#define   AIR_PHY_LED_BLINK_RX_IDLE_ERR		BIT(8)
+#define   AIR_PHY_LED_BLINK_FORCE_BLINK		BIT(9)
+#define   AIR_PHY_LED_BLINK_2500TX		BIT(10)
+#define   AIR_PHY_LED_BLINK_2500RX		BIT(11)
+
+/* Registers on BUCKPBUS */
+#define EN8811H_2P5G_LPA		0x3b30
+#define   EN8811H_2P5G_LPA_2P5G			BIT(0)
+
+#define EN8811H_FW_VERSION		0x3b3c
+
+#define EN8811H_POLARITY		0xca0f8
+#define   EN8811H_POLARITY_TX_NORMAL		BIT(0)
+#define   EN8811H_POLARITY_RX_REVERSE		BIT(1)
+
+#define EN8811H_GPIO_OUTPUT		0xcf8b8
+#define   EN8811H_GPIO_OUTPUT_345		(BIT(3) | BIT(4) | BIT(5))
+
+#define EN8811H_FW_CTRL_1		0x0f0018
+#define   EN8811H_FW_CTRL_1_START		0x0
+#define   EN8811H_FW_CTRL_1_FINISH		0x1
+#define EN8811H_FW_CTRL_2		0x800000
+#define EN8811H_FW_CTRL_2_LOADING		BIT(11)
+
+/* Led definitions */
+#define EN8811H_LED_COUNT	3
+
+/* Default LED setup:
+ * GPIO5 <-> LED0  On: Link detected, blink Rx/Tx
+ * GPIO4 <-> LED1  On: Link detected at 2500 or 1000 Mbps
+ * GPIO3 <-> LED2  On: Link detected at 2500 or  100 Mbps
+ */
+#define AIR_DEFAULT_TRIGGER_LED0 (BIT(TRIGGER_NETDEV_LINK)      | \
+				  BIT(TRIGGER_NETDEV_RX)        | \
+				  BIT(TRIGGER_NETDEV_TX))
+#define AIR_DEFAULT_TRIGGER_LED1 (BIT(TRIGGER_NETDEV_LINK_2500) | \
+				  BIT(TRIGGER_NETDEV_LINK_1000))
+#define AIR_DEFAULT_TRIGGER_LED2 (BIT(TRIGGER_NETDEV_LINK_2500) | \
+				  BIT(TRIGGER_NETDEV_LINK_100))
+
+struct led {
+	unsigned long rules;
+	unsigned long state;
+};
+
+struct en8811h_priv {
+	u32		firmware_version;
+	bool		mcu_needs_restart;
+	struct led	led[EN8811H_LED_COUNT];
+};
+
+enum {
+	AIR_PHY_LED_STATE_FORCE_ON,
+	AIR_PHY_LED_STATE_FORCE_BLINK,
+};
+
+enum {
+	AIR_PHY_LED_DUR_BLINK_32MS,
+	AIR_PHY_LED_DUR_BLINK_64MS,
+	AIR_PHY_LED_DUR_BLINK_128MS,
+	AIR_PHY_LED_DUR_BLINK_256MS,
+	AIR_PHY_LED_DUR_BLINK_512MS,
+	AIR_PHY_LED_DUR_BLINK_1024MS,
+};
+
+enum {
+	AIR_LED_DISABLE,
+	AIR_LED_ENABLE,
+};
+
+enum {
+	AIR_ACTIVE_LOW,
+	AIR_ACTIVE_HIGH,
+};
+
+enum {
+	AIR_LED_MODE_DISABLE,
+	AIR_LED_MODE_USER_DEFINE,
+};
+
+#define AIR_PHY_LED_DUR_UNIT	1024
+#define AIR_PHY_LED_DUR (AIR_PHY_LED_DUR_UNIT << AIR_PHY_LED_DUR_BLINK_64MS)
+
+static const unsigned long en8811h_led_trig = BIT(TRIGGER_NETDEV_FULL_DUPLEX) |
+					      BIT(TRIGGER_NETDEV_LINK)        |
+					      BIT(TRIGGER_NETDEV_LINK_10)     |
+					      BIT(TRIGGER_NETDEV_LINK_100)    |
+					      BIT(TRIGGER_NETDEV_LINK_1000)   |
+					      BIT(TRIGGER_NETDEV_LINK_2500)   |
+					      BIT(TRIGGER_NETDEV_RX)          |
+					      BIT(TRIGGER_NETDEV_TX);
+
+static int air_phy_read_page(struct phy_device *phydev)
+{
+	return __phy_read(phydev, AIR_EXT_PAGE_ACCESS);
+}
+
+static int air_phy_write_page(struct phy_device *phydev, int page)
+{
+	return __phy_write(phydev, AIR_EXT_PAGE_ACCESS, page);
+}
+
+static int __air_buckpbus_reg_write(struct phy_device *phydev,
+				    u32 pbus_address, u32 pbus_data)
+{
+	int ret;
+
+	ret = __phy_write(phydev, AIR_BPBUS_MODE, AIR_BPBUS_MODE_ADDR_FIXED);
+	if (ret < 0)
+		return ret;
+
+	ret = __phy_write(phydev, AIR_BPBUS_WR_ADDR_HIGH,
+			  upper_16_bits(pbus_address));
+	if (ret < 0)
+		return ret;
+
+	ret = __phy_write(phydev, AIR_BPBUS_WR_ADDR_LOW,
+			  lower_16_bits(pbus_address));
+	if (ret < 0)
+		return ret;
+
+	ret = __phy_write(phydev, AIR_BPBUS_WR_DATA_HIGH,
+			  upper_16_bits(pbus_data));
+	if (ret < 0)
+		return ret;
+
+	ret = __phy_write(phydev, AIR_BPBUS_WR_DATA_LOW,
+			  lower_16_bits(pbus_data));
+	if (ret < 0)
+		return ret;
+
+	return 0;
+}
+
+static int air_buckpbus_reg_write(struct phy_device *phydev,
+				  u32 pbus_address, u32 pbus_data)
+{
+	int saved_page;
+	int ret = 0;
+
+	saved_page = phy_select_page(phydev, AIR_PHY_PAGE_EXTENDED_4);
+
+	if (saved_page >= 0) {
+		ret = __air_buckpbus_reg_write(phydev, pbus_address,
+					       pbus_data);
+		if (ret < 0)
+			phydev_err(phydev, "%s 0x%08x failed: %d\n", __func__,
+				   pbus_address, ret);
+	}
+
+	return phy_restore_page(phydev, saved_page, ret);
+}
+
+static int __air_buckpbus_reg_read(struct phy_device *phydev,
+				   u32 pbus_address, u32 *pbus_data)
+{
+	int pbus_data_low, pbus_data_high;
+	int ret;
+
+	ret = __phy_write(phydev, AIR_BPBUS_MODE, AIR_BPBUS_MODE_ADDR_FIXED);
+	if (ret < 0)
+		return ret;
+
+	ret = __phy_write(phydev, AIR_BPBUS_RD_ADDR_HIGH,
+			  upper_16_bits(pbus_address));
+	if (ret < 0)
+		return ret;
+
+	ret = __phy_write(phydev, AIR_BPBUS_RD_ADDR_LOW,
+			  lower_16_bits(pbus_address));
+	if (ret < 0)
+		return ret;
+
+	pbus_data_high = __phy_read(phydev, AIR_BPBUS_RD_DATA_HIGH);
+	if (pbus_data_high < 0)
+		return ret;
+
+	pbus_data_low = __phy_read(phydev, AIR_BPBUS_RD_DATA_LOW);
+	if (pbus_data_low < 0)
+		return ret;
+
+	*pbus_data = pbus_data_low | (pbus_data_high << 16);
+	return 0;
+}
+
+static int air_buckpbus_reg_read(struct phy_device *phydev,
+				 u32 pbus_address, u32 *pbus_data)
+{
+	int saved_page;
+	int ret = 0;
+
+	saved_page = phy_select_page(phydev, AIR_PHY_PAGE_EXTENDED_4);
+
+	if (saved_page >= 0) {
+		ret = __air_buckpbus_reg_read(phydev, pbus_address, pbus_data);
+		if (ret < 0)
+			phydev_err(phydev, "%s 0x%08x failed: %d\n", __func__,
+				   pbus_address, ret);
+	}
+
+	return phy_restore_page(phydev, saved_page, ret);
+}
+
+static int __air_buckpbus_reg_modify(struct phy_device *phydev,
+				     u32 pbus_address, u32 mask, u32 set)
+{
+	int pbus_data_low, pbus_data_high;
+	u32 pbus_data_old, pbus_data_new;
+	int ret;
+
+	ret = __phy_write(phydev, AIR_BPBUS_MODE, AIR_BPBUS_MODE_ADDR_FIXED);
+	if (ret < 0)
+		return ret;
+
+	ret = __phy_write(phydev, AIR_BPBUS_RD_ADDR_HIGH,
+			  upper_16_bits(pbus_address));
+	if (ret < 0)
+		return ret;
+
+	ret = __phy_write(phydev, AIR_BPBUS_RD_ADDR_LOW,
+			  lower_16_bits(pbus_address));
+	if (ret < 0)
+		return ret;
+
+	pbus_data_high = __phy_read(phydev, AIR_BPBUS_RD_DATA_HIGH);
+	if (pbus_data_high < 0)
+		return ret;
+
+	pbus_data_low = __phy_read(phydev, AIR_BPBUS_RD_DATA_LOW);
+	if (pbus_data_low < 0)
+		return ret;
+
+	pbus_data_old = pbus_data_low | (pbus_data_high << 16);
+	pbus_data_new = (pbus_data_old & ~mask) | set;
+	if (pbus_data_new == pbus_data_old)
+		return 0;
+
+	ret = __phy_write(phydev, AIR_BPBUS_WR_ADDR_HIGH,
+			  upper_16_bits(pbus_address));
+	if (ret < 0)
+		return ret;
+
+	ret = __phy_write(phydev, AIR_BPBUS_WR_ADDR_LOW,
+			  lower_16_bits(pbus_address));
+	if (ret < 0)
+		return ret;
+
+	ret = __phy_write(phydev, AIR_BPBUS_WR_DATA_HIGH,
+			  upper_16_bits(pbus_data_new));
+	if (ret < 0)
+		return ret;
+
+	ret = __phy_write(phydev, AIR_BPBUS_WR_DATA_LOW,
+			  lower_16_bits(pbus_data_new));
+	if (ret < 0)
+		return ret;
+
+	return 0;
+}
+
+static int air_buckpbus_reg_modify(struct phy_device *phydev,
+				   u32 pbus_address, u32 mask, u32 set)
+{
+	int saved_page;
+	int ret = 0;
+
+	saved_page = phy_select_page(phydev, AIR_PHY_PAGE_EXTENDED_4);
+
+	if (saved_page >= 0) {
+		ret = __air_buckpbus_reg_modify(phydev, pbus_address, mask,
+						set);
+		if (ret < 0)
+			phydev_err(phydev, "%s 0x%08x failed: %d\n", __func__,
+				   pbus_address, ret);
+	}
+
+	return phy_restore_page(phydev, saved_page, ret);
+}
+
+static int __air_write_buf(struct phy_device *phydev, u32 address,
+			   const struct firmware *fw)
+{
+	unsigned int offset;
+	int ret;
+	u16 val;
+
+	ret = __phy_write(phydev, AIR_BPBUS_MODE, AIR_BPBUS_MODE_ADDR_INCR);
+	if (ret < 0)
+		return ret;
+
+	ret = __phy_write(phydev, AIR_BPBUS_WR_ADDR_HIGH,
+			  upper_16_bits(address));
+	if (ret < 0)
+		return ret;
+
+	ret = __phy_write(phydev, AIR_BPBUS_WR_ADDR_LOW,
+			  lower_16_bits(address));
+	if (ret < 0)
+		return ret;
+
+	for (offset = 0; offset < fw->size; offset += 4) {
+		val = get_unaligned_le16(&fw->data[offset + 2]);
+		ret = __phy_write(phydev, AIR_BPBUS_WR_DATA_HIGH, val);
+		if (ret < 0)
+			return ret;
+
+		val = get_unaligned_le16(&fw->data[offset]);
+		ret = __phy_write(phydev, AIR_BPBUS_WR_DATA_LOW, val);
+		if (ret < 0)
+			return ret;
+	}
+
+	return 0;
+}
+
+static int air_write_buf(struct phy_device *phydev, u32 address,
+			 const struct firmware *fw)
+{
+	int saved_page;
+	int ret = 0;
+
+	saved_page = phy_select_page(phydev, AIR_PHY_PAGE_EXTENDED_4);
+
+	if (saved_page >= 0) {
+		ret = __air_write_buf(phydev, address, fw);
+		if (ret < 0)
+			phydev_err(phydev, "%s 0x%08x failed: %d\n", __func__,
+				   address, ret);
+	}
+
+	return phy_restore_page(phydev, saved_page, ret);
+}
+
+static int en8811h_wait_mcu_ready(struct phy_device *phydev)
+{
+	int ret, reg_value;
+
+	/* Because of mdio-lock, may have to wait for multiple loads */
+	ret = phy_read_mmd_poll_timeout(phydev, MDIO_MMD_VEND1,
+					EN8811H_PHY_FW_STATUS, reg_value,
+					reg_value == EN8811H_PHY_READY,
+					20000, 7500000, true);
+	if (ret) {
+		phydev_err(phydev, "MCU not ready: 0x%x\n", reg_value);
+		return -ENODEV;
+	}
+
+	return 0;
+}
+
+static int en8811h_load_firmware(struct phy_device *phydev)
+{
+	struct en8811h_priv *priv = phydev->priv;
+	struct device *dev = &phydev->mdio.dev;
+	const struct firmware *fw1, *fw2;
+	int ret;
+
+	ret = request_firmware_direct(&fw1, EN8811H_MD32_DM, dev);
+	if (ret < 0)
+		return ret;
+
+	ret = request_firmware_direct(&fw2, EN8811H_MD32_DSP, dev);
+	if (ret < 0)
+		goto en8811h_load_firmware_rel1;
+
+	ret = air_buckpbus_reg_write(phydev, EN8811H_FW_CTRL_1,
+				     EN8811H_FW_CTRL_1_START);
+	if (ret < 0)
+		goto en8811h_load_firmware_out;
+
+	ret = air_buckpbus_reg_modify(phydev, EN8811H_FW_CTRL_2,
+				      EN8811H_FW_CTRL_2_LOADING,
+				      EN8811H_FW_CTRL_2_LOADING);
+	if (ret < 0)
+		goto en8811h_load_firmware_out;
+
+	ret = air_write_buf(phydev, AIR_FW_ADDR_DM,  fw1);
+	if (ret < 0)
+		goto en8811h_load_firmware_out;
+
+	ret = air_write_buf(phydev, AIR_FW_ADDR_DSP, fw2);
+	if (ret < 0)
+		goto en8811h_load_firmware_out;
+
+	ret = air_buckpbus_reg_modify(phydev, EN8811H_FW_CTRL_2,
+				      EN8811H_FW_CTRL_2_LOADING, 0);
+	if (ret < 0)
+		goto en8811h_load_firmware_out;
+
+	ret = air_buckpbus_reg_write(phydev, EN8811H_FW_CTRL_1,
+				     EN8811H_FW_CTRL_1_FINISH);
+	if (ret < 0)
+		goto en8811h_load_firmware_out;
+
+	ret = en8811h_wait_mcu_ready(phydev);
+
+	air_buckpbus_reg_read(phydev, EN8811H_FW_VERSION,
+			      &priv->firmware_version);
+	phydev_info(phydev, "MD32 firmware version: %08x\n",
+		    priv->firmware_version);
+
+en8811h_load_firmware_out:
+	release_firmware(fw2);
+
+en8811h_load_firmware_rel1:
+	release_firmware(fw1);
+
+	if (ret < 0)
+		phydev_err(phydev, "Load firmware failed: %d\n", ret);
+
+	return ret;
+}
+
+static int en8811h_restart_mcu(struct phy_device *phydev)
+{
+	int ret;
+
+	ret = air_buckpbus_reg_write(phydev, EN8811H_FW_CTRL_1,
+				     EN8811H_FW_CTRL_1_START);
+	if (ret < 0)
+		return ret;
+
+	ret = air_buckpbus_reg_write(phydev, EN8811H_FW_CTRL_1,
+				     EN8811H_FW_CTRL_1_FINISH);
+	if (ret < 0)
+		return ret;
+
+	return en8811h_wait_mcu_ready(phydev);
+}
+
+static int air_hw_led_on_set(struct phy_device *phydev, u8 index, bool on)
+{
+	struct en8811h_priv *priv = phydev->priv;
+	bool changed;
+
+	if (index >= EN8811H_LED_COUNT)
+		return -EINVAL;
+
+	if (on)
+		changed = !test_and_set_bit(AIR_PHY_LED_STATE_FORCE_ON,
+					    &priv->led[index].state);
+	else
+		changed = !!test_and_clear_bit(AIR_PHY_LED_STATE_FORCE_ON,
+					       &priv->led[index].state);
+
+	changed |= (priv->led[index].rules != 0);
+
+	if (changed)
+		return phy_modify_mmd(phydev, MDIO_MMD_VEND2,
+				      AIR_PHY_LED_ON(index),
+				      AIR_PHY_LED_ON_MASK,
+				      on ? AIR_PHY_LED_ON_FORCE_ON : 0);
+
+	return 0;
+}
+
+static int air_hw_led_blink_set(struct phy_device *phydev, u8 index,
+				bool blinking)
+{
+	struct en8811h_priv *priv = phydev->priv;
+	bool changed;
+
+	if (index >= EN8811H_LED_COUNT)
+		return -EINVAL;
+
+	if (blinking)
+		changed = !test_and_set_bit(AIR_PHY_LED_STATE_FORCE_BLINK,
+					    &priv->led[index].state);
+	else
+		changed = !!test_and_clear_bit(AIR_PHY_LED_STATE_FORCE_BLINK,
+					       &priv->led[index].state);
+
+	changed |= (priv->led[index].rules != 0);
+
+	if (changed)
+		return phy_write_mmd(phydev, MDIO_MMD_VEND2,
+				     AIR_PHY_LED_BLINK(index),
+				     blinking ?
+				     AIR_PHY_LED_BLINK_FORCE_BLINK : 0);
+	else
+		return 0;
+}
+
+static int air_led_blink_set(struct phy_device *phydev, u8 index,
+			     unsigned long *delay_on,
+			     unsigned long *delay_off)
+{
+	struct en8811h_priv *priv = phydev->priv;
+	bool blinking = false;
+	int err;
+
+	if (index >= EN8811H_LED_COUNT)
+		return -EINVAL;
+
+	if (delay_on && delay_off && (*delay_on > 0) && (*delay_off > 0)) {
+		blinking = true;
+		*delay_on = 50;
+		*delay_off = 50;
+	}
+
+	err = air_hw_led_blink_set(phydev, index, blinking);
+	if (err)
+		return err;
+
+	/* led-blink set, so switch led-on off */
+	err = air_hw_led_on_set(phydev, index, false);
+	if (err)
+		return err;
+
+	/* hw-control is off*/
+	if (!!test_bit(AIR_PHY_LED_STATE_FORCE_BLINK, &priv->led[index].state))
+		priv->led[index].rules = 0;
+
+	return 0;
+}
+
+static int air_led_brightness_set(struct phy_device *phydev, u8 index,
+				  enum led_brightness value)
+{
+	struct en8811h_priv *priv = phydev->priv;
+	int err;
+
+	if (index >= EN8811H_LED_COUNT)
+		return -EINVAL;
+
+	/* led-on set, so switch led-blink off */
+	err = air_hw_led_blink_set(phydev, index, false);
+	if (err)
+		return err;
+
+	err = air_hw_led_on_set(phydev, index, (value != LED_OFF));
+	if (err)
+		return err;
+
+	/* hw-control is off */
+	if (!!test_bit(AIR_PHY_LED_STATE_FORCE_ON, &priv->led[index].state))
+		priv->led[index].rules = 0;
+
+	return 0;
+}
+
+static int air_led_hw_control_get(struct phy_device *phydev, u8 index,
+				  unsigned long *rules)
+{
+	struct en8811h_priv *priv = phydev->priv;
+
+	if (index >= EN8811H_LED_COUNT)
+		return -EINVAL;
+
+	*rules = priv->led[index].rules;
+
+	return 0;
+};
+
+static int air_led_hw_control_set(struct phy_device *phydev, u8 index,
+				  unsigned long rules)
+{
+	struct en8811h_priv *priv = phydev->priv;
+	u16 on = 0, blink = 0;
+	int ret;
+
+	if (index >= EN8811H_LED_COUNT)
+		return -EINVAL;
+
+	priv->led[index].rules = rules;
+
+	if (rules & BIT(TRIGGER_NETDEV_FULL_DUPLEX))
+		on |= AIR_PHY_LED_ON_FDX;
+
+	if (rules & (BIT(TRIGGER_NETDEV_LINK_10) | BIT(TRIGGER_NETDEV_LINK)))
+		on |= AIR_PHY_LED_ON_LINK10;
+
+	if (rules & (BIT(TRIGGER_NETDEV_LINK_100) | BIT(TRIGGER_NETDEV_LINK)))
+		on |= AIR_PHY_LED_ON_LINK100;
+
+	if (rules & (BIT(TRIGGER_NETDEV_LINK_1000) | BIT(TRIGGER_NETDEV_LINK)))
+		on |= AIR_PHY_LED_ON_LINK1000;
+
+	if (rules & (BIT(TRIGGER_NETDEV_LINK_2500) | BIT(TRIGGER_NETDEV_LINK)))
+		on |= AIR_PHY_LED_ON_LINK2500;
+
+	if (rules & BIT(TRIGGER_NETDEV_RX)) {
+		blink |= AIR_PHY_LED_BLINK_10RX   |
+			 AIR_PHY_LED_BLINK_100RX  |
+			 AIR_PHY_LED_BLINK_1000RX |
+			 AIR_PHY_LED_BLINK_2500RX;
+	}
+
+	if (rules & BIT(TRIGGER_NETDEV_TX)) {
+		blink |= AIR_PHY_LED_BLINK_10TX   |
+			 AIR_PHY_LED_BLINK_100TX  |
+			 AIR_PHY_LED_BLINK_1000TX |
+			 AIR_PHY_LED_BLINK_2500TX;
+	}
+
+	if (blink || on) {
+		/* switch hw-control on, so led-on and led-blink are off */
+		clear_bit(AIR_PHY_LED_STATE_FORCE_ON,
+			  &priv->led[index].state);
+		clear_bit(AIR_PHY_LED_STATE_FORCE_BLINK,
+			  &priv->led[index].state);
+	} else {
+		priv->led[index].rules = 0;
+	}
+
+	ret = phy_modify_mmd(phydev, MDIO_MMD_VEND2, AIR_PHY_LED_ON(index),
+			     AIR_PHY_LED_ON_MASK, on);
+
+	if (ret < 0)
+		return ret;
+
+	return phy_write_mmd(phydev, MDIO_MMD_VEND2, AIR_PHY_LED_BLINK(index),
+			     blink);
+};
+
+static int air_led_init(struct phy_device *phydev, u8 index, u8 state, u8 pol)
+{
+	int val = 0;
+	int err;
+
+	if (index >= EN8811H_LED_COUNT)
+		return -EINVAL;
+
+	if (state == AIR_LED_ENABLE)
+		val |= AIR_PHY_LED_ON_ENABLE;
+	else
+		val &= ~AIR_PHY_LED_ON_ENABLE;
+
+	if (pol == AIR_ACTIVE_HIGH)
+		val |= AIR_PHY_LED_ON_POLARITY;
+	else
+		val &= ~AIR_PHY_LED_ON_POLARITY;
+
+	err = phy_modify_mmd(phydev, MDIO_MMD_VEND2, AIR_PHY_LED_ON(index),
+			     AIR_PHY_LED_ON_ENABLE |
+			     AIR_PHY_LED_ON_POLARITY, val);
+
+	if (err < 0)
+		return err;
+
+	return 0;
+}
+
+static int air_leds_init(struct phy_device *phydev, int num, int dur, int mode)
+{
+	struct en8811h_priv *priv = phydev->priv;
+	int ret, i;
+
+	ret = phy_write_mmd(phydev, MDIO_MMD_VEND2, AIR_PHY_LED_DUR_BLINK,
+			    dur);
+	if (ret < 0)
+		return ret;
+
+	ret = phy_write_mmd(phydev, MDIO_MMD_VEND2, AIR_PHY_LED_DUR_ON,
+			    dur >> 1);
+	if (ret < 0)
+		return ret;
+
+	switch (mode) {
+	case AIR_LED_MODE_DISABLE:
+		ret = phy_modify_mmd(phydev, MDIO_MMD_VEND2, AIR_PHY_LED_BCR,
+				     AIR_PHY_LED_BCR_EXT_CTRL |
+				     AIR_PHY_LED_BCR_MODE_MASK, 0);
+		if (ret < 0)
+			return ret;
+		break;
+	case AIR_LED_MODE_USER_DEFINE:
+		ret = phy_modify_mmd(phydev, MDIO_MMD_VEND2, AIR_PHY_LED_BCR,
+				     AIR_PHY_LED_BCR_EXT_CTRL |
+				     AIR_PHY_LED_BCR_CLK_EN,
+				     AIR_PHY_LED_BCR_EXT_CTRL |
+				     AIR_PHY_LED_BCR_CLK_EN);
+		if (ret < 0)
+			return ret;
+		break;
+	default:
+		phydev_err(phydev, "LED mode %d is not supported\n", mode);
+		return -EINVAL;
+	}
+
+	for (i = 0; i < num; ++i) {
+		ret = air_led_init(phydev, i, AIR_LED_ENABLE, AIR_ACTIVE_HIGH);
+		if (ret < 0) {
+			phydev_err(phydev, "LED%d init failed: %d\n", i, ret);
+			return ret;
+		}
+		air_led_hw_control_set(phydev, i, priv->led[i].rules);
+	}
+
+	return 0;
+}
+
+static int en8811h_led_hw_is_supported(struct phy_device *phydev, u8 index,
+				       unsigned long rules)
+{
+	if (index >= EN8811H_LED_COUNT)
+		return -EINVAL;
+
+	/* All combinations of the supported triggers are allowed */
+	if (rules & ~en8811h_led_trig)
+		return -EOPNOTSUPP;
+
+	return 0;
+};
+
+static int en8811h_probe(struct phy_device *phydev)
+{
+	struct en8811h_priv *priv;
+	int ret;
+
+	priv = devm_kzalloc(&phydev->mdio.dev, sizeof(struct en8811h_priv),
+			    GFP_KERNEL);
+	if (!priv)
+		return -ENOMEM;
+	phydev->priv = priv;
+
+	ret = en8811h_load_firmware(phydev);
+	if (ret < 0)
+		return ret;
+
+	/* mcu has just restarted after firmware load */
+	priv->mcu_needs_restart = false;
+
+	priv->led[0].rules = AIR_DEFAULT_TRIGGER_LED0;
+	priv->led[1].rules = AIR_DEFAULT_TRIGGER_LED1;
+	priv->led[2].rules = AIR_DEFAULT_TRIGGER_LED2;
+
+	/* MDIO_DEVS1/2 empty, so set mmds_present bits here */
+	phydev->c45_ids.mmds_present |= MDIO_DEVS_PMAPMD | MDIO_DEVS_AN;
+
+	ret = air_leds_init(phydev, EN8811H_LED_COUNT, AIR_PHY_LED_DUR,
+			    AIR_LED_MODE_DISABLE);
+	if (ret < 0) {
+		phydev_err(phydev, "Failed to disable leds: %d\n", ret);
+		return ret;
+	}
+
+	/* Configure led gpio pins as output */
+	ret = air_buckpbus_reg_modify(phydev, EN8811H_GPIO_OUTPUT,
+				      EN8811H_GPIO_OUTPUT_345,
+				      EN8811H_GPIO_OUTPUT_345);
+	if (ret < 0)
+		return ret;
+
+	return 0;
+}
+
+static int en8811h_config_init(struct phy_device *phydev)
+{
+	struct en8811h_priv *priv = phydev->priv;
+	struct device *dev = &phydev->mdio.dev;
+	u32 pbus_value;
+	int ret;
+
+	/* If restart happened in .probe(), no need to restart now */
+	if (priv->mcu_needs_restart) {
+		ret = en8811h_restart_mcu(phydev);
+		if (ret < 0)
+			return ret;
+	} else {
+		/* Next calls to .config_init() mcu needs to restart */
+		priv->mcu_needs_restart = true;
+	}
+
+	/* Select mode 1, the only mode supported.
+	 * Configures the SerDes for 2500Base-X with rate adaptation
+	 */
+	ret = phy_write_mmd(phydev, MDIO_MMD_VEND1, AIR_PHY_MCU_CMD_1,
+			    AIR_PHY_MCU_CMD_1_MODE1);
+	if (ret < 0)
+		return ret;
+	ret = phy_write_mmd(phydev, MDIO_MMD_VEND1, AIR_PHY_MCU_CMD_2,
+			    AIR_PHY_MCU_CMD_2_MODE1);
+	if (ret < 0)
+		return ret;
+	ret = phy_write_mmd(phydev, MDIO_MMD_VEND1, AIR_PHY_MCU_CMD_3,
+			    AIR_PHY_MCU_CMD_3_MODE1);
+	if (ret < 0)
+		return ret;
+	ret = phy_write_mmd(phydev, MDIO_MMD_VEND1, AIR_PHY_MCU_CMD_4,
+			    AIR_PHY_MCU_CMD_4_MODE1);
+	if (ret < 0)
+		return ret;
+
+	/* Serdes polarity */
+	pbus_value = 0;
+	if (device_property_read_bool(dev, "airoha,pnswap-rx"))
+		pbus_value |=  EN8811H_POLARITY_RX_REVERSE;
+	else
+		pbus_value &= ~EN8811H_POLARITY_RX_REVERSE;
+	if (device_property_read_bool(dev, "airoha,pnswap-tx"))
+		pbus_value &= ~EN8811H_POLARITY_TX_NORMAL;
+	else
+		pbus_value |=  EN8811H_POLARITY_TX_NORMAL;
+	ret = air_buckpbus_reg_modify(phydev, EN8811H_POLARITY,
+				      EN8811H_POLARITY_RX_REVERSE |
+				      EN8811H_POLARITY_TX_NORMAL, pbus_value);
+	if (ret < 0)
+		return ret;
+
+	ret = air_leds_init(phydev, EN8811H_LED_COUNT, AIR_PHY_LED_DUR,
+			    AIR_LED_MODE_USER_DEFINE);
+	if (ret < 0) {
+		phydev_err(phydev, "Failed to initialize leds: %d\n", ret);
+		return ret;
+	}
+
+	return 0;
+}
+
+static int en8811h_get_features(struct phy_device *phydev)
+{
+	linkmode_set_bit_array(phy_basic_ports_array,
+			       ARRAY_SIZE(phy_basic_ports_array),
+			       phydev->supported);
+
+	return genphy_c45_pma_read_abilities(phydev);
+}
+
+static int en8811h_get_rate_matching(struct phy_device *phydev,
+				     phy_interface_t iface)
+{
+	return RATE_MATCH_PAUSE;
+}
+
+static int en8811h_config_aneg(struct phy_device *phydev)
+{
+	bool changed = false;
+	int ret;
+	u32 adv;
+
+	if (phydev->autoneg == AUTONEG_DISABLE) {
+		phydev_warn(phydev, "Disabling autoneg is not supported\n");
+		return -EINVAL;
+	}
+
+	adv = linkmode_adv_to_mii_10gbt_adv_t(phydev->advertising);
+
+	ret = phy_modify_mmd_changed(phydev, MDIO_MMD_AN, MDIO_AN_10GBT_CTRL,
+				     MDIO_AN_10GBT_CTRL_ADV2_5G, adv);
+	if (ret < 0)
+		return ret;
+	if (ret > 0)
+		changed = true;
+
+	return __genphy_config_aneg(phydev, changed);
+}
+
+static int en8811h_read_status(struct phy_device *phydev)
+{
+	struct en8811h_priv *priv = phydev->priv;
+	u32 pbus_value;
+	int ret, val;
+
+	ret = genphy_update_link(phydev);
+	if (ret)
+		return ret;
+
+	phydev->master_slave_get = MASTER_SLAVE_CFG_UNSUPPORTED;
+	phydev->master_slave_state = MASTER_SLAVE_STATE_UNSUPPORTED;
+	phydev->speed = SPEED_UNKNOWN;
+	phydev->duplex = DUPLEX_UNKNOWN;
+	phydev->pause = 0;
+	phydev->asym_pause = 0;
+	phydev->rate_matching = RATE_MATCH_PAUSE;
+
+	ret = genphy_read_master_slave(phydev);
+	if (ret < 0)
+		return ret;
+
+	ret = genphy_read_lpa(phydev);
+	if (ret < 0)
+		return ret;
+
+	/* Get link partner 2.5GBASE-T ability from vendor register */
+	ret = air_buckpbus_reg_read(phydev, EN8811H_2P5G_LPA, &pbus_value);
+	if (ret < 0)
+		return ret;
+	linkmode_mod_bit(ETHTOOL_LINK_MODE_2500baseT_Full_BIT,
+			 phydev->lp_advertising,
+			 pbus_value & EN8811H_2P5G_LPA_2P5G);
+
+	if (phydev->autoneg_complete)
+		phy_resolve_aneg_pause(phydev);
+
+	if (!phydev->link)
+		return 0;
+
+	/* Get real speed from vendor register */
+	val = phy_read(phydev, AIR_AUX_CTRL_STATUS);
+	if (val < 0)
+		return val;
+	switch (val & AIR_AUX_CTRL_STATUS_SPEED_MASK) {
+	case AIR_AUX_CTRL_STATUS_SPEED_2500:
+		phydev->speed = SPEED_2500;
+		break;
+	case AIR_AUX_CTRL_STATUS_SPEED_1000:
+		phydev->speed = SPEED_1000;
+		break;
+	case AIR_AUX_CTRL_STATUS_SPEED_100:
+		phydev->speed = SPEED_100;
+		break;
+	}
+
+	/* Firmware before version 24011202 has no vendor register 2P5G_LPA.
+	 * Assume link partner advertised it if connected at 2500Mbps.
+	 */
+	if (priv->firmware_version < 0x24011202) {
+		linkmode_mod_bit(ETHTOOL_LINK_MODE_2500baseT_Full_BIT,
+				 phydev->lp_advertising,
+				 phydev->speed == SPEED_2500);
+	}
+
+	/* Only supports full duplex */
+	phydev->duplex = DUPLEX_FULL;
+
+	return 0;
+}
+
+static int en8811h_clear_intr(struct phy_device *phydev)
+{
+	int ret;
+
+	ret = phy_write_mmd(phydev, MDIO_MMD_VEND1, AIR_PHY_MCU_CMD_3,
+			    AIR_PHY_MCU_CMD_3_DOCMD);
+	if (ret < 0)
+		return ret;
+
+	ret = phy_write_mmd(phydev, MDIO_MMD_VEND1, AIR_PHY_MCU_CMD_4,
+			    AIR_PHY_MCU_CMD_4_INTCLR);
+	if (ret < 0)
+		return ret;
+
+	return 0;
+}
+
+static irqreturn_t en8811h_handle_interrupt(struct phy_device *phydev)
+{
+	int ret;
+
+	ret = en8811h_clear_intr(phydev);
+	if (ret < 0) {
+		phy_error(phydev);
+		return IRQ_NONE;
+	}
+
+	phy_trigger_machine(phydev);
+
+	return IRQ_HANDLED;
+}
+
+static struct phy_driver en8811h_driver[] = {
+{
+	PHY_ID_MATCH_MODEL(EN8811H_PHY_ID),
+	.name			= "Airoha EN8811H",
+	.probe			= en8811h_probe,
+	.get_features		= en8811h_get_features,
+	.config_init		= en8811h_config_init,
+	.get_rate_matching	= en8811h_get_rate_matching,
+	.config_aneg		= en8811h_config_aneg,
+	.read_status		= en8811h_read_status,
+	.config_intr		= en8811h_clear_intr,
+	.handle_interrupt	= en8811h_handle_interrupt,
+	.led_hw_is_supported	= en8811h_led_hw_is_supported,
+	.read_page		= air_phy_read_page,
+	.write_page		= air_phy_write_page,
+	.led_blink_set		= air_led_blink_set,
+	.led_brightness_set	= air_led_brightness_set,
+	.led_hw_control_set	= air_led_hw_control_set,
+	.led_hw_control_get	= air_led_hw_control_get,
+} };
+
+module_phy_driver(en8811h_driver);
+
+static struct mdio_device_id __maybe_unused en8811h_tbl[] = {
+	{ PHY_ID_MATCH_MODEL(EN8811H_PHY_ID) },
+	{ }
+};
+
+MODULE_DEVICE_TABLE(mdio, en8811h_tbl);
+MODULE_FIRMWARE(EN8811H_MD32_DM);
+MODULE_FIRMWARE(EN8811H_MD32_DSP);
+
+MODULE_DESCRIPTION("Airoha EN8811H PHY drivers");
+MODULE_AUTHOR("Airoha");
+MODULE_AUTHOR("Eric Woudstra <ericwouds@gmail.com>");
+MODULE_LICENSE("GPL");
