From 1824520e7477bedf76bd08c32261c755e6405cd9 Mon Sep 17 00:00:00 2001
From: Daniel Golle <daniel@makrotopia.org>
Date: Mon, 12 Aug 2024 02:56:41 +0100
Subject: [PATCH] mtd: spinand: set bitflip_threshold to 75% of ECC strength

Reporting an unclean read from SPI-NAND only when the maximum number
of correctable bitflip errors has been hit seems a bit late.
UBI LEB scrubbing, which depends on the lower MTD device reporting
correctable bitflips, then only kicks in when it's almost too late.

Set bitflip_threshold to 75% of the ECC strength, which is also the
default for raw NAND.

Signed-off-by: Daniel Golle <daniel@makrotopia.org>
Reviewed-by: Frieder Schrempf <frieder.schrempf@kontron.de>
Signed-off-by: Miquel Raynal <miquel.raynal@bootlin.com>
Link: https://lore.kernel.org/linux-mtd/2117e387260b0a96f95b8e1652ff79e0e2d71d53.1723427450.git.daniel@makrotopia.org
---
 drivers/mtd/nand/spi/core.c | 1 +
 1 file changed, 1 insertion(+)

--- a/drivers/mtd/nand/spi/core.c
+++ b/drivers/mtd/nand/spi/core.c
@@ -1290,6 +1290,7 @@ static int spinand_init(struct spinand_d
 	/* Propagate ECC information to mtd_info */
 	mtd->ecc_strength = nanddev_get_ecc_conf(nand)->strength;
 	mtd->ecc_step_size = nanddev_get_ecc_conf(nand)->step_size;
+	mtd->bitflip_threshold = DIV_ROUND_UP(mtd->ecc_strength * 3, 4);
 
 	ret = spinand_create_dirmaps(spinand);
 	if (ret) {
