From 854d71c555dfc3383c1fde7d9989b6046e21093d Mon Sep 17 00:00:00 2001
From: Heiner Kallweit <hkallweit1@gmail.com>
Date: Wed, 9 Oct 2024 07:48:05 +0200
Subject: [PATCH] r8169: remove original workaround for RTL8125 broken rx issue

Now that we have b9c7ac4fe22c ("r8169: disable ALDPS per default for
RTL8125"), the first attempt to fix the issue shouldn't be needed
any longer. So let's effectively revert 621735f59064 ("r8169: fix
rare issue with broken rx after link-down on RTL8125") and see
whether anybody complains.

Signed-off-by: Heiner Kallweit <hkallweit1@gmail.com>
Reviewed-by: Simon Horman <horms@kernel.org>
Link: https://patch.msgid.link/382d8c88-cbce-400f-ad62-fda0181c7e38@gmail.com
Signed-off-by: Jakub Kicinski <kuba@kernel.org>
---
 drivers/net/ethernet/realtek/r8169_main.c | 4 ----
 1 file changed, 4 deletions(-)

--- a/drivers/net/ethernet/realtek/r8169_main.c
+++ b/drivers/net/ethernet/realtek/r8169_main.c
@@ -4779,11 +4779,7 @@ static void r8169_phylink_handler(struct
 	if (netif_carrier_ok(ndev)) {
 		rtl_link_chg_patch(tp);
 		pm_request_resume(d);
-		netif_wake_queue(tp->dev);
 	} else {
-		/* In few cases rx is broken after link-down otherwise */
-		if (rtl_is_8125(tp))
-			rtl_schedule_task(tp, RTL_FLAG_TASK_RESET_NO_QUEUE_WAKE);
 		pm_runtime_idle(d);
 	}
 
