From 064fbc4e9b5a6dbda7fe7b67dc7e9e95d31f8d75 Mon Sep 17 00:00:00 2001
From: Daniel Golle <daniel@makrotopia.org>
Date: Thu, 4 Jul 2024 11:14:55 +0100
Subject: [PATCH] net: ethernet: mtk_eth_soc: implement .{get,set}_pauseparam
 ethtool ops

Implement operations to get and set flow-control link parameters.
Both is done by simply calling phylink_ethtool_{get,set}_pauseparam().
Fix whitespace in mtk_ethtool_ops while at it.

Signed-off-by: Daniel Golle <daniel@makrotopia.org>
Reviewed-by: Michal Kubiak <michal.kubiak@intel.com>
Reviewed-by: Russell King (Oracle) <rmk+kernel@armlinux.org.uk>
Tested-by: Rui Salvaterra <rsalvaterra@gmail.com>
Link: https://patch.msgid.link/e3ece47323444631d6cb479f32af0dfd6d145be0.1720088047.git.daniel@makrotopia.org
Signed-off-by: Jakub Kicinski <kuba@kernel.org>
---
 drivers/net/ethernet/mediatek/mtk_eth_soc.c | 18 +++++++++++++++++-
 1 file changed, 17 insertions(+), 1 deletion(-)

--- a/drivers/net/ethernet/mediatek/mtk_eth_soc.c
+++ b/drivers/net/ethernet/mediatek/mtk_eth_soc.c
@@ -4498,6 +4498,20 @@ static int mtk_set_rxnfc(struct net_devi
 	return ret;
 }
 
+static void mtk_get_pauseparam(struct net_device *dev, struct ethtool_pauseparam *pause)
+{
+	struct mtk_mac *mac = netdev_priv(dev);
+
+	phylink_ethtool_get_pauseparam(mac->phylink, pause);
+}
+
+static int mtk_set_pauseparam(struct net_device *dev, struct ethtool_pauseparam *pause)
+{
+	struct mtk_mac *mac = netdev_priv(dev);
+
+	return phylink_ethtool_set_pauseparam(mac->phylink, pause);
+}
+
 static u16 mtk_select_queue(struct net_device *dev, struct sk_buff *skb,
 			    struct net_device *sb_dev)
 {
@@ -4526,8 +4540,10 @@ static const struct ethtool_ops mtk_etht
 	.get_strings		= mtk_get_strings,
 	.get_sset_count		= mtk_get_sset_count,
 	.get_ethtool_stats	= mtk_get_ethtool_stats,
+	.get_pauseparam		= mtk_get_pauseparam,
+	.set_pauseparam		= mtk_set_pauseparam,
 	.get_rxnfc		= mtk_get_rxnfc,
-	.set_rxnfc              = mtk_set_rxnfc,
+	.set_rxnfc		= mtk_set_rxnfc,
 };
 
 static const struct net_device_ops mtk_netdev_ops = {
