// SPDX-License-Identifier: (GPL-2.0 OR MIT)

/dts-v1/;

#include "mt7981b-cudy-wr3000-nand.dtsi"

/ {
	model = "Cudy WR3000E v1";
	compatible = "cudy,wr3000e-v1", "mediatek,mt7981";

	aliases {
		label-mac-device = &gmac0;
		led-boot = &led_power;
		led-failsafe = &led_power;
		led-running = &led_power;
		led-upgrade = &led_power;
		serial0 = &uart0;
	};

	leds {
		compatible = "gpio-leds";

		led_power: led-power {
			function = LED_FUNCTION_POWER;
			color = <LED_COLOR_ID_BLUE>;
			gpios = <&pio 8 GPIO_ACTIVE_LOW>;
		};

		led-lan-1 {
			function = LED_FUNCTION_LAN;
			color = <LED_COLOR_ID_BLUE>;
			gpios = <&pio 9 GPIO_ACTIVE_LOW>;
		};

		led-lan-2 {
			function = LED_FUNCTION_LAN;
			color = <LED_COLOR_ID_RED>;
			gpios = <&pio 5 GPIO_ACTIVE_LOW>;
		};

		led-wan {
			function = LED_FUNCTION_WAN_ONLINE;
			color = <LED_COLOR_ID_BLUE>;
			gpios = <&pio 11 GPIO_ACTIVE_LOW>;
		};

		led-wps-1 {
			function = LED_FUNCTION_WPS;
			color = <LED_COLOR_ID_BLUE>;
			gpios = <&pio 10 GPIO_ACTIVE_LOW>;
		};

		led-wps-2 {
			function = LED_FUNCTION_WPS;
			color = <LED_COLOR_ID_RED>;
			gpios = <&pio 4 GPIO_ACTIVE_LOW>;
		};

		led-wlan2g {
			function = LED_FUNCTION_WLAN_2GHZ;
			color = <LED_COLOR_ID_BLUE>;
			gpios = <&pio 6 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "phy0tpt";
		};

		led-wlan5g {
			function = LED_FUNCTION_WLAN_5GHZ;
			color = <LED_COLOR_ID_BLUE>;
			gpios = <&pio 7 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "phy1tpt";
		};
	};
};
&switch {
	ports {
		#address-cells = <1>;
		#size-cells = <0>;

		port@0 {
			reg = <0>;
			label = "wan";

			nvmem-cell-names = "mac-address";
			nvmem-cells = <&macaddr_bdinfo_de00 1>;
		};

		port@1 {
			reg = <1>;
			label = "lan1";
		};

		port@2 {
			reg = <2>;
			label = "lan2";
		};

		port@3 {
			reg = <3>;
			label = "lan3";
		};

		port@4 {
			reg = <4>;
			label = "lan4";
		};

		port@6 {
			reg = <6>;
			label = "cpu";
			ethernet = <&gmac0>;
			phy-mode = "2500base-x";

			fixed-link {
				speed = <2500>;
				full-duplex;
				pause;
			};
		};
	};
};
